SAFE WORK METHOD STATEMENT (SWMS)
Demolish a small building · Demolition · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Business (PCBU) name and ABN
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Person responsible for ensuring compliance
	

	Prepared by
	

	Document number and revision
	

	Date given to principal contractor
	

	Review date
	


2. HIGH RISK CONSTRUCTION WORK COVERED BY THIS SWMS
	
	Risk of a person falling more than 2 metres

	
	Work on a telecommunication tower

	
	Demolition of an element of a structure that is load-bearing or related to its physical integrity

	
	Likely to involve disturbing asbestos

	
	Structural alterations or repairs that require temporary support to prevent collapse

	
	Work in or near a confined space

	
	Work in or near a shaft or trench with an excavated depth greater than 1.5 metres

	
	Work in or near a tunnel

	
	Use of explosives

	
	Work on or near pressurised gas distribution mains or piping

	
	Work on or near chemical, fuel or refrigerant lines

	
	Work on or near energised electrical installations or services

	
	Work in an area that may have a contaminated or flammable atmosphere

	
	Work involving tilt-up or precast concrete elements

	
	Work on, in or next to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	X
	Work in an area with movement of powered mobile plant

	
	Work in an area with artificial extremes of temperature

	
	Work in or near water or other liquid that involves a risk of drowning

	
	Diving work


3. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check the asbestos register, get asbestos removed, and get services disconnected
	Disturbing asbestos
Electric shock from live wiring
Gas and fuel lines
Hitting underground services
	Extreme
	- Before work, check the asbestos register (workplaces built before 2004). For homes, or if there is no register, have a competent person identify asbestos or assume it is present. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Engineering]
- Friable asbestos (Class A) and more than 10 square metres of non-friable asbestos (Class B) must be removed by a licensed removalist. [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Isolate the power before any work. Do not do live work except in the limited cases the WHS Regulations allow (r.157; in Qld, the Electrical Safety Regulation 2013). [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Test before you touch: prove dead at the point of work with a voltage tester, proving the tester on a known live source before and after (AS/NZS 4836). [Engineering]
- Only licensed electricians do electrical work. [Administrative]
- Isolate and purge the line before work, with the owner's approval. [Eliminate]
- Lock off and tag the isolation valve. [Isolate]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Engineering]
- Only licensed gasfitters work on gas lines. [Administrative]
- Keep machine buckets well clear of marked services and use a spotter. [Isolate]
- Scan the area with a cable locator before digging and mark services on the ground. [Engineering]
- Hand dig or vacuum excavate to expose services before using a machine near them. [Engineering]
- Lodge a free BYDA (Before You Dig Australia) request and get the plans before any digging. [Administrative]
	Medium
	

	2
	Fence the site and set up traffic and public control
	Public entering the work area
Road traffic
	Extreme
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving plant or materials across public paths. [Administrative]
- Do the work at low-traffic times, or close the road or lane with approval. [Eliminate]
- Put solid barriers between the work and traffic where speeds are high, not just cones. [Isolate]
- Use a truck-mounted attenuator or buffer vehicle on high speed roads. [Engineering]
- Have a Traffic Management Plan. Signs and cones are set out by accredited traffic controllers to your state's rules. [Administrative]
- Get a road occupancy or street works permit from the road authority before you start. [Administrative]
- Park work vehicles to shield the work zone, with beacons on. [Administrative]
- Wear day and night hi-vis clothing (AS/NZS 4602.1). [PPE]
	Medium
	

	3
	Strip out by hand before machine demolition
	Lifting and carrying heavy loads
Cuts from sharp edges
Falling from height
	Extreme
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile work platform or EWP instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Everyone working at height holds a White Card and has been briefed on this SWMS before going up. [Administrative]
- Have a written emergency and rescue plan, tested before work starts, so a worker hanging in a harness can be brought down within minutes (WHS Regulations r.80). [Administrative]
	Medium
	

	4
	Demolish with the excavator, keeping everyone outside the exclusion zone
	Being hit by mobile plant
Structural collapse during alterations
Demolition and falling debris
	Extreme
	- Separate people and plant with barriers, exclusion zones and marked walkways. [Isolate]
- Use plant with working reversing alarms, cameras and lights. [Engineering]
- Have a traffic management plan showing plant routes, loading areas and pedestrian paths. [Administrative]
- Use a spotter when reversing or working near people. [Administrative]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Administrative]
- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Eliminate]
- Keep everyone clear of the area under and next to the work. [Isolate]
- Install temporary props, needles or shoring as designed before removing any support. [Engineering]
- Follow the engineer's sequence. Do not change it without approval. [Administrative]
- Check props daily. Do not remove them until the permanent support is in and approved. [Administrative]
- Install temporary support to the engineer's or temporary works design before any load bearing element is altered. [Administrative]
- Check for asbestos, lead, live services and structural risks before demolition starts. [Eliminate]
- Disconnect and cap power, gas and water before demolition. [Isolate]
- Set an exclusion zone bigger than the distance the structure could fall. [Isolate]
- Use a machine with a guarded cab instead of hand demolition where practical. [Engineering]
- Use chutes or bins to get debris down. Never drop it from height. [Engineering]
- Notify your state WHS regulator before demolition work where required. [Administrative]
	Medium
	

	5
	Keep dust down with water
	General dust
Silica dust from concrete, brick, stone and tiles
Loud noise
	Extreme
	- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
- If the job involves engineered stone: do not supply, fabricate or install engineered stone benchtops, panels or slabs (banned since 1 July 2024). Removing, repairing or making minor changes to existing engineered stone is only allowed with water suppression or on-tool extraction, a fitted respirator, and written notice to the regulator before the work starts. [Eliminate]
- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- If the cutting, grinding or drilling is high risk, prepare a silica risk control plan (or include the r.529CA assessment in this SWMS), train workers in silica risks and give them the plan before work starts. [Administrative]
- Wear a fit-tested P2 (or better) respirator. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard 1 metre away, wear hearing protection. [Administrative]
- Keep exposure below 85 dB(A) over 8 hours. Give hearing tests to workers who often need hearing protection. [Administrative]
	Medium
	

	6
	Sort and load waste into trucks, then level the site
	Being hit by mobile plant
Road traffic
Poor housekeeping and waste
	Extreme
	- Operators hold a High Risk Work Licence where needed (for example forklift) and are trained and assessed on other plant. [Administrative]
- Do a pre-start check on each machine every day and record it. [Administrative]
- Wear hi-vis clothing and a hard hat. [PPE]
- Being hit by mobile plant: see step 4 for the full controls [Administrative]
- Road traffic: see step 2 for the full controls [Administrative]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skip bins and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
	Medium
	


4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Steel cap boots
Hard hat
Hi-vis shirt or vest
Safety glasses
P2 dust mask
Hearing protection (earmuffs or plugs)
Cut-resistant gloves
Half-face respirator (P2 or P3 filters)
Overalls
Work gloves
	Excavator (Verification of competency (VOC) for the machine)
Skid steer (Bobcat) (Verification of competency (VOC) for the machine)
Tipper or site dumper (Driver licence for the vehicle class, VOC for site dumpers)
Hand tools
Trailer
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 000
	

	Nearest hospital
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Work Health and Safety Regulations 2011, Part 6.3 (Victoria: OHS Regulations 2017).
Keep this SWMS, and every revised version, until the high risk construction work is finished, where workers and inspectors can see it on site. If a notifiable incident happens during the work, keep it for at least 2 years after the incident.
7. SIGN-OFF
By signing below, each person confirms they have read and understood this SWMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/au/swms/demolition/small-building-demolition/
