SAFE WORK METHOD STATEMENT (SWMS)
Rewire a house · Electrical · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Business (PCBU) name and ABN
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Person responsible for ensuring compliance
	

	Prepared by
	

	Document number and revision
	

	Date given to principal contractor
	

	Review date
	


2. HIGH RISK CONSTRUCTION WORK COVERED BY THIS SWMS
	
	Risk of a person falling more than 2 metres

	
	Work on a telecommunication tower

	
	Demolition of an element of a structure that is load-bearing or related to its physical integrity

	
	Likely to involve disturbing asbestos

	
	Structural alterations or repairs that require temporary support to prevent collapse

	
	Work in or near a confined space

	
	Work in or near a shaft or trench with an excavated depth greater than 1.5 metres

	
	Work in or near a tunnel

	
	Use of explosives

	
	Work on or near pressurised gas distribution mains or piping

	
	Work on or near chemical, fuel or refrigerant lines

	X
	Work on or near energised electrical installations or services

	
	Work in an area that may have a contaminated or flammable atmosphere

	
	Work involving tilt-up or precast concrete elements

	
	Work on, in or next to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	
	Work in an area with movement of powered mobile plant

	
	Work in an area with artificial extremes of temperature

	
	Work in or near water or other liquid that involves a risk of drowning

	
	Diving work


3. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Agree a room by room plan with the occupants and protect floors and furniture
	Working in an occupied home or building
Slips and trips
	Medium
	- Plan noisy, dusty or risky work for when the building is empty. [Eliminate]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Isolate]
- Keep fire exits and paths clear at all times. [Administrative]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Administrative]
- Lock away tools, chemicals and materials each day, out of reach of children. [Administrative]
- Clean up dust and debris at the end of each day. [Administrative]
- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Engineering]
- Slips and trips: see step 7 for the full controls [Administrative]
	Low
	

	2
	Check the asbestos register and look for old lead paint before cutting into walls and ceilings
	Disturbing asbestos
Lead paint dust and fumes
	Extreme
	- Before work, check the asbestos register (workplaces built before 2004). For homes, or if there is no register, have a competent person identify asbestos or assume it is present. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Engineering]
- Friable asbestos (Class A) and more than 10 square metres of non-friable asbestos (Class B) must be removed by a licensed removalist. [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Wear a fitted P2 (or better) respirator and disposable coveralls. [PPE]
- Test old paint for lead before you sand, scrape, cut or heat it. [Eliminate]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Substitute]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Isolate]
- Clean up with an H-class vacuum and wet wipes. Never dry sweep. [Engineering]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Administrative]
- Wear a P2 (or better) respirator, disposable coveralls and gloves. [PPE]
	Medium
	

	3
	Isolate the circuits being worked on, lock out and danger tag and test to prove dead; run any temporary supply through RCD protection
	Electric shock from live wiring
Stored energy
Electric shock from leads and power tools
	Extreme
	- Isolate the power before any work. Do not do live work except in the limited cases the WHS Regulations allow (r.157; in Qld, the Electrical Safety Regulation 2013). [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Test before you touch: prove dead at the point of work with a voltage tester, proving the tester on a known live source before and after (AS/NZS 4836). [Engineering]
- Only licensed electricians do electrical work. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- Release or block all stored energy before work: release the pressure in pipes, tanks and hoses, bleed hydraulics, release springs, lower loads. [Eliminate]
- Lock out and tag all energy sources with personal locks. [Isolate]
- Put mechanical blocks or props under raised parts like buckets, tipper bodies and doors. [Engineering]
- Test that the system is dead and nothing can move before you start. [Administrative]
- Follow the maker's procedure, for example for garage door and roller door springs. [Administrative]
- Use battery-powered tools where you can. [Substitute]
- Plug all tools into an RCD-protected outlet or a portable RCD. [Engineering]
- Keep leads off the ground and out of water, using lead stands or hooks. [Engineering]
- Check leads, plugs and tools before every use. Tag out and remove anything damaged. [Administrative]
- Test and tag leads, tools and RCDs at the intervals in AS/NZS 3012 (every 3 months on construction sites). Push-button test portable RCDs before each use. [Administrative]
- Do not use tools in rain or wet areas unless they are rated for it. [Administrative]
	Medium
	

	4
	Work in the ceiling space only on joists, with lighting and short breaks in hot weather
	Falling through a floor opening or void
Heat stress
Poor lighting and night work
Bites and stings
	Extreme
	- Cover every hole and penetration with a fixed, secured cover marked "HOLE" or "DANGER". [Isolate]
- Put guardrails with toe boards around stairwells, lift shafts, voids and open edges. [Isolate]
- Install stairs early and fit temporary handrails as soon as they go in. [Engineering]
- Never remove a cover or guardrail without approval. Put it back straight away. [Administrative]
- Schedule heavy work for the cooler part of the day. [Eliminate]
- Provide shade over work and rest areas, and fans or cooling in roof spaces. [Engineering]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Administrative]
- Take regular rest breaks in the shade, more often as it gets hotter. [Administrative]
- Plan work for daylight hours where you can. [Eliminate]
- Set up enough temporary lighting for the task, walkways, stairs and access points. [Engineering]
- Aim lights so they do not dazzle plant operators or drivers. [Engineering]
- Check lighting before work starts and carry a torch or head lamp. [Administrative]
- Check work areas before starting, and get pest control to remove nests. [Eliminate]
- Look before you reach into dark spaces. [Administrative]
- Ask owners to keep pets away from the work area. [Administrative]
- Know who has allergies and keep their medication, such as an adrenaline auto-injector, close by. [Administrative]
- Know snake bite first aid: pressure immobilisation bandage, keep still and call 000. [Administrative]
	Medium
	

	5
	Scan for pipes, then chase walls and drill holes using dust extraction
	Silica dust from concrete, brick, stone and tiles
General dust
Injury from power tools
Gas and fuel lines
	Extreme
	- If the job involves engineered stone: do not supply, fabricate or install engineered stone benchtops, panels or slabs (banned since 1 July 2024). Removing, repairing or making minor changes to existing engineered stone is only allowed with water suppression or on-tool extraction, a fitted respirator, and written notice to the regulator before the work starts. [Eliminate]
- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- If the cutting, grinding or drilling is high risk, prepare a silica risk control plan (or include the r.529CA assessment in this SWMS), train workers in silica risks and give them the plan before work starts. [Administrative]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Keep all guards fitted and working. Never tie back or remove a guard. [Engineering]
- Clamp or secure the work piece. Do not hold it by hand. [Engineering]
- Only trained, competent people use power tools, following the maker's instructions. [Administrative]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Administrative]
- Isolate and purge the line before work, with the owner's approval. [Eliminate]
- Lock off and tag the isolation valve. [Isolate]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Engineering]
- Only licensed gasfitters work on gas lines. [Administrative]
	Medium
	

	6
	Strip out old wiring, treating every cable as live until it is proven dead
	Electric shock from live wiring
Cuts from sharp edges
	Extreme
	- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
- Electric shock from live wiring: see step 3 for the full controls [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Wear cut-resistant gloves and long sleeves. [PPE]
	Medium
	

	7
	Pull in new cables, keeping walkways and stairs clear
	Slips and trips
Lifting and carrying heavy loads
	High
	- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Engineering]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Engineering]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Administrative]
- Keep work areas, stairs and access paths well lit. [Administrative]
- Wear safety boots with good grip, laced up. [PPE]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium
	

	8
	Fit off power points, switches and lights from a stable step or platform
	Electric shock from leads and power tools
Falling from a ladder
Repetitive work and awkward postures
	High
	- Wear safety boots and dry gloves. [PPE]
- Electric shock from leads and power tools: see step 3 for the full controls [Administrative]
- Use a platform ladder, mobile scaffold or EWP for longer jobs instead of a straight ladder. [Substitute]
- Use industrial-rated ladders (AS/NZS 1892, 120 kg or more) in good condition. Remove any damaged ladder from site. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Administrative]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Substitute]
- Set work up at waist height on benches or trestles where you can. [Engineering]
- Use light tools with good grips, and keep blades and bits sharp. [Engineering]
- Rotate tasks and take short breaks every hour on repetitive work. [Administrative]
- Warm up before heavy physical work and report aches and pains early. [Administrative]
	Medium
	

	9
	Test every circuit, re-energise, make good and hand over the certificate
	Electric shock from live wiring
Poor housekeeping and waste
	Extreme
	- Electric shock from live wiring: see step 3 for the full controls [Administrative]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skip bins and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Medium
	


4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Steel cap boots
Safety glasses
P2 dust mask
Work gloves
Knee pads
Half-face respirator (P2 or P3 filters)
Overalls
Insulated electrical gloves
Arc-rated clothing and face shield
Sun protection (brim hat, long sleeves, SPF 50+)
Hi-vis shirt or vest
Hearing protection (earmuffs or plugs)
Cut-resistant gloves
Hard hat
	Electrical test equipment
Power drill
Hand tools
Step ladder
Rotary hammer drill
	Electrical isolation permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 000
	

	Nearest hospital
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Work Health and Safety Regulations 2011, Part 6.3 (Victoria: OHS Regulations 2017).
Keep this SWMS, and every revised version, until the high risk construction work is finished, where workers and inspectors can see it on site. If a notifiable incident happens during the work, keep it for at least 2 years after the incident.
7. SIGN-OFF
By signing below, each person confirms they have read and understood this SWMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/au/swms/electrical/house-rewiring/
