SAFE WORK METHOD STATEMENT (SWMS)
Backfill and compaction · Excavation and earthworks · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Business (PCBU) name and ABN
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Person responsible for ensuring compliance
	

	Prepared by
	

	Document number and revision
	

	Date given to principal contractor
	

	Review date
	


2. HIGH RISK CONSTRUCTION WORK COVERED BY THIS SWMS
	
	Risk of a person falling more than 2 metres

	
	Work on a telecommunication tower

	
	Demolition of an element of a structure that is load-bearing or related to its physical integrity

	
	Likely to involve disturbing asbestos

	
	Structural alterations or repairs that require temporary support to prevent collapse

	
	Work in or near a confined space

	
	Work in or near a shaft or trench with an excavated depth greater than 1.5 metres

	
	Work in or near a tunnel

	
	Use of explosives

	
	Work on or near pressurised gas distribution mains or piping

	
	Work on or near chemical, fuel or refrigerant lines

	
	Work on or near energised electrical installations or services

	
	Work in an area that may have a contaminated or flammable atmosphere

	
	Work involving tilt-up or precast concrete elements

	
	Work on, in or next to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	X
	Work in an area with movement of powered mobile plant

	
	Work in an area with artificial extremes of temperature

	
	Work in or near water or other liquid that involves a risk of drowning

	
	Diving work


3. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check services are inspected before backfilling
	Hitting underground services
	Extreme
	- Keep machine buckets well clear of marked services and use a spotter. [Isolate]
- Scan the area with a cable locator before digging and mark services on the ground. [Engineering]
- Hand dig or vacuum excavate to expose services before using a machine near them. [Engineering]
- Lodge a free BYDA (Before You Dig Australia) request and get the plans before any digging. [Administrative]
- Keep plans or locate tickets on site and check them again if the work area grows. [Administrative]
- If you hit a service, stop, get everyone clear, and call the owner and emergency services. [Administrative]
- Wear safety boots, gloves and hi-vis when digging. [PPE]
	Medium
	

	2
	Place fill in layers with the machine, keeping a spotter
	Being hit by mobile plant
	Extreme
	- Separate people and plant with barriers, exclusion zones and marked walkways. [Isolate]
- Use plant with working reversing alarms, cameras and lights. [Engineering]
- Have a traffic management plan showing plant routes, loading areas and pedestrian paths. [Administrative]
- Use a spotter when reversing or working near people. [Administrative]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Administrative]
- Operators hold a High Risk Work Licence where needed (for example forklift) and are trained and assessed on other plant. [Administrative]
- Do a pre-start check on each machine every day and record it. [Administrative]
- Wear hi-vis clothing and a hard hat. [PPE]
	Medium
	

	3
	Compact each layer, rotating operators to limit vibration
	Hand-arm and whole-body vibration
Loud noise
	High
	- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Substitute]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Engineering]
- Limit trigger time on high-vibration tools and rotate workers. [Administrative]
- Keep hands warm and dry, and take regular breaks. [Administrative]
- Report tingling, numbness or white fingers early. [Administrative]
- Wear gloves to keep hands warm and dry. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard 1 metre away, wear hearing protection. [Administrative]
- Keep exposure below 85 dB(A) over 8 hours. Give hearing tests to workers who often need hearing protection. [Administrative]
- Wear earplugs or earmuffs rated for the noise. [PPE]
	Medium
	

	4
	Keep compactors away from trench edges
	Trench or excavation collapse
	Extreme
	- Use methods that keep people out of the trench, such as directional boring or working from the surface. [Eliminate]
- Barricade or cover the excavation so people and plant cannot fall in. [Isolate]
- Shore, bench or batter the walls of any trench 1.5 metres deep or more before anyone goes in, unless a geotechnical engineer advises in writing that the sides are safe. [Engineering]
- Keep spoil, materials and plant at least 1 metre back from the edge. [Engineering]
- Provide a safe way in and out, such as a ladder near where people work. [Engineering]
- Inspect the excavation at the start of each shift and after rain or anything that could weaken it. Record it. [Administrative]
- Never work alone in a trench. Watch for water, cracks and bulging walls, and get out if you see them. [Administrative]
- Wear a hard hat, hi-vis and safety boots. [PPE]
	Medium
	

	5
	Clean up and take compaction tests
	Poor housekeeping and waste
	Medium
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skip bins and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Steel cap boots
Hi-vis shirt or vest
Hearing protection (earmuffs or plugs)
Work gloves
Hard hat
	Wacker plate
Skid steer (Bobcat) (Verification of competency (VOC) for the machine)
Excavator (Verification of competency (VOC) for the machine)
	Excavation / dig permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 000
	

	Nearest hospital
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Work Health and Safety Regulations 2011, Part 6.3 (Victoria: OHS Regulations 2017).
Keep this SWMS, and every revised version, until the high risk construction work is finished, where workers and inspectors can see it on site. If a notifiable incident happens during the work, keep it for at least 2 years after the incident.
7. SIGN-OFF
By signing below, each person confirms they have read and understood this SWMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/au/swms/excavation/backfill-compaction/
