SAFE WORK METHOD STATEMENT (SWMS)
Interior painting · Painting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Business (PCBU) name and ABN
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Person responsible for ensuring compliance
	

	Prepared by
	

	Document number and revision
	

	Date given to principal contractor
	

	Review date
	


2. HIGH RISK CONSTRUCTION WORK COVERED BY THIS SWMS
	
	Risk of a person falling more than 2 metres

	
	Work on a telecommunication tower

	
	Demolition of an element of a structure that is load-bearing or related to its physical integrity

	
	Likely to involve disturbing asbestos

	
	Structural alterations or repairs that require temporary support to prevent collapse

	
	Work in or near a confined space

	
	Work in or near a shaft or trench with an excavated depth greater than 1.5 metres

	
	Work in or near a tunnel

	
	Use of explosives

	
	Work on or near pressurised gas distribution mains or piping

	
	Work on or near chemical, fuel or refrigerant lines

	
	Work on or near energised electrical installations or services

	
	Work in an area that may have a contaminated or flammable atmosphere

	
	Work involving tilt-up or precast concrete elements

	
	Work on, in or next to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	
	Work in an area with movement of powered mobile plant

	
	Work in an area with artificial extremes of temperature

	
	Work in or near water or other liquid that involves a risk of drowning

	
	Diving work


3. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Agree work areas with occupants and protect floors and furniture
	Working in an occupied home or building
Slips and trips
	Medium
	- Plan noisy, dusty or risky work for when the building is empty. [Eliminate]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Isolate]
- Keep fire exits and paths clear at all times. [Administrative]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Administrative]
- Lock away tools, chemicals and materials each day, out of reach of children. [Administrative]
- Clean up dust and debris at the end of each day. [Administrative]
- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Engineering]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Engineering]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Administrative]
- Keep work areas, stairs and access paths well lit. [Administrative]
- Wear safety boots with good grip, laced up. [PPE]
	Low
	

	2
	Test old paint for lead before sanding
	Lead paint dust and fumes
	High
	- Test old paint for lead before you sand, scrape, cut or heat it. [Eliminate]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Substitute]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Isolate]
- Clean up with an H-class vacuum and wet wipes. Never dry sweep. [Engineering]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Administrative]
- Wear a P2 (or better) respirator, disposable coveralls and gloves. [PPE]
	Low
	

	3
	Fill and sand walls with a dust mask and vacuum sander
	General dust
Repetitive work and awkward postures
	Medium
	- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
- Wear a dust mask and safety glasses. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Substitute]
- Set work up at waist height on benches or trestles where you can. [Engineering]
- Use light tools with good grips, and keep blades and bits sharp. [Engineering]
- Rotate tasks and take short breaks every hour on repetitive work. [Administrative]
- Warm up before heavy physical work and report aches and pains early. [Administrative]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium
	

	4
	Paint from a platform ladder, not chairs or tins
	Falling from a ladder
Repetitive work and awkward postures
	High
	- Use a platform ladder, mobile scaffold or EWP for longer jobs instead of a straight ladder. [Substitute]
- Use industrial-rated ladders (AS/NZS 1892, 120 kg or more) in good condition. Remove any damaged ladder from site. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Administrative]
- Do not stand on the top three rungs of an extension ladder or the top step of a stepladder. [Administrative]
- Check the ladder before each use: feet, rungs, stiles and locks. [Administrative]
- Wear non-slip safety boots with clean soles. [PPE]
- Repetitive work and awkward postures: see step 3 for the full controls [Administrative]
	Medium
	

	5
	Keep windows open and lids on tins
	Hazardous chemicals
Flammable liquids and gases
	High
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitute]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) before use and keep a register of hazardous chemicals on site. [Administrative]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Use non-flammable or water-based products where you can. [Substitute]
- Keep ignition sources away: no smoking, no hot work and no running engines near flammables. [Isolate]
- Store fuels and solvents in approved, closed containers in a ventilated area away from the work. [Engineering]
- Refuel equipment outdoors with the engine off and cool. [Administrative]
- Keep only what you need for the day on site. [Administrative]
- Store gas cylinders upright, secured and outdoors. [Administrative]
- Keep a suitable fire extinguisher where flammables are used or stored. [Administrative]
- Wear chemical gloves and safety glasses when pouring or mixing. [PPE]
	Medium
	

	6
	Clean brushes away from drains and clear drop sheets
	Poor housekeeping and waste
Slips and trips
	Medium
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skip bins and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
- Slips and trips: see step 1 for the full controls [Administrative]
	Low
	


4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Steel cap boots
Safety glasses
P2 dust mask
Chemical-resistant gloves (nitrile)
Half-face respirator (P2 or P3 filters)
Overalls
Work gloves
Knee pads
Hard hat
Safety goggles
	Platform ladder
Step ladder
Power sander
Hand tools
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 000
	

	Nearest hospital
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Work Health and Safety Regulations 2011, Part 6.3 (Victoria: OHS Regulations 2017).
Keep this SWMS, and every revised version, until the high risk construction work is finished, where workers and inspectors can see it on site. If a notifiable incident happens during the work, keep it for at least 2 years after the incident.
7. SIGN-OFF
By signing below, each person confirms they have read and understood this SWMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/au/swms/painting/interior-painting/
