SAFE WORK METHOD STATEMENT (SWMS)
Pressure washing and surface prep · Painting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Business (PCBU) name and ABN
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Person responsible for ensuring compliance
	

	Prepared by
	

	Document number and revision
	

	Date given to principal contractor
	

	Review date
	


2. HIGH RISK CONSTRUCTION WORK COVERED BY THIS SWMS
	
	Risk of a person falling more than 2 metres

	
	Work on a telecommunication tower

	
	Demolition of an element of a structure that is load-bearing or related to its physical integrity

	
	Likely to involve disturbing asbestos

	
	Structural alterations or repairs that require temporary support to prevent collapse

	
	Work in or near a confined space

	
	Work in or near a shaft or trench with an excavated depth greater than 1.5 metres

	
	Work in or near a tunnel

	
	Use of explosives

	
	Work on or near pressurised gas distribution mains or piping

	
	Work on or near chemical, fuel or refrigerant lines

	
	Work on or near energised electrical installations or services

	
	Work in an area that may have a contaminated or flammable atmosphere

	
	Work involving tilt-up or precast concrete elements

	
	Work on, in or next to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	
	Work in an area with movement of powered mobile plant

	
	Work in an area with artificial extremes of temperature

	
	Work in or near water or other liquid that involves a risk of drowning

	
	Diving work


3. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Cover power points and outside lights, and keep leads off wet ground
	Electric shock from leads and power tools
Electric shock from live wiring
	Extreme
	- Use battery-powered tools where you can. [Substitute]
- Plug all tools into an RCD-protected outlet or a portable RCD. [Engineering]
- Keep leads off the ground and out of water, using lead stands or hooks. [Engineering]
- Check leads, plugs and tools before every use. Tag out and remove anything damaged. [Administrative]
- Test and tag leads, tools and RCDs at the intervals in AS/NZS 3012 (every 3 months on construction sites). Push-button test portable RCDs before each use. [Administrative]
- Do not use tools in rain or wet areas unless they are rated for it. [Administrative]
- Wear safety boots and dry gloves. [PPE]
- Isolate the power before any work. Do not do live work except in the limited cases the WHS Regulations allow (r.157; in Qld, the Electrical Safety Regulation 2013). [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Test before you touch: prove dead at the point of work with a voltage tester, proving the tester on a known live source before and after (AS/NZS 4836). [Engineering]
- Only licensed electricians do electrical work. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium
	

	2
	Check surfaces for asbestos and lead paint first
	Disturbing asbestos
Lead paint dust and fumes
	Extreme
	- Before work, check the asbestos register (workplaces built before 2004). For homes, or if there is no register, have a competent person identify asbestos or assume it is present. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Engineering]
- Friable asbestos (Class A) and more than 10 square metres of non-friable asbestos (Class B) must be removed by a licensed removalist. [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Wear a fitted P2 (or better) respirator and disposable coveralls. [PPE]
- Test old paint for lead before you sand, scrape, cut or heat it. [Eliminate]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Substitute]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Isolate]
- Clean up with an H-class vacuum and wet wipes. Never dry sweep. [Engineering]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Administrative]
- Wear a P2 (or better) respirator, disposable coveralls and gloves. [PPE]
	Medium
	

	3
	Never use the pressure washer from a ladder
	Falling from a ladder
High pressure water jetting
	High
	- Use a platform ladder, mobile scaffold or EWP for longer jobs instead of a straight ladder. [Substitute]
- Use industrial-rated ladders (AS/NZS 1892, 120 kg or more) in good condition. Remove any damaged ladder from site. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Administrative]
- Do not stand on the top three rungs of an extension ladder or the top step of a stepladder. [Administrative]
- Check the ladder before each use: feet, rungs, stiles and locks. [Administrative]
- Wear non-slip safety boots with clean soles. [PPE]
- Set an exclusion zone around the jetting area. [Isolate]
- Use a dead man's trigger that stops the jet when released, and check hoses and fittings before use. [Engineering]
- Only trained operators use high pressure jetting gear. [Administrative]
- Never point the lance at anyone or put a hand in front of it. [Administrative]
- Treat any jetting injury as serious and go to hospital, even if it looks small. [Administrative]
- Wear a face shield, waterproof clothing, gloves, hearing protection and safety boots. [PPE]
	Medium
	

	4
	Mix and apply cleaning chemicals as the label says
	Hazardous chemicals
	Medium
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitute]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) before use and keep a register of hazardous chemicals on site. [Administrative]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
	Medium
	

	5
	Wash down, keeping the lance away from people
	High pressure water jetting
Loud noise
Slips and trips
	High
	- High pressure water jetting: see step 3 for the full controls [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard 1 metre away, wear hearing protection. [Administrative]
- Keep exposure below 85 dB(A) over 8 hours. Give hearing tests to workers who often need hearing protection. [Administrative]
- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Engineering]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Engineering]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Administrative]
- Keep work areas, stairs and access paths well lit. [Administrative]
	Medium
	

	6
	Stop runoff entering stormwater drains and clean up
	Poor housekeeping and waste
	Medium
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skip bins and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Steel cap boots
Safety goggles
Chemical-resistant gloves (nitrile)
Hearing protection (earmuffs or plugs)
Work gloves
Half-face respirator (P2 or P3 filters)
Overalls
Hard hat
Face shield
	Pressure cleaner
Extension ladder
Generator
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 000
	

	Nearest hospital
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Work Health and Safety Regulations 2011, Part 6.3 (Victoria: OHS Regulations 2017).
Keep this SWMS, and every revised version, until the high risk construction work is finished, where workers and inspectors can see it on site. If a notifiable incident happens during the work, keep it for at least 2 years after the incident.
7. SIGN-OFF
By signing below, each person confirms they have read and understood this SWMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/au/swms/painting/pressure-washing-prep/
