SAFE WORK METHOD STATEMENT (SWMS)
Bathroom rough-in plumbing · Plumbing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Business (PCBU) name and ABN
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Person responsible for ensuring compliance
	

	Prepared by
	

	Document number and revision
	

	Date given to principal contractor
	

	Review date
	


2. HIGH RISK CONSTRUCTION WORK COVERED BY THIS SWMS
	
	Risk of a person falling more than 2 metres

	
	Work on a telecommunication tower

	
	Demolition of an element of a structure that is load-bearing or related to its physical integrity

	
	Likely to involve disturbing asbestos

	
	Structural alterations or repairs that require temporary support to prevent collapse

	
	Work in or near a confined space

	
	Work in or near a shaft or trench with an excavated depth greater than 1.5 metres

	
	Work in or near a tunnel

	
	Use of explosives

	
	Work on or near pressurised gas distribution mains or piping

	
	Work on or near chemical, fuel or refrigerant lines

	
	Work on or near energised electrical installations or services

	
	Work in an area that may have a contaminated or flammable atmosphere

	
	Work involving tilt-up or precast concrete elements

	
	Work on, in or next to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	
	Work in an area with movement of powered mobile plant

	
	Work in an area with artificial extremes of temperature

	
	Work in or near water or other liquid that involves a risk of drowning

	
	Diving work


3. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Isolate water to the area and confirm power is off to any circuits in the walls
	Electric shock from live wiring
Stored energy
	Extreme
	- Isolate the power before any work. Do not do live work except in the limited cases the WHS Regulations allow (r.157; in Qld, the Electrical Safety Regulation 2013). [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Test before you touch: prove dead at the point of work with a voltage tester, proving the tester on a known live source before and after (AS/NZS 4836). [Engineering]
- Only licensed electricians do electrical work. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
- Release or block all stored energy before work: release the pressure in pipes, tanks and hoses, bleed hydraulics, release springs, lower loads. [Eliminate]
- Lock out and tag all energy sources with personal locks. [Isolate]
- Put mechanical blocks or props under raised parts like buckets, tipper bodies and doors. [Engineering]
- Test that the system is dead and nothing can move before you start. [Administrative]
- Follow the maker's procedure, for example for garage door and roller door springs. [Administrative]
- Wear safety glasses and gloves. [PPE]
	Medium
	

	2
	Check walls and floors for asbestos before cutting
	Disturbing asbestos
	Extreme
	- Before work, check the asbestos register (workplaces built before 2004). For homes, or if there is no register, have a competent person identify asbestos or assume it is present. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Engineering]
- Friable asbestos (Class A) and more than 10 square metres of non-friable asbestos (Class B) must be removed by a licensed removalist. [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Wear a fitted P2 (or better) respirator and disposable coveralls. [PPE]
	Medium
	

	3
	Cut slab or wall chases with water suppression or dust extraction
	Silica dust from concrete, brick, stone and tiles
Saw cuts and kickback
Loud noise
Hand-arm and whole-body vibration
	Extreme
	- If the job involves engineered stone: do not supply, fabricate or install engineered stone benchtops, panels or slabs (banned since 1 July 2024). Removing, repairing or making minor changes to existing engineered stone is only allowed with water suppression or on-tool extraction, a fitted respirator, and written notice to the regulator before the work starts. [Eliminate]
- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- If the cutting, grinding or drilling is high risk, prepare a silica risk control plan (or include the r.529CA assessment in this SWMS), train workers in silica risks and give them the plan before work starts. [Administrative]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Engineering]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Engineering]
- Use a sharp, undamaged blade made for the material. [Administrative]
- Stand to one side of the blade line, out of the kickback path. [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- Keep exposure below 85 dB(A) over 8 hours. Give hearing tests to workers who often need hearing protection. [Administrative]
- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Substitute]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Engineering]
- Limit trigger time on high-vibration tools and rotate workers. [Administrative]
- Keep hands warm and dry, and take regular breaks. [Administrative]
	Medium
	

	4
	Run waste and water pipes, working at floor level with knee pads
	Lifting and carrying heavy loads
Repetitive work and awkward postures
Cuts from sharp edges
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Substitute]
- Set work up at waist height on benches or trestles where you can. [Engineering]
- Use light tools with good grips, and keep blades and bits sharp. [Engineering]
- Rotate tasks and take short breaks every hour on repetitive work. [Administrative]
- Warm up before heavy physical work and report aches and pains early. [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
	Medium
	

	5
	Glue solvent joints with ventilation and no flames nearby
	Hazardous chemicals
Flammable liquids and gases
	High
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitute]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) before use and keep a register of hazardous chemicals on site. [Administrative]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Use non-flammable or water-based products where you can. [Substitute]
- Keep ignition sources away: no smoking, no hot work and no running engines near flammables. [Isolate]
- Store fuels and solvents in approved, closed containers in a ventilated area away from the work. [Engineering]
- Refuel equipment outdoors with the engine off and cool. [Administrative]
- Keep only what you need for the day on site. [Administrative]
- Store gas cylinders upright, secured and outdoors. [Administrative]
- Keep a suitable fire extinguisher where flammables are used or stored. [Administrative]
- Wear chemical gloves and safety glasses when pouring or mixing. [PPE]
	Medium
	

	6
	Pressure test the pipework and clean up
	Pressure testing
Poor housekeeping and waste
	Medium
	- Test with water instead of air or gas where the system allows it. Never put water in refrigerant pipework, which is tested with dry nitrogen. [Substitute]
- Keep people out of the test area with signs and barriers. [Isolate]
- Use a calibrated gauge and a relief valve set to protect the system. [Engineering]
- Test to the pressure the system calls for and hold it for the set time. Never go over. [Administrative]
- Release the pressure fully before tightening anything or fixing leaks. [Administrative]
- Wear safety glasses or a face shield. [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skip bins and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Steel cap boots
Safety glasses
P2 dust mask
Hearing protection (earmuffs or plugs)
Knee pads
Work gloves
Half-face respirator (P2 or P3 filters)
Overalls
Cut-resistant gloves
Chemical-resistant gloves (nitrile)
Safety goggles
Face shield
	Power drill
Rotary hammer drill
Pipe press tool
Hand tools
Concrete saw
	Electrical isolation permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 000
	

	Nearest hospital
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Work Health and Safety Regulations 2011, Part 6.3 (Victoria: OHS Regulations 2017).
Keep this SWMS, and every revised version, until the high risk construction work is finished, where workers and inspectors can see it on site. If a notifiable incident happens during the work, keep it for at least 2 years after the incident.
7. SIGN-OFF
By signing below, each person confirms they have read and understood this SWMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/au/swms/plumbing/bathroom-rough-in/
