SAFE WORK METHOD STATEMENT (SWMS)
Replace fascia and soffits · Roofing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Business (PCBU) name and ABN
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Person responsible for ensuring compliance
	

	Prepared by
	

	Document number and revision
	

	Date given to principal contractor
	

	Review date
	


2. HIGH RISK CONSTRUCTION WORK COVERED BY THIS SWMS
	
	Risk of a person falling more than 2 metres

	
	Work on a telecommunication tower

	
	Demolition of an element of a structure that is load-bearing or related to its physical integrity

	
	Likely to involve disturbing asbestos

	
	Structural alterations or repairs that require temporary support to prevent collapse

	
	Work in or near a confined space

	
	Work in or near a shaft or trench with an excavated depth greater than 1.5 metres

	
	Work in or near a tunnel

	
	Use of explosives

	
	Work on or near pressurised gas distribution mains or piping

	
	Work on or near chemical, fuel or refrigerant lines

	
	Work on or near energised electrical installations or services

	
	Work in an area that may have a contaminated or flammable atmosphere

	
	Work involving tilt-up or precast concrete elements

	
	Work on, in or next to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	
	Work in an area with movement of powered mobile plant

	
	Work in an area with artificial extremes of temperature

	
	Work in or near water or other liquid that involves a risk of drowning

	
	Diving work


3. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Barricade below and set up a mobile scaffold or secured ladder
	Public entering the work area
Falling from a ladder
Falling from height
	Extreme
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Administrative]
- Use a platform ladder, mobile scaffold or EWP for longer jobs instead of a straight ladder. [Substitute]
- Use industrial-rated ladders (AS/NZS 1892, 120 kg or more) in good condition. Remove any damaged ladder from site. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Administrative]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile work platform or EWP instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Everyone working at height holds a White Card and has been briefed on this SWMS before going up. [Administrative]
- Have a written emergency and rescue plan, tested before work starts, so a worker hanging in a harness can be brought down within minutes (WHS Regulations r.80). [Administrative]
	Medium
	

	2
	Check soffit sheets for asbestos and old paint for lead before removing
	Disturbing asbestos
Lead paint dust and fumes
	Extreme
	- Before work, check the asbestos register (workplaces built before 2004). For homes, or if there is no register, have a competent person identify asbestos or assume it is present. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Engineering]
- Friable asbestos (Class A) and more than 10 square metres of non-friable asbestos (Class B) must be removed by a licensed removalist. [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Wear a fitted P2 (or better) respirator and disposable coveralls. [PPE]
- Test old paint for lead before you sand, scrape, cut or heat it. [Eliminate]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Substitute]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Isolate]
- Clean up with an H-class vacuum and wet wipes. Never dry sweep. [Engineering]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Administrative]
- Wear a P2 (or better) respirator, disposable coveralls and gloves. [PPE]
	Medium
	

	3
	Remove gutters and old fascia boards, lowering them by hand
	Lifting and carrying heavy loads
Falling tools and materials
Cuts from sharp edges
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
	Medium
	

	4
	Cut and fix new boards and soffit lining
	Saw cuts and kickback
Nail gun injuries
Wood and MDF dust
Loud noise
	High
	- Keep blade guards fitted and working, and use the riving knife on table saws. [Engineering]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Engineering]
- Use a sharp, undamaged blade made for the material. [Administrative]
- Stand to one side of the blade line, out of the kickback path. [Administrative]
- Use a nail gun with a sequential (single shot) trigger, not a contact or bump trigger. [Substitute]
- Disconnect the air or battery before clearing jams, adjusting or moving between work areas. [Engineering]
- Keep your free hand at least 30 cm from the nailing point. [Administrative]
- Never point the gun at anyone or carry it with your finger on the trigger. [Administrative]
- Buy pre-cut or pre-finished timber where you can. [Substitute]
- Cut outdoors or in a well-ventilated area away from others. [Isolate]
- Use saws and sanders with dust extraction connected to an M-class (or better) vacuum. [Engineering]
- Clean up with a vacuum, not a broom or compressed air. [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- Keep exposure below 85 dB(A) over 8 hours. Give hearing tests to workers who often need hearing protection. [Administrative]
	Medium
	

	5
	Refit gutters, clean up and remove access
	Poor housekeeping and waste
Falling from a ladder
	High
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skip bins and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
- Do not stand on the top three rungs of an extension ladder or the top step of a stepladder. [Administrative]
- Check the ladder before each use: feet, rungs, stiles and locks. [Administrative]
- Wear non-slip safety boots with clean soles. [PPE]
- Falling from a ladder: see step 1 for the full controls [Administrative]
	Medium
	


4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Steel cap boots
Safety glasses
Work gloves
P2 dust mask
Hearing protection (earmuffs or plugs)
Hi-vis shirt or vest
Hard hat
Half-face respirator (P2 or P3 filters)
Overalls
Cut-resistant gloves
	Mobile scaffold (Scaffolding HRWL (SB or higher) to erect, alter or dismantle where a person or object could fall more than 4 m)
Extension ladder
Circular saw
Nail gun
Hand tools
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 000
	

	Nearest hospital
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Work Health and Safety Regulations 2011, Part 6.3 (Victoria: OHS Regulations 2017).
Keep this SWMS, and every revised version, until the high risk construction work is finished, where workers and inspectors can see it on site. If a notifiable incident happens during the work, keep it for at least 2 years after the incident.
7. SIGN-OFF
By signing below, each person confirms they have read and understood this SWMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/au/swms/roofing/fascia-soffit-replacement/
