SAFE WORK METHOD STATEMENT (SWMS)
Re-roof: strip and replace a roof · Roofing · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Business (PCBU) name and ABN
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Person responsible for ensuring compliance
	

	Prepared by
	

	Document number and revision
	

	Date given to principal contractor
	

	Review date
	


2. HIGH RISK CONSTRUCTION WORK COVERED BY THIS SWMS
	X
	Risk of a person falling more than 2 metres

	
	Work on a telecommunication tower

	
	Demolition of an element of a structure that is load-bearing or related to its physical integrity

	
	Likely to involve disturbing asbestos

	
	Structural alterations or repairs that require temporary support to prevent collapse

	
	Work in or near a confined space

	
	Work in or near a shaft or trench with an excavated depth greater than 1.5 metres

	
	Work in or near a tunnel

	
	Use of explosives

	
	Work on or near pressurised gas distribution mains or piping

	
	Work on or near chemical, fuel or refrigerant lines

	
	Work on or near energised electrical installations or services

	
	Work in an area that may have a contaminated or flammable atmosphere

	
	Work involving tilt-up or precast concrete elements

	
	Work on, in or next to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	X
	Work in an area with movement of powered mobile plant

	
	Work in an area with artificial extremes of temperature

	
	Work in or near water or other liquid that involves a risk of drowning

	
	Diving work


3. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check the asbestos register and get any asbestos roof removed by a licensed removalist first
	Disturbing asbestos
	Extreme
	- Before work, check the asbestos register (workplaces built before 2004). For homes, or if there is no register, have a competent person identify asbestos or assume it is present. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Engineering]
- Friable asbestos (Class A) and more than 10 square metres of non-friable asbestos (Class B) must be removed by a licensed removalist. [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Wear a fitted P2 (or better) respirator and disposable coveralls. [PPE]
	Medium
	

	2
	Check the weather and power lines, and plan the crane, hoist and skip bin positions
	Contact with overhead power lines
Strong wind and storms
Crane and lifting failure
	High
	- Ask the network operator to turn off, move or insulate the lines before work starts. [Eliminate]
- Use non-conductive (fibreglass) ladders near any power lines. [Substitute]
- Mark the safe distance with flags, tape or goal posts and keep all plant and people outside it. [Isolate]
- Keep out of the No Go Zone set by your state and the network operator, or get written approval and a safety observer. In NSW and Qld, untrained people and plant stay at least 3 m from lines on poles up to 132 kV, 6 m up to 330 kV and 8 m above 330 kV. In Victoria the limits differ, and work within 8 m of tower lines needs a spotter and the network operator's permission. [Administrative]
- Use a dedicated spotter whenever plant moves or raises anything near lines. [Administrative]
- Treat all lines as live. If plant touches a line, stay in the cab and keep everyone well away. [Administrative]
- Check the forecast each morning and plan work at height and lifting around the weather. [Eliminate]
- Tie down or weigh down loose sheets, panels, boards and rubbish at the end of each shift. [Engineering]
- Set wind limits for roof work, platforms and cranes, using the manufacturer's limits, and stop when they are reached. [Administrative]
- Stop work and get down in lightning. Wait 30 minutes after the last thunder before going back up. [Administrative]
- Check scaffold, fencing and edge protection after strong wind before anyone uses them. [Administrative]
- Barricade the lift zone and keep everyone out from under the load. [Isolate]
- Use a crane rated for the load at the radius, set up on firm ground with outrigger pads. [Engineering]
- Check slings, chains, shackles and hooks before use. Remove anything damaged or not tagged. [Engineering]
- Plan the lift: weight, radius, ground, path and landing area. Use a written lift plan for complex lifts. [Administrative]
- Crane operators and doggers or riggers hold the right High Risk Work Licence. [Administrative]
	Medium
	

	3
	Erect full perimeter scaffold edge protection, a waste chute and an exclusion zone below
	Falling from a roof edge
Scaffold collapse or fall from scaffold
Falling tools and materials
Public entering the work area
	Extreme
	- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Eliminate]
- Install edge protection or guardrails on all open roof edges before work starts. [Isolate]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Engineering]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Engineering]
- Only workers briefed on this SWMS go on the roof. Stop and review the SWMS if the roof, weather or method changes. [Administrative]
- Have a written emergency and rescue plan, tested before work starts, for any worker using a harness (WHS Regulations r.80). [Administrative]
- Scaffold is built, altered and taken down only by a competent scaffolder, on a firm base with sole boards and ties. [Engineering]
- Fit guardrails, mid rails and toe boards on every working platform. [Engineering]
- Use mobile scaffolds only on firm, level ground with castors locked and outriggers fitted. Never move one with anyone on it. [Engineering]
- Scaffold where a person or object could fall more than 4 metres is built by a licensed scaffolder (High Risk Work Licence). [Administrative]
- Do not use a scaffold over 4 metres until the scaffolder gives a written handover certificate. [Administrative]
- Inspect the scaffold before first use, after any change or bad weather, and at least every 30 days. Record it on the scaffold tag. [Administrative]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Falling tools and materials: see step 5 for the full controls [Administrative]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
	Medium
	

	4
	Strip the old roof in sections so the building stays covered if rain comes
	Strong wind and storms
Falling through a fragile roof or skylight
Lifting and carrying heavy loads
Cuts from sharp edges
	Extreme
	- Do not carry large sheets on roofs in wind. [Administrative]
- Wear a hard hat with a chin strap at height in windy conditions. [PPE]
- Strong wind and storms: see step 2 for the full controls [Administrative]
- Work from underneath or from an EWP so nobody stands on the fragile roof. [Eliminate]
- Cover or guard every skylight and fragile sheet with a fixed, marked cover or mesh before work starts. [Isolate]
- Install safety mesh under new roof sheeting, and use crawl boards or staging to spread the load on fragile surfaces. [Engineering]
- Use fall arrest on rated anchors when working near fragile areas. [Engineering]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitute]
- Lifting and carrying heavy loads: see step 7 for the full controls [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
	Medium
	

	5
	Lower waste in the chute or by crane, never throw it off
	Falling tools and materials
Crane and lifting failure
Poor housekeeping and waste
	High
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Use tag lines to control loads and agree on clear radio or hand signals. [Administrative]
- Stop lifting in high wind or when the operator cannot see the signaller. [Administrative]
- Never ride on a load or hook. [Administrative]
- Crane and lifting failure: see step 2 for the full controls [Administrative]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skip bins and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
	Medium
	

	6
	Check and repair the roof framing, guarding any gaps
	Structural collapse during alterations
Falling from height
	Extreme
	- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Eliminate]
- Keep everyone clear of the area under and next to the work. [Isolate]
- Install temporary props, needles or shoring as designed before removing any support. [Engineering]
- Follow the engineer's sequence. Do not change it without approval. [Administrative]
- Check props daily. Do not remove them until the permanent support is in and approved. [Administrative]
- Install temporary support to the engineer's or temporary works design before any load bearing element is altered. [Administrative]
- Wear a hard hat and safety boots. [PPE]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Falling from height: see step 7 for the full controls [Administrative]
	Medium
	

	7
	Install safety mesh, sarking and battens
	Falling from height
Lifting and carrying heavy loads
	Extreme
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile work platform or EWP instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Everyone working at height holds a White Card and has been briefed on this SWMS before going up. [Administrative]
- Have a written emergency and rescue plan, tested before work starts, so a worker hanging in a harness can be brought down within minutes (WHS Regulations r.80). [Administrative]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium
	

	8
	Land new roofing materials by crane or hoist, spreading loads across the frame
	Crane and lifting failure
Structural collapse during alterations
	High
	- Wear a hard hat, hi-vis, gloves and safety boots. [PPE]
- Crane and lifting failure: see step 2 for the full controls [Administrative]
- Structural collapse during alterations: see step 6 for the full controls [Administrative]
	Medium
	

	9
	Lay the new roof, taking breaks in heat and sun
	Lifting and carrying heavy loads
Heat stress
Sun exposure (UV)
	High
	- Lifting and carrying heavy loads: see step 7 for the full controls [Administrative]
- Schedule heavy work for the cooler part of the day. [Eliminate]
- Provide shade over work and rest areas, and fans or cooling in roof spaces. [Engineering]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Administrative]
- Take regular rest breaks in the shade, more often as it gets hotter. [Administrative]
- Let new and returning workers build up to full work in the heat over about a week. [Administrative]
- Plan outdoor work for early morning or late afternoon when UV is lower. [Eliminate]
- Put shade covers over fixed work areas. [Engineering]
- Check the UV index each day. Use sun protection when it is 3 or higher. [Administrative]
- Check your skin regularly and see a doctor about any new or changing spots. [Administrative]
- Wear a broad-brim hat or hard hat brim, long sleeves, sunglasses and SPF 50+ sunscreen, reapplied every 2 hours. [PPE]
	Medium
	

	10
	Fit flashings, ridge capping, gutters and downpipes
	Injury from power tools
Angle grinder injuries
Cuts from sharp edges
	High
	- Keep all guards fitted and working. Never tie back or remove a guard. [Engineering]
- Clamp or secure the work piece. Do not hold it by hand. [Engineering]
- Only trained, competent people use power tools, following the maker's instructions. [Administrative]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Administrative]
- No loose clothing, jewellery or long hair near spinning parts. [Administrative]
- Use a guarded saw or a different tool where you can. [Substitute]
- Keep the guard on and use the side handle. Never remove the guard. [Engineering]
- Use the right disc for the job, rated for the grinder's speed. Check it for cracks first. [Administrative]
- Only trained people change discs, with the grinder unplugged or the battery out. [Administrative]
- Keep both hands on the grinder and let the disc stop before putting it down. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Wear cut-resistant gloves and long sleeves. [PPE]
- Cuts from sharp edges: see step 4 for the full controls [Administrative]
	Medium
	

	11
	Clean the roof and site, then dismantle scaffold once the roof is signed off
	Poor housekeeping and waste
Scaffold collapse or fall from scaffold
	Extreme
	- Wear gloves when handling waste. [PPE]
- Poor housekeeping and waste: see step 5 for the full controls [Administrative]
- Do not overload platforms. Know the duty rating and keep material stacks over the standards. [Administrative]
- Never remove ties, braces, guardrails or boards. Only the scaffolder alters the scaffold. [Administrative]
- Wear a hard hat and safety boots on and around the scaffold. [PPE]
- Scaffold collapse or fall from scaffold: see step 3 for the full controls [Administrative]
	Medium
	


4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Steel cap boots
Safety harness and lanyard
Hard hat
Cut-resistant gloves
Safety glasses
P2 dust mask
Hearing protection (earmuffs or plugs)
Sun protection (brim hat, long sleeves, SPF 50+)
Half-face respirator (P2 or P3 filters)
Overalls
Work gloves
Hi-vis shirt or vest
Face shield
	Fixed scaffold (Scaffolding HRWL (SB, SI or SA) to erect, alter or dismantle where a fall of more than 4 m is possible)
Crane (Franna or mobile) (HRWL for the crane class (e.g. C2, CN, C6), plus Dogging licence (DG) where slinging needs judgement or the load is out of the operator's view)
Telehandler (3 t or less: trained and assessed (VOC). Over 3 t with a jib, hook or winch: High Risk Work Licence CN (non-slewing mobile crane). Slewing telehandlers: slewing crane licence (C2, C6 and up). Victoria: any non-slewing telehandler over 3 t needs CN or the Victorian telehandler licence)
Angle grinder
Power drill
Trailer
	Lift plan
Roof access permit
Working at heights permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 000
	

	Nearest hospital
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Work Health and Safety Regulations 2011, Part 6.3 (Victoria: OHS Regulations 2017).
Keep this SWMS, and every revised version, until the high risk construction work is finished, where workers and inspectors can see it on site. If a notifiable incident happens during the work, keep it for at least 2 years after the incident.
7. SIGN-OFF
By signing below, each person confirms they have read and understood this SWMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/au/swms/roofing/re-roofing/
