SAFE WORK METHOD STATEMENT (SWMS)
Install a skylight · Roofing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Business (PCBU) name and ABN
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Person responsible for ensuring compliance
	

	Prepared by
	

	Document number and revision
	

	Date given to principal contractor
	

	Review date
	


2. HIGH RISK CONSTRUCTION WORK COVERED BY THIS SWMS
	X
	Risk of a person falling more than 2 metres

	
	Work on a telecommunication tower

	
	Demolition of an element of a structure that is load-bearing or related to its physical integrity

	
	Likely to involve disturbing asbestos

	
	Structural alterations or repairs that require temporary support to prevent collapse

	
	Work in or near a confined space

	
	Work in or near a shaft or trench with an excavated depth greater than 1.5 metres

	
	Work in or near a tunnel

	
	Use of explosives

	
	Work on or near pressurised gas distribution mains or piping

	
	Work on or near chemical, fuel or refrigerant lines

	
	Work on or near energised electrical installations or services

	
	Work in an area that may have a contaminated or flammable atmosphere

	
	Work involving tilt-up or precast concrete elements

	
	Work on, in or next to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	
	Work in an area with movement of powered mobile plant

	
	Work in an area with artificial extremes of temperature

	
	Work in or near water or other liquid that involves a risk of drowning

	
	Diving work


3. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up roof access and edge protection, and protect the room below from falling debris
	Falling from a roof edge
Falling from a ladder
Falling tools and materials
	Extreme
	- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Eliminate]
- Install edge protection or guardrails on all open roof edges before work starts. [Isolate]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Engineering]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Engineering]
- Only workers briefed on this SWMS go on the roof. Stop and review the SWMS if the roof, weather or method changes. [Administrative]
- Use one safe, controlled access point and keep others off the roof. [Administrative]
- Have a written emergency and rescue plan, tested before work starts, for any worker using a harness (WHS Regulations r.80). [Administrative]
- Use a platform ladder, mobile scaffold or EWP for longer jobs instead of a straight ladder. [Substitute]
- Use industrial-rated ladders (AS/NZS 1892, 120 kg or more) in good condition. Remove any damaged ladder from site. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Administrative]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
	Medium
	

	2
	Mark out the opening, checking for cables, pipes and roof framing in the ceiling space
	Electric shock from live wiring
Heat stress
	Extreme
	- Isolate the power before any work. Do not do live work except in the limited cases the WHS Regulations allow (r.157; in Qld, the Electrical Safety Regulation 2013). [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Test before you touch: prove dead at the point of work with a voltage tester, proving the tester on a known live source before and after (AS/NZS 4836). [Engineering]
- Only licensed electricians do electrical work. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
- Schedule heavy work for the cooler part of the day. [Eliminate]
- Provide shade over work and rest areas, and fans or cooling in roof spaces. [Engineering]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Administrative]
- Take regular rest breaks in the shade, more often as it gets hotter. [Administrative]
- Let new and returning workers build up to full work in the heat over about a week. [Administrative]
- Watch each other for dizziness, headache, confusion or stopping sweating. Stop work, cool down and get help. [Administrative]
- Have a hot weather plan, including when work stops. [Administrative]
- Wear light, loose, long-sleeved clothing, a hat or brim, and sunscreen. [PPE]
	Medium
	

	3
	Cut the roof and ceiling opening, then cover or guard the hole straight away
	Falling through a floor opening or void
Saw cuts and kickback
General dust
	Extreme
	- Cover every hole and penetration with a fixed, secured cover marked "HOLE" or "DANGER". [Isolate]
- Put guardrails with toe boards around stairwells, lift shafts, voids and open edges. [Isolate]
- Install stairs early and fit temporary handrails as soon as they go in. [Engineering]
- Never remove a cover or guardrail without approval. Put it back straight away. [Administrative]
- Inspect covers and barriers daily and after other trades have been through. [Administrative]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Engineering]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Engineering]
- Use a sharp, undamaged blade made for the material. [Administrative]
- Stand to one side of the blade line, out of the kickback path. [Administrative]
- Let the blade stop fully before reaching in or putting the saw down. [Administrative]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
	Medium
	

	4
	Fit the skylight frame and flashing, carrying the glass unit with two people
	Lifting and carrying heavy loads
Glass handling and breakage
Cuts from sharp edges
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Use suction lifters, glass trolleys or a glazing robot for large panes. [Engineering]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Engineering]
- Use two or more people for large panes, and clear the carry route first. [Administrative]
- Mark new glass with tape or stickers so nobody walks into it. [Administrative]
- Clean up broken glass straight away into a marked container. [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
	Medium
	

	5
	Install the light shaft and patch the ceiling
	Falling from a ladder
General dust
Injury from power tools
	High
	- Do not stand on the top three rungs of an extension ladder or the top step of a stepladder. [Administrative]
- Check the ladder before each use: feet, rungs, stiles and locks. [Administrative]
- Wear non-slip safety boots with clean soles. [PPE]
- Falling from a ladder: see step 1 for the full controls [Administrative]
- Wear a dust mask and safety glasses. [PPE]
- General dust: see step 3 for the full controls [Administrative]
- Keep all guards fitted and working. Never tie back or remove a guard. [Engineering]
- Clamp or secure the work piece. Do not hold it by hand. [Engineering]
- Only trained, competent people use power tools, following the maker's instructions. [Administrative]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Administrative]
- No loose clothing, jewellery or long hair near spinning parts. [Administrative]
	Medium
	

	6
	Seal and water test, then clean up and remove access
	Poor housekeeping and waste
Slips and trips
	Medium
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skip bins and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Engineering]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Engineering]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Administrative]
- Keep work areas, stairs and access paths well lit. [Administrative]
- Wear safety boots with good grip, laced up. [PPE]
	Low
	


4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Steel cap boots
Safety harness and lanyard
Cut-resistant gloves
Safety glasses
P2 dust mask
Sun protection (brim hat, long sleeves, SPF 50+)
Hard hat
Hearing protection (earmuffs or plugs)
Work gloves
	Extension ladder
Mobile scaffold (Scaffolding HRWL (SB or higher) to erect, alter or dismantle where a person or object could fall more than 4 m)
Power drill
Circular saw
Hand tools
	Roof access permit
Working at heights permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 000
	

	Nearest hospital
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Work Health and Safety Regulations 2011, Part 6.3 (Victoria: OHS Regulations 2017).
Keep this SWMS, and every revised version, until the high risk construction work is finished, where workers and inspectors can see it on site. If a notifiable incident happens during the work, keep it for at least 2 years after the incident.
7. SIGN-OFF
By signing below, each person confirms they have read and understood this SWMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/au/swms/roofing/skylight-installation/
