FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Blockwork wall · Bricklaying · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check footing and starter bars, capping rebar
	Impalement on rebar
	High
	- Cover or cap all exposed bar ends with approved caps or covers. [Engineering]
- Bend bars over where the design allows. [Engineering]
- Use edge protection near starter bars so nobody can fall onto them. [Engineering]
- Keep walkways clear of exposed bars and mark the hazard. [Administrative]
- Wear gloves, safety glasses and safety boots when handling bar. [PPE]
	Low
	

	2
	Move blocks with plant or two people
	Lifting and carrying heavy loads
Being hit by heavy equipment
	Critical
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or equipment instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Separate people and equipment with barriers, exclusion zones and marked walkways. [Engineering (guarding)]
- Use equipment with working backup alarms, cameras and lights. [Engineering]
- Have a site traffic plan showing equipment routes, loading areas and pedestrian paths. [Administrative]
- Use a spotter when backing up or working near people. [Administrative]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Administrative]
- Operators are trained and competent for each machine. [Administrative]
- Do a pre-start check on each machine every day and record it. [Administrative]
- Wear hi-vis clothing and a hard hat. [PPE]
	Medium
	

	3
	Cut blocks with water suppression
	Silica dust from concrete, brick, stone and tiles
Saw cuts and kickback
Loud noise
	Critical
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitution]
- Cut outdoors or in a separate area, with other people well away and upwind. [Engineering (guarding)]
- Use water on the blade or on-tool dust extraction connected to a HEPA vacuum. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- Have a silica exposure control plan where your province requires one. [Administrative]
- Wear a fit-tested N95 (or better) respirator. [PPE]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Engineering]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Engineering]
- Use a sharp, undamaged blade made for the material. [Administrative]
- Stand to one side of the blade line, out of the kickback path. [Administrative]
- Let the blade stop fully before reaching in or putting the saw down. [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy equipment away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard 1 metre away, wear hearing protection. [Administrative]
	Medium
	

	4
	Lay blocks from scaffold once above chest height
	Falling from height
Repetitive work and awkward postures
	Critical
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Elimination]
- Install guardrails or edge protection on all open edges before work starts. [Engineering (guarding)]
- Use a scaffold, mobile work platform or aerial work platform instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Fall protection plan in place where required. Workers trained in fall protection (Working at Heights training in Ontario). [Administrative]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Administrative]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Substitution]
- Set work up at waist height on benches or trestles where you can. [Engineering]
- Use light tools with good grips, and keep blades and bits sharp. [Engineering]
- Rotate tasks and take short breaks every hour on repetitive work. [Administrative]
- Warm up before heavy physical work and report aches and pains early. [Administrative]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium
	

	5
	Core fill with pump or mixer, propping walls as needed
	Wet concrete and cement burns
Structural collapse during alterations
	High
	- Use long-handled tools and pumps to cut down contact. [Engineering]
- Wash concrete off skin straight away with clean water. [Administrative]
- Have clean water and eye wash at the pour. [Administrative]
- Wear waterproof gloves, long sleeves and rubber boots with pants worn over the top. [PPE]
- Wear safety glasses or goggles to stop splashes. [PPE]
- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Elimination]
- Keep everyone clear of the area under and next to the work. [Engineering (guarding)]
- Install temporary props, needles or shoring as designed before removing any support. [Engineering]
- Follow the engineer's sequence. Do not change it without approval. [Administrative]
- Check props daily. Do not remove them until the permanent support is in and approved. [Administrative]
- Wear a hard hat and safety boots. [PPE]
	Medium
	

	6
	Clean up
	Poor housekeeping and waste
	Medium
	- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Hard hat (CSA Z94.1)
Chemical-resistant gloves
Safety glasses (CSA Z94.3)
N95 respirator
Hearing protection
Work gloves
High-visibility vest (CSA Z96)
Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
Knee pads
Safety goggles
	Frame scaffold (Provincial scaffold erector training)
Cement mixer
Concrete saw (cut-off saw)
Concrete pump truck
Telehandler (Provincial lift truck or telehandler operator training)
	None required


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/ca/flha/bricklaying/blockwork-wall/
