FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Concrete driveway · Concreting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up traffic and pedestrian control at the street
	Road traffic
Public entering the work area
	Critical
	- Do the work at low-traffic times, or close the road or lane with approval. [Elimination]
- Put solid barriers between the work and traffic where speeds are high, not just cones. [Engineering (guarding)]
- Use a truck-mounted attenuator or buffer vehicle on high speed roads. [Engineering]
- Set up signs and cones to your provincial traffic control manual, with trained traffic control persons. [Administrative]
- Get a road occupancy permit from the municipality or road authority before you start. [Administrative]
- Park work vehicles to shield the work zone, with beacons on. [Administrative]
- Wear high-visibility clothing to CSA Z96. [PPE]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Public entering the work area: see step 6 for the full controls [Administrative]
	Medium
	

	2
	Locate services, then excavate and level the base with the skid steer
	Hitting underground services
Being hit by heavy equipment
	Critical
	- Keep machine buckets well clear of marked services and use a spotter. [Engineering (guarding)]
- Scan the area with a cable locator before digging and mark services on the ground. [Engineering]
- Hand expose or hydrovac services before machine digging inside the locate tolerance zone. [Engineering]
- Click Before You Dig: lodge a locate request with your provincial one-call service and wait for the locates. [Administrative]
- Follow your province's ground disturbance rules and keep locate sheets on site. [Administrative]
- Keep plans or locate tickets on site and check them again if the work area grows. [Administrative]
- If you hit a service, stop, get everyone clear, and call the owner and emergency services. [Administrative]
- Wear safety boots, gloves and hi-vis when digging. [PPE]
- Separate people and equipment with barriers, exclusion zones and marked walkways. [Engineering (guarding)]
- Use equipment with working backup alarms, cameras and lights. [Engineering]
- Have a site traffic plan showing equipment routes, loading areas and pedestrian paths. [Administrative]
- Use a spotter when backing up or working near people. [Administrative]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Administrative]
- Operators are trained and competent for each machine. [Administrative]
- Do a pre-start check on each machine every day and record it. [Administrative]
- Wear hi-vis clothing and a hard hat. [PPE]
	Medium
	

	3
	Compact base, set forms and rebar
	Hand-arm and whole-body vibration
Loud noise
Impalement on rebar
Lifting and carrying heavy loads
	High
	- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Substitution]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Engineering]
- Limit trigger time on high-vibration tools and rotate workers. [Administrative]
- Keep hands warm and dry, and take regular breaks. [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy equipment away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- Cover or cap all exposed bar ends with approved caps or covers. [Engineering]
- Bend bars over where the design allows. [Engineering]
- Use edge protection near starter bars so nobody can fall onto them. [Engineering]
- Keep walkways clear of exposed bars and mark the hazard. [Administrative]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or equipment instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
	Medium
	

	4
	Pour and finish the concrete
	Wet concrete and cement burns
Heat stress
Sun exposure (UV)
	High
	- Use long-handled tools and pumps to cut down contact. [Engineering]
- Wash concrete off skin straight away with clean water. [Administrative]
- Have clean water and eye wash at the pour. [Administrative]
- Wear waterproof gloves, long sleeves and rubber boots with pants worn over the top. [PPE]
- Wear safety glasses or goggles to stop splashes. [PPE]
- Schedule heavy work for the cooler part of the day. [Elimination]
- Provide shade over work and rest areas, and fans or cooling in attics. [Engineering]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Administrative]
- Take regular rest breaks in the shade, more often as it gets hotter. [Administrative]
- Let new and returning workers build up to full work in the heat over about a week. [Administrative]
- Plan outdoor work for early morning or late afternoon when UV is lower. [Elimination]
- Put shade covers over fixed work areas. [Engineering]
- Check the UV index each day. Use sun protection when it is 3 or higher. [Administrative]
- Check your skin regularly and see a doctor about any new or changing spots. [Administrative]
- Wear a broad-brim hat or hard hat brim, long sleeves, sunglasses and SPF 30 or higher sunscreen, reapplied every 2 hours. [PPE]
	Medium
	

	5
	Saw cut control joints with water suppression
	Silica dust from concrete, brick, stone and tiles
Saw cuts and kickback
Loud noise
	Critical
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitution]
- Cut outdoors or in a separate area, with other people well away and upwind. [Engineering (guarding)]
- Use water on the blade or on-tool dust extraction connected to a HEPA vacuum. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- Have a silica exposure control plan where your province requires one. [Administrative]
- Wear a fit-tested N95 (or better) respirator. [PPE]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Engineering]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Engineering]
- Use a sharp, undamaged blade made for the material. [Administrative]
- Stand to one side of the blade line, out of the kickback path. [Administrative]
- Let the blade stop fully before reaching in or putting the saw down. [Administrative]
- If you have to shout to be heard 1 metre away, wear hearing protection. [Administrative]
- Wear earplugs or earmuffs rated for the noise. [PPE]
- Loud noise: see step 3 for the full controls [Administrative]
	Medium
	

	6
	Clean up, wash out away from drains and barricade until cured
	Poor housekeeping and waste
Public entering the work area
	High
	- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower buckets and booms, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving equipment or materials across public paths. [Administrative]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
High-visibility vest (CSA Z96)
Chemical-resistant gloves
Safety glasses (CSA Z94.3)
Hearing protection
Sun protection (sunscreen, hat, long sleeves)
Hard hat (CSA Z94.1)
Work gloves
Safety goggles
Knee pads
Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
N95 respirator
	Skid steer (Provincial operator training)
Plate tamper
Concrete saw (cut-off saw)
Hand tools
Concrete pump truck
	None required


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/concreting/driveway-concreting/
