FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Install outlets · Electrical · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Locate the circuit at the electrical panel, isolate it, apply lockout and tags and test to prove dead
	Electric shock from live wiring
	Critical
	- Isolate the power before any work. Do not work live. [Elimination]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Engineering (guarding)]
- Test before you touch: prove dead at the point of work with a tested voltage tester. [Engineering]
- Only licensed electricians do electrical work, to the Canadian Electrical Code and provincial rules. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If energized work cannot be avoided, use a permit, a safety observer and insulated tools, following CSA Z462. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium
	

	2
	Scan the wall for pipes and cables before cutting the hole
	Electric shock from live wiring
Gas and fuel lines
	Critical
	- Electric shock from live wiring: see step 1 for the full controls [Administrative]
- Isolate and purge the line before work, with the owner's approval. [Elimination]
- Lock off and tag the isolation valve. [Engineering (guarding)]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Engineering]
- Only licensed gas fitters work on gas lines. [Administrative]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Administrative]
- Know where the shut-off valve is and what to do if a leak happens. [Administrative]
- Wear safety glasses and gloves, and keep a fire extinguisher close by. [PPE]
	Medium
	

	3
	Cut in the box and run the cable, keeping dust down
	General dust
Injury from power tools
Falling from a ladder
	High
	- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitution]
- Seal off the work area with plastic sheeting in occupied buildings. [Engineering (guarding)]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
- Keep all guards fitted and working. Never tie back or remove a guard. [Engineering]
- Clamp or secure the work piece. Do not hold it by hand. [Engineering]
- Only trained, competent people use power tools, following the maker's instructions. [Administrative]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Administrative]
- No loose clothing, jewellery or long hair near spinning parts. [Administrative]
- Use a platform ladder, mobile scaffold or aerial work platform for longer jobs instead of a straight ladder. [Substitution]
- Use CSA Grade 1, 1A or 1AA ladders in good condition. Remove any damaged ladder from site. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the side rails. Do not overreach. [Administrative]
	Medium
	

	4
	Terminate the outlet and check connections are tight
	Electric shock from cords and power tools
Repetitive work and awkward postures
	High
	- Use battery-powered tools where you can. [Substitution]
- Use GFCI protection on all temporary power and portable tools. [Engineering]
- Keep cords off the ground and out of water, using stands or hooks. [Engineering]
- Check cords, plugs and tools before every use. Tag out and remove anything damaged. [Administrative]
- Do not use tools in rain or wet areas unless they are rated for it. [Administrative]
- Wear safety boots and dry gloves. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Substitution]
- Set work up at waist height on benches or trestles where you can. [Engineering]
- Use light tools with good grips, and keep blades and bits sharp. [Engineering]
- Rotate tasks and take short breaks every hour on repetitive work. [Administrative]
- Warm up before heavy physical work and report aches and pains early. [Administrative]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium
	

	5
	Test polarity, ground and GFCI protection, then restore power and clean up
	Electric shock from live wiring
Poor housekeeping and waste
	Critical
	- Electric shock from live wiring: see step 1 for the full controls [Administrative]
- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Safety glasses (CSA Z94.3)
Work gloves
Rubber insulating gloves
Arc flash PPE (CSA Z462)
N95 respirator
Hearing protection
Hard hat (CSA Z94.1)
Knee pads
	Electrical test meter
Power drill
Hand tools
	Lockout permit


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/electrical/power-point-installation/
