FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Window installation · Glazing · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check frames and paint for lead and asbestos
	Lead paint dust and fumes
Disturbing asbestos
	Critical
	- Test old paint for lead before you sand, scrape, cut or heat it. [Elimination]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Substitution]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Engineering (guarding)]
- Clean up with a HEPA vacuum and wet wipes. Never dry sweep. [Engineering]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Administrative]
- Wear a fit-tested respirator with P100 filters, disposable coveralls and gloves. [PPE]
- Get an asbestos survey before work on buildings built before 1990. [Elimination]
- Seal off the work area and keep everyone else out. [Engineering (guarding)]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with a HEPA vacuum. [Engineering]
- Follow your province's asbestos rules, including notification and trained or certified workers where required. [Administrative]
- In BC, a qualified person must inspect and write a hazardous materials report before demolition or renovation, and asbestos abatement must be done by a WorkSafeBC licensed contractor (since 1 January 2024). [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Wear a fit-tested respirator suited to the work, and disposable coveralls. [PPE]
	Medium
	

	2
	Protect occupants and furnishings and set exclusion areas inside and out
	Working in an occupied home or building
Public entering the work area
	High
	- Plan noisy, dusty or risky work for when the building is empty. [Elimination]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Engineering (guarding)]
- Keep fire exits and paths clear at all times. [Administrative]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Administrative]
- Lock away tools, chemicals and materials each day, out of reach of children. [Administrative]
- Clean up dust and debris at the end of each day. [Administrative]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower buckets and booms, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving equipment or materials across public paths. [Administrative]
	Low
	

	3
	Set up access for upper floor windows and barricade below
	Falling from height
Scaffold collapse or fall from scaffold
Falling tools and materials
	Critical
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Elimination]
- Install guardrails or edge protection on all open edges before work starts. [Engineering (guarding)]
- Use a scaffold, mobile work platform or aerial work platform instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Fall protection plan in place where required. Workers trained in fall protection (Working at Heights training in Ontario). [Administrative]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Administrative]
- Scaffold is built, altered and taken down only by trained workers supervised by a competent worker, on a firm base with sole boards and ties. [Engineering]
- Fit guardrails, mid rails and toe boards on every working platform. [Engineering]
- Use mobile scaffolds only on firm, level ground with castors locked and outriggers fitted. Never move one with anyone on it. [Engineering]
- A competent worker inspects the scaffold before use each shift, after any change and after bad weather, and tags every access point: green safe, yellow caution, red do not use. [Administrative]
- Do not overload platforms. Know the rated load and keep material stacks over the frames. [Administrative]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
	Medium
	

	4
	Remove beads and old glass first, wearing cut gloves
	Glass handling and breakage
Cuts from sharp edges
	High
	- Use suction lifters, glass trolleys or a glazing robot for large panes. [Engineering]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Engineering]
- Glass handling and breakage: see step 7 for the full controls [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Wear cut-resistant gloves and long sleeves. [PPE]
	Medium
	

	5
	Remove the old frame, guarding the open hole
	Falling through a floor opening or void
Lifting and carrying heavy loads
	Critical
	- Cover every hole and penetration with a fixed, secured cover marked "HOLE" or "DANGER". [Engineering (guarding)]
- Put guardrails with toe boards around stairwells, lift shafts, voids and open edges. [Engineering (guarding)]
- Install stairs early and fit temporary handrails as soon as they go in. [Engineering]
- Never remove a cover or guardrail without approval. Put it back straight away. [Administrative]
- Inspect covers and barriers daily and after other trades have been through. [Administrative]
- Keep lighting good enough to see openings, especially on lower floors and in the evening. [Administrative]
- Use a harness clipped to a rated anchor when working right next to an open void. [PPE]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Lifting and carrying heavy loads: see step 7 for the full controls [Administrative]
	Medium
	

	6
	Check the opening and lintel, and prop it if it is not sound
	Structural collapse during alterations
	High
	- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Elimination]
- Keep everyone clear of the area under and next to the work. [Engineering (guarding)]
- Install temporary props, needles or shoring as designed before removing any support. [Engineering]
- Follow the engineer's sequence. Do not change it without approval. [Administrative]
- Check props daily. Do not remove them until the permanent support is in and approved. [Administrative]
- Wear a hard hat and safety boots. [PPE]
	Medium
	

	7
	Lift new windows with two people or suction lifters
	Lifting and carrying heavy loads
Glass handling and breakage
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or equipment instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Use suction lifters, glass trolleys or a glazing robot for large panes. [Engineering]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Engineering]
- Use two or more people for large panes, and clear the carry route first. [Administrative]
- Mark new glass with tape or stickers so nobody walks into it. [Administrative]
- Clean up broken glass straight away into a marked container. [Administrative]
- Wear cut-resistant gloves, arm guards, safety glasses and safety boots. [PPE]
	Medium
	

	8
	Fix, pack, seal and flash the window
	Injury from power tools
Hazardous chemicals
	Medium
	- Keep all guards fitted and working. Never tie back or remove a guard. [Engineering]
- Clamp or secure the work piece. Do not hold it by hand. [Engineering]
- Only trained, competent people use power tools, following the maker's instructions. [Administrative]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Administrative]
- No loose clothing, jewellery or long hair near spinning parts. [Administrative]
- Wear safety glasses and hearing protection. Do not wear loose gloves on drills or other rotating tools. [PPE]
- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and WHMIS labels before use. Workers have WHMIS training. [Administrative]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
	Medium
	

	9
	Make good, then clean up broken glass and waste
	Poor housekeeping and waste
Cuts from sharp edges
	Medium
	- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
- Cuts from sharp edges: see step 4 for the full controls [Administrative]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Cut-resistant gloves
Safety glasses (CSA Z94.3)
Hard hat (CSA Z94.1)
Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
Coveralls
Work gloves
N95 respirator
High-visibility vest (CSA Z96)
Hearing protection
Chemical-resistant gloves
Safety goggles
	Power drill
Rolling scaffold (Provincial scaffold training)
Hand tools
Platform ladder
	Fall protection plan


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/ca/flha/glazing/window-installation/
