FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Rooftop unit replacement · HVAC · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Plan the crane lift and close the area below
	Crane and lifting failure
Public entering the work area
Contact with overhead power lines
	High
	- Barricade the lift zone and keep everyone out from under the load. [Engineering (guarding)]
- Use a crane rated for the load at the radius, set up on firm ground with outrigger pads. [Engineering]
- Check slings, chains, shackles and hooks before use. Remove anything damaged or not tagged. [Engineering]
- Plan the lift: weight, radius, ground, path and landing area. Use a written lift plan for complex lifts. [Administrative]
- Use certified crane operators and trained riggers and signallers, as your province requires. [Administrative]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower buckets and booms, remove ladders and lock tools away. [Administrative]
- Ask the utility to de-energize, move or insulate the lines before work starts. [Elimination]
- Use non-conductive (fibreglass) ladders near any power lines. [Substitution]
- Mark the safe distance with flags, tape or goal posts and keep all equipment and people outside it. [Engineering (guarding)]
- Keep to the provincial limits of approach and contact the utility before working near lines. [Administrative]
- Use a dedicated spotter whenever equipment moves or raises anything near lines. [Administrative]
- Treat all lines as live. If equipment touches a line, stay in the cab and keep everyone well away. [Administrative]
	Medium
	

	2
	Set up roof edge protection or harness anchors
	Falling from a roof edge
Falling through a fragile roof or skylight
	Critical
	- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Elimination]
- Install edge protection or guardrails on all open roof edges before work starts. [Engineering (guarding)]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Engineering]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Engineering]
- Use one safe, controlled access point and keep others off the roof. [Administrative]
- Stop roof work in strong wind or rain, and when the roof is wet, icy or covered in dust or frost. [Administrative]
- Wear a harness clipped to a rated anchor when using restraint or fall arrest, and soft-soled non-slip boots. [PPE]
- Work from underneath or from an aerial work platform so nobody stands on the fragile roof. [Elimination]
- Cover or guard every skylight and fragile sheet with a fixed, marked cover or mesh before work starts. [Engineering (guarding)]
- Install safety mesh under new roof sheeting, and use crawl boards or staging to spread the load on fragile surfaces. [Engineering]
- Use fall arrest on rated anchors when working near fragile areas. [Engineering]
- Treat all roof sheets as fragile until a competent person confirms they are not. Old fibre cement and plastic sheets are fragile. [Administrative]
- Put "Fragile roof" signs at every roof access point. [Administrative]
- Never walk on sheets between purlins or along skylights. Stay on boards or staging. [Administrative]
- Wear a full body harness clipped to a rated anchor. [PPE]
	Medium
	

	3
	Isolate power and gas, apply lockout and tags
	Electric shock from live wiring
Gas and fuel lines
	Critical
	- Isolate the power before any work. Do not work live. [Elimination]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Engineering (guarding)]
- Test before you touch: prove dead at the point of work with a tested voltage tester. [Engineering]
- Only licensed electricians do electrical work, to the Canadian Electrical Code and provincial rules. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If energized work cannot be avoided, use a permit, a safety observer and insulated tools, following CSA Z462. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
- Isolate and purge the line before work, with the owner's approval. [Elimination]
- Lock off and tag the isolation valve. [Engineering (guarding)]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Engineering]
- Only licensed gas fitters work on gas lines. [Administrative]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Administrative]
- Know where the shut-off valve is and what to do if a leak happens. [Administrative]
- Wear safety glasses and gloves, and keep a fire extinguisher close by. [PPE]
	Medium
	

	4
	Recover refrigerant before disconnecting
	Refrigerant leaks
	Medium
	- Recover refrigerant into an approved cylinder before opening the system. Never vent it. [Engineering (guarding)]
- Ventilate closed spaces and use a leak detector during the work. [Engineering]
- Only certified refrigeration technicians handle refrigerants, as your province requires. [Administrative]
- With flammable refrigerants (such as R32 or R290), remove ignition sources and use spark-free tools. [Administrative]
- Wear cold-rated gloves and safety glasses or a face shield. [PPE]
	Low
	

	5
	Lift out the old unit and set the new one, keeping clear of the load
	Crane and lifting failure
Falling tools and materials
Strong wind and storms
	High
	- Use tag lines to control loads and agree on clear radio or hand signals. [Administrative]
- Stop lifting in high wind or when the operator cannot see the signaller. [Administrative]
- Never ride on a load or hook. [Administrative]
- Crane and lifting failure: see step 1 for the full controls [Administrative]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Check the forecast each morning and plan work at height and lifting around the weather. [Elimination]
- Tie down or weigh down loose sheets, panels, boards and rubbish at the end of each shift. [Engineering]
- Set wind limits for roof work, platforms and cranes, using the manufacturer's limits, and stop when they are reached. [Administrative]
- Stop work and get down in lightning. Wait 30 minutes after the last thunder before going back up. [Administrative]
- Check scaffold, fencing and edge protection after strong wind before anyone uses them. [Administrative]
	Medium
	

	6
	Connect, commission and clean the roof
	Electric shock from live wiring
Poor housekeeping and waste
	Critical
	- Electric shock from live wiring: see step 3 for the full controls [Administrative]
- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Hard hat (CSA Z94.1)
Full body harness (fall arrest)
High-visibility vest (CSA Z96)
Work gloves
Safety glasses (CSA Z94.3)
Sun protection (sunscreen, hat, long sleeves)
Rubber insulating gloves
Arc flash PPE (CSA Z462)
Face shield
	Mobile crane (Provincial crane operator certification, qualified rigger)
Hand tools
Electrical test meter
Extension ladder
	Lift plan
Roof access permit
Fall protection plan
Lockout permit


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/ca/flha/hvac/rooftop-unit-replacement/
