FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Split system AC unit installation · HVAC · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Plan unit positions, checking walls for cables and pipes
	Electric shock from live wiring
Gas and fuel lines
	Critical
	- Isolate the power before any work. Do not work live. [Elimination]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Engineering (guarding)]
- Electric shock from live wiring: see step 8 for the full controls [Administrative]
- Isolate and purge the line before work, with the owner's approval. [Elimination]
- Lock off and tag the isolation valve. [Engineering (guarding)]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Engineering]
- Only licensed gas fitters work on gas lines. [Administrative]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Administrative]
- Know where the shut-off valve is and what to do if a leak happens. [Administrative]
- Wear safety glasses and gloves, and keep a fire extinguisher close by. [PPE]
	Medium
	

	2
	Set up a platform ladder or scaffold for high walls and the outdoor unit
	Falling from a ladder
Falling from height
	Critical
	- Use a platform ladder, mobile scaffold or aerial work platform for longer jobs instead of a straight ladder. [Substitution]
- Use CSA Grade 1, 1A or 1AA ladders in good condition. Remove any damaged ladder from site. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the side rails. Do not overreach. [Administrative]
- Do not stand on the top three rungs of an extension ladder or the top step of a stepladder. [Administrative]
- Check the ladder before each use: feet, rungs, side rails and locks. [Administrative]
- Wear non-slip safety boots with clean soles. [PPE]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Elimination]
- Install guardrails or edge protection on all open edges before work starts. [Engineering (guarding)]
- Use a scaffold, mobile work platform or aerial work platform instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Fall protection plan in place where required. Workers trained in fall protection (Working at Heights training in Ontario). [Administrative]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Administrative]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
	Medium
	

	3
	Core drill the wall with dust extraction
	Silica dust from concrete, brick, stone and tiles
Loud noise
Injury from power tools
	Critical
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitution]
- Cut outdoors or in a separate area, with other people well away and upwind. [Engineering (guarding)]
- Use water on the blade or on-tool dust extraction connected to a HEPA vacuum. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- Have a silica exposure control plan where your province requires one. [Administrative]
- Wear a fit-tested N95 (or better) respirator. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy equipment away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard 1 metre away, wear hearing protection. [Administrative]
- Keep all guards fitted and working. Never tie back or remove a guard. [Engineering]
- Clamp or secure the work piece. Do not hold it by hand. [Engineering]
- Only trained, competent people use power tools, following the maker's instructions. [Administrative]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Administrative]
- No loose clothing, jewellery or long hair near spinning parts. [Administrative]
	Medium
	

	4
	Fix the wall bracket and mount the indoor unit
	Falling from a ladder
Lifting and carrying heavy loads
	High
	- Falling from a ladder: see step 2 for the full controls [Administrative]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Lifting and carrying heavy loads: see step 5 for the full controls [Administrative]
	Medium
	

	5
	Lift the outdoor unit with two people onto its bracket or pad
	Lifting and carrying heavy loads
Falling from height
	Critical
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or equipment instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Falling from height: see step 2 for the full controls [Administrative]
	Medium
	

	6
	Run and flare the pipework, brazing only under a hot work permit
	Refrigerant leaks
Fire from hot works
Burns from hot surfaces
	Critical
	- Recover refrigerant into an approved cylinder before opening the system. Never vent it. [Engineering (guarding)]
- Ventilate closed spaces and use a leak detector during the work. [Engineering]
- Only certified refrigeration technicians handle refrigerants, as your province requires. [Administrative]
- With flammable refrigerants (such as R32 or R290), remove ignition sources and use spark-free tools. [Administrative]
- Wear cold-rated gloves and safety glasses or a face shield. [PPE]
- Use cold work methods where you can, such as bolting, press fittings or cutting with a saw instead of a torch. [Elimination]
- Move anything that can burn at least 10 metres away, or cover it with fire blankets. [Engineering (guarding)]
- Use fire-resistant screens to stop sparks reaching people or gaps in walls and floors. [Engineering]
- Get a hot work permit before starting. [Administrative]
- Keep a charged fire extinguisher and fire blanket at the work spot. [Administrative]
- Isolate heating systems and let parts cool before you touch them. [Elimination]
- Fit guards or insulation on hot pipes and equipment. [Engineering]
- Mark hot items with chalk or a "HOT" sign so others know. [Administrative]
- Keep a first aid kit and cool running water nearby for burns. [Administrative]
- Wear heat-resistant gloves and long sleeves. [PPE]
	Medium
	

	7
	Pressure test with dry nitrogen through a regulator, keeping clear of fittings under pressure
	Pressure testing
	Medium
	- Test with water instead of air or gas where the system allows it. Never put water in refrigerant pipework, which is tested with dry nitrogen. [Substitution]
- Keep people out of the test area with signs and barriers. [Engineering (guarding)]
- Use a calibrated gauge and a relief valve set to protect the system. [Engineering]
- Test to the pressure the system calls for and hold it for the set time. Never go over. [Administrative]
- Release the pressure fully before tightening anything or fixing leaks. [Administrative]
- Wear safety glasses or a face shield. [PPE]
	Low
	

	8
	Electrical connection by a licensed electrician, with the circuit isolated
	Electric shock from live wiring
	Critical
	- Isolate the power before any work. Do not work live. [Elimination]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Engineering (guarding)]
- Test before you touch: prove dead at the point of work with a tested voltage tester. [Engineering]
- Only licensed electricians do electrical work, to the Canadian Electrical Code and provincial rules. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If energized work cannot be avoided, use a permit, a safety observer and insulated tools, following CSA Z462. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium
	

	9
	Vacuum the system, open the service valves to let the outdoor unit's factory charge into the pipework, then commission
	Refrigerant leaks
	Medium
	- Refrigerant leaks: see step 6 for the full controls [Administrative]
	Low
	

	10
	Clean up and show the client how to use the system
	Poor housekeeping and waste
	Medium
	- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Safety glasses (CSA Z94.3)
Work gloves
N95 respirator
Hearing protection
Rubber insulating gloves
Arc flash PPE (CSA Z462)
Hard hat (CSA Z94.1)
Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
Face shield
Welding gloves
Coveralls
	Power drill
Core drill
Extension ladder
Electrical test meter
Hand tools
	Lockout permit
Hot work permit


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/ca/flha/hvac/split-system-installation/
