FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Tree removal and pruning with a chainsaw · Landscaping · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Assess the tree for lean, decay and dead wood, check for power lines and buildings, and plan escape routes; keep 2 tree lengths clear when felling
	Contact with overhead power lines
Falling tools and materials
	High
	- Ask the utility to de-energize, move or insulate the lines before work starts. [Elimination]
- Use non-conductive (fibreglass) ladders near any power lines. [Substitution]
- Mark the safe distance with flags, tape or goal posts and keep all equipment and people outside it. [Engineering (guarding)]
- Keep to the provincial limits of approach and contact the utility before working near lines. [Administrative]
- Use a dedicated spotter whenever equipment moves or raises anything near lines. [Administrative]
- Treat all lines as live. If equipment touches a line, stay in the cab and keep everyone well away. [Administrative]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Falling tools and materials: see step 7 for the full controls [Administrative]
	Medium
	

	2
	Set up the drop zone with barriers and traffic or pedestrian control
	Public entering the work area
Road traffic
	Critical
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower buckets and booms, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving equipment or materials across public paths. [Administrative]
- Do the work at low-traffic times, or close the road or lane with approval. [Elimination]
- Put solid barriers between the work and traffic where speeds are high, not just cones. [Engineering (guarding)]
- Use a truck-mounted attenuator or buffer vehicle on high speed roads. [Engineering]
- Set up signs and cones to your provincial traffic control manual, with trained traffic control persons. [Administrative]
- Get a road occupancy permit from the municipality or road authority before you start. [Administrative]
- Park work vehicles to shield the work zone, with beacons on. [Administrative]
- Wear high-visibility clothing to CSA Z96. [PPE]
	Medium
	

	3
	Check the chainsaw, chain brake and PPE before starting
	Chainsaw injuries
Loud noise
	High
	- Use a different tool where you can, such as a pole saw or hand saw for small branches. [Substitution]
- Use a saw with a working chain brake, chain catcher and low-kickback chain, kept sharp and tensioned. [Engineering]
- Only trained operators use chainsaws. [Administrative]
- Never cut above shoulder height or from a ladder. [Administrative]
- When felling, keep everyone at least two tree lengths away. [Administrative]
- Wear chainsaw chaps, chainsaw boots, gloves, a helmet with face screen and hearing protection. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy equipment away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Loud noise: see step 10 for the full controls [Administrative]
	Medium
	

	4
	Look for nests, wasps and snakes before climbing or cutting
	Bites and stings
	Medium
	- Check work areas before starting, and get pest control to remove nests. [Elimination]
- Look before you reach into dark spaces. [Administrative]
- Ask owners to keep pets away from the work area. [Administrative]
- Know who has allergies and keep their medication, such as an epinephrine auto-injector, close by. [Administrative]
- Wear gloves, long sleeves and boots. Use insect repellent outdoors. [PPE]
	Medium
	

	5
	Set up the aerial work platform on firm ground outside the drop zone
	Aerial work platform tip-over or crush
Contact with overhead power lines
	Critical
	- Check the ground before setting up. Use outriggers and spreader pads, and keep clear of trenches, pits and slopes. [Engineering]
- Use a platform with tilt alarm and secondary guarding (anti-entrapment) where there is an overhead crush risk. [Engineering]
- Operators are trained to CSA B354.8 and the manufacturer's instructions, and the platform is inspected to CSA B354.7. [Administrative]
- Do a pre-start check each day. Keep a trained person on the ground who can lower the platform in an emergency. [Administrative]
- Never exceed the safe working load, climb on the rails or use a ladder in the basket. [Administrative]
- In boom-type platforms, wear a harness clipped to the basket anchor point. [PPE]
- Contact with overhead power lines: see step 1 for the full controls [Administrative]
	Medium
	

	6
	Cut from the ground or the aerial work platform, never from a ladder
	Falling from height
Chainsaw injuries
	Critical
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Elimination]
- Install guardrails or edge protection on all open edges before work starts. [Engineering (guarding)]
- Use a scaffold, mobile work platform or aerial work platform instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Fall protection plan in place where required. Workers trained in fall protection (Working at Heights training in Ontario). [Administrative]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Administrative]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
- Chainsaw injuries: see step 3 for the full controls [Administrative]
	Medium
	

	7
	Drop limbs in sections into the clear drop zone. Before cutting bent or loaded wood, work out which side is under tension and stand clear of where it will spring
	Falling tools and materials
	High
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Administrative]
- Wear a hard hat anywhere objects could fall. [PPE]
	Medium
	

	8
	Fell the stem with a scarf cut on the felling side and a back cut that leaves a hinge, call a warning, then step back along the planned escape route
	Falling tools and materials
Chainsaw injuries
	High
	- Falling tools and materials: see step 7 for the full controls [Administrative]
- Chainsaw injuries: see step 3 for the full controls [Administrative]
	Medium
	

	9
	Refuel with the engine off and the saw cool, on bare ground away from ignition, using an approved fuel can, with an extinguisher at the vehicle
	Fire and emergencies
	High
	- Provide fire extinguishers suited to the site, checked and easy to reach. [Engineering]
- Keep exits and escape routes clear and signed. [Engineering]
- Have a site emergency plan: alarm, exits, assembly point and emergency contacts. [Administrative]
- Keep a stocked first aid kit and at least one trained first aider on site. [Administrative]
- Know the site address and how emergency services get in. Call 911. [Administrative]
- Go through the emergency plan with every worker and visitor at induction. [Administrative]
- Keep flammable materials and rubbish away from exits and escape routes. [Administrative]
	Medium
	

	10
	Chip or stack wood: feed the chipper butt first from the side, never reach past the feed control bar or kick material in, and stop and isolate it before clearing a jam; then clean up
	Lifting and carrying heavy loads
Hand-arm and whole-body vibration
Loud noise
Poor housekeeping and waste
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or equipment instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Substitution]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Engineering]
- Limit trigger time on high-vibration tools and rotate workers. [Administrative]
- Keep hands warm and dry, and take regular breaks. [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy equipment away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Chainsaw pants or chaps
Hard hat (CSA Z94.1)
Face shield
Hearing protection
Work gloves
CSA green triangle safety boots (CSA Z195)
High-visibility vest (CSA Z96)
Safety glasses (CSA Z94.3)
Cut-resistant gloves
Coveralls
Full body harness (fall arrest)
	Chainsaw
Boom lift (Provincial aerial work platform operator training (CSA B354.8))
Trailer
Hand tools
	Fall protection plan


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/landscaping/tree-removal/
