FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Lead paint removal · Painting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Test the paint, tell the occupants, and keep children and pregnant people away
	Lead paint dust and fumes
Working in an occupied home or building
	High
	- Test old paint for lead before you sand, scrape, cut or heat it. [Elimination]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Substitution]
- Lead paint dust and fumes: see step 8 for the full controls [Administrative]
- Plan noisy, dusty or risky work for when the building is empty. [Elimination]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Engineering (guarding)]
- Keep fire exits and paths clear at all times. [Administrative]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Administrative]
- Lock away tools, chemicals and materials each day, out of reach of children. [Administrative]
- Clean up dust and debris at the end of each day. [Administrative]
	Low
	

	2
	Turn off heating and cooling and close windows and vents in the work area
	Lead paint dust and fumes
General dust
	High
	- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Engineering (guarding)]
- Clean up with a HEPA vacuum and wet wipes. Never dry sweep. [Engineering]
- Lead paint dust and fumes: see step 8 for the full controls [Administrative]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitution]
- Seal off the work area with plastic sheeting in occupied buildings. [Engineering (guarding)]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
- Wear a dust mask and safety glasses. [PPE]
	Low
	

	3
	Seal the area with plastic and warning signs
	Lead paint dust and fumes
Public entering the work area
	High
	- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Administrative]
- Wear a fit-tested respirator with P100 filters, disposable coveralls and gloves. [PPE]
- Lead paint dust and fumes: see step 8 for the full controls [Administrative]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower buckets and booms, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving equipment or materials across public paths. [Administrative]
	Low
	

	4
	Put on coveralls and a fitted respirator, and set up a wash point
	Lead paint dust and fumes
Hazardous chemicals
	High
	- Lead paint dust and fumes: see step 8 for the full controls [Administrative]
- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Hazardous chemicals: see step 6 for the full controls [Administrative]
	Medium
	

	5
	Mist and wet scrape the paint; no dry sanding or open flame
	Lead paint dust and fumes
Hazardous chemicals
	High
	- Lead paint dust and fumes: see step 8 for the full controls [Administrative]
- Read the Safety Data Sheet (SDS) and WHMIS labels before use. Workers have WHMIS training. [Administrative]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Administrative]
- Hazardous chemicals: see step 6 for the full controls [Administrative]
	Medium
	

	6
	Use chemical strippers with ventilation and chemical gloves
	Hazardous chemicals
Flammable liquids and gases
	High
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and WHMIS labels before use. Workers have WHMIS training. [Administrative]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Use non-flammable or water-based products where you can. [Substitution]
- Keep ignition sources away: no smoking, no hot work and no running engines near flammables. [Engineering (guarding)]
- Store fuels and solvents in approved, closed containers in a ventilated area away from the work. [Engineering]
- Refuel equipment outdoors with the engine off and cool. [Administrative]
- Keep only what you need for the day on site. [Administrative]
- Store gas cylinders upright, secured and outdoors. [Administrative]
- Keep a suitable fire extinguisher where flammables are used or stored. [Administrative]
- Wear chemical gloves and safety glasses when pouring or mixing. [PPE]
	Medium
	

	7
	Use a heat gun only on low settings, below the temperature that makes lead fumes
	Burns from hot surfaces
Fire from hot works
Lead paint dust and fumes
	Critical
	- Isolate heating systems and let parts cool before you touch them. [Elimination]
- Fit guards or insulation on hot pipes and equipment. [Engineering]
- Mark hot items with chalk or a "HOT" sign so others know. [Administrative]
- Keep a first aid kit and cool running water nearby for burns. [Administrative]
- Wear heat-resistant gloves and long sleeves. [PPE]
- Use cold work methods where you can, such as bolting, press fittings or cutting with a saw instead of a torch. [Elimination]
- Move anything that can burn at least 10 metres away, or cover it with fire blankets. [Engineering (guarding)]
- Use fire-resistant screens to stop sparks reaching people or gaps in walls and floors. [Engineering]
- Get a hot work permit before starting. [Administrative]
- Keep a charged fire extinguisher and fire blanket at the work spot. [Administrative]
- Lead paint dust and fumes: see step 8 for the full controls [Administrative]
	Medium
	

	8
	Clean with an H-class vacuum and wet wipes, never dry sweep
	Lead paint dust and fumes
Poor housekeeping and waste
	High
	- Test old paint for lead before you sand, scrape, cut or heat it. [Elimination]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Substitution]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Engineering (guarding)]
- Clean up with a HEPA vacuum and wet wipes. Never dry sweep. [Engineering]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Administrative]
- Wear a fit-tested respirator with P100 filters, disposable coveralls and gloves. [PPE]
- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	

	9
	Bag waste, remove coveralls in the work area and wash before eating
	Lead paint dust and fumes
	High
	- Lead paint dust and fumes: see step 8 for the full controls [Administrative]
	Low
	

	10
	Check the area is clean before removing plastic and letting occupants back in
	Lead paint dust and fumes
Working in an occupied home or building
	High
	- Lead paint dust and fumes: see step 8 for the full controls [Administrative]
- Working in an occupied home or building: see step 1 for the full controls [Administrative]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety glasses (CSA Z94.3)
Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
Coveralls
Chemical-resistant gloves
CSA green triangle safety boots (CSA Z195)
Work gloves
N95 respirator
High-visibility vest (CSA Z96)
Safety goggles
Welding gloves
Face shield
	Heat gun
HEPA vacuum
Power sander
Hand tools
	Hot work permit


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/painting/lead-paint-removal/
