FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Pressure washing and surface prep · Painting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Cover power points and outside lights, and keep leads off wet ground
	Electric shock from cords and power tools
Electric shock from live wiring
	Critical
	- Use battery-powered tools where you can. [Substitution]
- Use GFCI protection on all temporary power and portable tools. [Engineering]
- Keep cords off the ground and out of water, using stands or hooks. [Engineering]
- Check cords, plugs and tools before every use. Tag out and remove anything damaged. [Administrative]
- Do not use tools in rain or wet areas unless they are rated for it. [Administrative]
- Wear safety boots and dry gloves. [PPE]
- Isolate the power before any work. Do not work live. [Elimination]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Engineering (guarding)]
- Test before you touch: prove dead at the point of work with a tested voltage tester. [Engineering]
- Only licensed electricians do electrical work, to the Canadian Electrical Code and provincial rules. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If energized work cannot be avoided, use a permit, a safety observer and insulated tools, following CSA Z462. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium
	

	2
	Check surfaces for asbestos and lead paint first
	Disturbing asbestos
Lead paint dust and fumes
	Critical
	- Get an asbestos survey before work on buildings built before 1990. [Elimination]
- Seal off the work area and keep everyone else out. [Engineering (guarding)]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with a HEPA vacuum. [Engineering]
- Follow your province's asbestos rules, including notification and trained or certified workers where required. [Administrative]
- In BC, a qualified person must inspect and write a hazardous materials report before demolition or renovation, and asbestos abatement must be done by a WorkSafeBC licensed contractor (since 1 January 2024). [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Wear a fit-tested respirator suited to the work, and disposable coveralls. [PPE]
- Test old paint for lead before you sand, scrape, cut or heat it. [Elimination]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Substitution]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Engineering (guarding)]
- Clean up with a HEPA vacuum and wet wipes. Never dry sweep. [Engineering]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Administrative]
- Wear a fit-tested respirator with P100 filters, disposable coveralls and gloves. [PPE]
	Medium
	

	3
	Never use the pressure washer from a ladder
	Falling from a ladder
High pressure water jetting
	High
	- Use a platform ladder, mobile scaffold or aerial work platform for longer jobs instead of a straight ladder. [Substitution]
- Use CSA Grade 1, 1A or 1AA ladders in good condition. Remove any damaged ladder from site. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the side rails. Do not overreach. [Administrative]
- Do not stand on the top three rungs of an extension ladder or the top step of a stepladder. [Administrative]
- Check the ladder before each use: feet, rungs, side rails and locks. [Administrative]
- Wear non-slip safety boots with clean soles. [PPE]
- Set an exclusion zone around the jetting area. [Engineering (guarding)]
- Use a dead man's trigger that stops the jet when released, and check hoses and fittings before use. [Engineering]
- Only trained operators use high pressure jetting gear. [Administrative]
- Never point the lance at anyone or put a hand in front of it. [Administrative]
- Treat any jetting injury as serious and go to hospital, even if it looks small. [Administrative]
- Wear a face shield, waterproof clothing, gloves, hearing protection and safety boots. [PPE]
	Medium
	

	4
	Mix and apply cleaning chemicals as the label says
	Hazardous chemicals
	Medium
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and WHMIS labels before use. Workers have WHMIS training. [Administrative]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
	Medium
	

	5
	Wash down, keeping the lance away from people
	High pressure water jetting
Loud noise
Slips and trips
	High
	- High pressure water jetting: see step 3 for the full controls [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy equipment away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard 1 metre away, wear hearing protection. [Administrative]
- Plan walkways and keep them clear of materials, hoses and leads. [Elimination]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Engineering]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Engineering]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Administrative]
- Keep work areas, stairs and access paths well lit. [Administrative]
	Medium
	

	6
	Stop runoff entering storm drain drains and clean up
	Poor housekeeping and waste
	Medium
	- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Safety goggles
Chemical-resistant gloves
Hearing protection
Work gloves
Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
Coveralls
Hard hat (CSA Z94.1)
Face shield
	Pressure washer
Extension ladder
Portable generator
	None required


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/painting/pressure-washing-prep/
