FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Suspended ceiling installation · Drywall · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Plan aerial work platform use and close the area below
	Aerial work platform tip-over or crush
Falling tools and materials
	Critical
	- Check the ground before setting up. Use outriggers and spreader pads, and keep clear of trenches, pits and slopes. [Engineering]
- Use a platform with tilt alarm and secondary guarding (anti-entrapment) where there is an overhead crush risk. [Engineering]
- Operators are trained to CSA B354.8 and the manufacturer's instructions, and the platform is inspected to CSA B354.7. [Administrative]
- Do a pre-start check each day. Keep a trained person on the ground who can lower the platform in an emergency. [Administrative]
- Never exceed the safe working load, climb on the rails or use a ladder in the basket. [Administrative]
- In boom-type platforms, wear a harness clipped to the basket anchor point. [PPE]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Administrative]
- Wear a hard hat anywhere objects could fall. [PPE]
	Medium
	

	2
	Drill fixings into the slab with dust extraction
	Silica dust from concrete, brick, stone and tiles
Loud noise
Injury from power tools
	Critical
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitution]
- Cut outdoors or in a separate area, with other people well away and upwind. [Engineering (guarding)]
- Use water on the blade or on-tool dust extraction connected to a HEPA vacuum. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- Have a silica exposure control plan where your province requires one. [Administrative]
- Wear a fit-tested N95 (or better) respirator. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy equipment away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- If you have to shout to be heard 1 metre away, wear hearing protection. [Administrative]
- Keep all guards fitted and working. Never tie back or remove a guard. [Engineering]
- Clamp or secure the work piece. Do not hold it by hand. [Engineering]
- Only trained, competent people use power tools, following the maker's instructions. [Administrative]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Administrative]
- No loose clothing, jewellery or long hair near spinning parts. [Administrative]
	Medium
	

	3
	Hang grid and wires, watching sharp grid ends
	Cuts from sharp edges
Repetitive work and awkward postures
	Medium
	- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Wear cut-resistant gloves and long sleeves. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Substitution]
- Set work up at waist height on benches or trestles where you can. [Engineering]
- Use light tools with good grips, and keep blades and bits sharp. [Engineering]
- Rotate tasks and take short breaks every hour on repetitive work. [Administrative]
- Warm up before heavy physical work and report aches and pains early. [Administrative]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium
	

	4
	Drop in tiles and clean up
	General dust
Poor housekeeping and waste
	Medium
	- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitution]
- Seal off the work area with plastic sheeting in occupied buildings. [Engineering (guarding)]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
- Wear a dust mask and safety glasses. [PPE]
- Order materials to size and send packaging back where you can. [Elimination]
- Put waste bins and chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Safety glasses (CSA Z94.3)
Hard hat (CSA Z94.1)
N95 respirator
Cut-resistant gloves
Full body harness (fall arrest)
High-visibility vest (CSA Z96)
Respirator fit tested to CSA Z94.4 (P100 for dust, or the type the air test calls for)
Hearing protection
Work gloves
Knee pads
	Scissor lift (Provincial aerial work platform operator training (CSA B354.8))
Platform ladder
Power drill
Rotary hammer
Hand tools
	Fall protection plan


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/plastering/suspended-ceiling-installation/
