FIELD LEVEL HAZARD ASSESSMENT (FLHA)
Install roof edge protection · Scaffolding · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Plan the system to suit the roof pitch and gutter height
	Falling from a roof edge
	Critical
	- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Elimination]
- Install edge protection or guardrails on all open roof edges before work starts. [Engineering (guarding)]
- Falling from a roof edge: see step 2 for the full controls [Administrative]
	Medium
	

	2
	Install from a aerial work platform or scaffold, or harnessed to an anchor
	Falling from a roof edge
Aerial work platform tip-over or crush
Falling from height
	Critical
	- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Elimination]
- Install edge protection or guardrails on all open roof edges before work starts. [Engineering (guarding)]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Engineering]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Engineering]
- Use one safe, controlled access point and keep others off the roof. [Administrative]
- Check the ground before setting up. Use outriggers and spreader pads, and keep clear of trenches, pits and slopes. [Engineering]
- Use a platform with tilt alarm and secondary guarding (anti-entrapment) where there is an overhead crush risk. [Engineering]
- Operators are trained to CSA B354.8 and the manufacturer's instructions, and the platform is inspected to CSA B354.7. [Administrative]
- Do a pre-start check each day. Keep a trained person on the ground who can lower the platform in an emergency. [Administrative]
- Never exceed the safe working load, climb on the rails or use a ladder in the basket. [Administrative]
- In boom-type platforms, wear a harness clipped to the basket anchor point. [PPE]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Elimination]
- Install guardrails or edge protection on all open edges before work starts. [Engineering (guarding)]
- Use a scaffold, mobile work platform or aerial work platform instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Fall protection plan in place where required. Workers trained in fall protection (Working at Heights training in Ontario). [Administrative]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Administrative]
	Medium
	

	3
	Fix brackets into sound structure
	Structural collapse during alterations
Injury from power tools
	High
	- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Elimination]
- Keep everyone clear of the area under and next to the work. [Engineering (guarding)]
- Install temporary props, needles or shoring as designed before removing any support. [Engineering]
- Follow the engineer's sequence. Do not change it without approval. [Administrative]
- Check props daily. Do not remove them until the permanent support is in and approved. [Administrative]
- Wear a hard hat and safety boots. [PPE]
- Keep all guards fitted and working. Never tie back or remove a guard. [Engineering]
- Clamp or secure the work piece. Do not hold it by hand. [Engineering]
- Only trained, competent people use power tools, following the maker's instructions. [Administrative]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Administrative]
- No loose clothing, jewellery or long hair near spinning parts. [Administrative]
- Wear safety glasses and hearing protection. Do not wear loose gloves on drills or other rotating tools. [PPE]
	Medium
	

	4
	Fit rails and mesh, keeping tools tethered
	Falling tools and materials
Lifting and carrying heavy loads
	High
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Administrative]
- Wear a hard hat anywhere objects could fall. [PPE]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or equipment instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium
	

	5
	Inspect and hand over before roof work starts
	Falling from a roof edge
	Critical
	- Stop roof work in strong wind or rain, and when the roof is wet, icy or covered in dust or frost. [Administrative]
- Wear a harness clipped to a rated anchor when using restraint or fall arrest, and soft-soled non-slip boots. [PPE]
- Falling from a roof edge: see step 2 for the full controls [Administrative]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	CSA green triangle safety boots (CSA Z195)
Full body harness (fall arrest)
Hard hat (CSA Z94.1)
Work gloves
Sun protection (sunscreen, hat, long sleeves)
High-visibility vest (CSA Z96)
Safety glasses (CSA Z94.3)
Hearing protection
	Frame scaffold (Provincial scaffold erector training)
Boom lift (Provincial aerial work platform operator training (CSA B354.8))
Hand tools
Power drill
	Roof access permit
Fall protection plan


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Muster point
	

	First aid attendant
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Provincial occupational health and safety law (e.g. Ontario OHSA and O. Reg. 213/91, BC OHS Regulation, Alberta OHS Code).
Keep completed hazard assessments for at least 3 years (COR auditors sample the last 12 months). Review this FLHA and re-sign whenever the task, crew or conditions change.
6. END OF SHIFT REVIEW
	Area cleaned up and safe (yes / no)
	

	Permits closed
	

	Incidents or near misses
	

	Hazards remaining
	


7. SIGN-OFF
By signing below, each person confirms they have read and understood this FLHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/ca/flha/scaffolding/roof-edge-protection-install/
