RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Brick cleaning and acid washing · Bricklaying · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Read the safety data sheet and set up an eyewash
	Hazardous chemicals
	Workers, Occupants
	Medium (9)
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Reduce / substitute]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Control (engineering)]
- Do a COSHH assessment and read the Safety Data Sheet (SDS) before use. [Control (procedures)]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Control (procedures)]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Control (procedures)]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Control (procedures)]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
	Medium (6)
	

	2
	Protect windows, plants and drains
	Hazardous chemicals
Public entering the work area
	Workers, Occupants, Public, Children
	High (12)
	- Hazardous chemicals: see step 1 for the full controls [Control (procedures)]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Control (engineering)]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Control (procedures)]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Control (procedures)]
- Use a spotter when moving plant or materials across public paths. [Control (procedures)]
	Medium (6)
	

	3
	Always add acid to water, never water to acid
	Hazardous chemicals
Eye injuries
	Workers, Occupants, People nearby
	Medium (9)
	- Hazardous chemicals: see step 1 for the full controls [Control (procedures)]
- Use tool guards and screens to stop flying particles. [Control (engineering)]
- Use dust extraction and water to keep dust out of the air. [Control (engineering)]
- Keep others out of the area when cutting, grinding or chipping. [Control (procedures)]
- Keep an eye wash station or eye wash bottles on site. [Control (procedures)]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
	Medium (6)
	

	4
	Apply and wash off from the bottom up
	High pressure water jetting
Slips and trips
	Workers, People nearby, Visitors, Public
	Medium (8)
	- Set an exclusion zone around the jetting area. [Isolate]
- Use a dead man's trigger that stops the jet when released, and check hoses and fittings before use. [Control (engineering)]
- Only trained operators use high pressure jetting gear. [Control (procedures)]
- Never point the lance at anyone or put a hand in front of it. [Control (procedures)]
- Treat any jetting injury as serious and go to hospital, even if it looks small. [Control (procedures)]
- Wear a face shield, waterproof clothing, gloves, hearing protection and safety boots. [PPE]
- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Control (engineering)]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Control (engineering)]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Control (procedures)]
- Keep work areas, stairs and access paths well lit. [Control (procedures)]
- Wear safety boots with good grip, laced up. [PPE]
	Low (4)
	

	5
	Neutralise and dispose of runoff, then clean up
	Poor housekeeping and waste
	Workers, Visitors
	Medium (8)
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Read the safety data sheet and set up an eyewash
2. Protect windows, plants and drains
3. Always add acid to water, never water to acid
4. Apply and wash off from the bottom up
5. Neutralise and dispose of runoff, then clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety goggles
Face shield
Chemical-resistant gloves
Coveralls
Safety boots
Half-mask respirator (P3 filters)
Hi-vis vest
Safety glasses
Rigger gloves
Ear defenders
	Pressure washer (jet wash)
Knapsack sprayer (City and Guilds PA1 and PA6 (or Lantra equivalent) for pesticides)
Mobile access tower (PASMA certificate)
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/bricklaying/brick-cleaning/
