RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Brick repointing · Bricklaying · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up access and barricade below
	Falling from height
Public entering the work area
	Workers, People below, Public, Children
	Very high (20)
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile tower or MEWP instead of working off a ladder. [Control (engineering)]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Control (engineering)]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Control (procedures)]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Control (engineering)]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Control (procedures)]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Control (procedures)]
- Use a spotter when moving plant or materials across public paths. [Control (procedures)]
	Medium (5)
	

	2
	Rake out joints with a grinder on extraction, wearing a respirator
	Silica dust from concrete, brick, stone and tiles
Angle grinder injuries
Loud noise
Eye injuries
	Workers, People nearby
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Silica dust from concrete, brick, stone and tiles: see step 4 for the full controls [Control (procedures)]
- Use a guarded saw or a different tool where you can. [Reduce / substitute]
- Keep the guard on and use the side handle. Never remove the guard. [Control (engineering)]
- Use the right disc for the job, rated for the grinder's speed. Check it for cracks first. [Control (procedures)]
- Only trained people change discs, with the grinder unplugged or the battery out. [Control (procedures)]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
- Use tool guards and screens to stop flying particles. [Control (engineering)]
- Use dust extraction and water to keep dust out of the air. [Control (engineering)]
- Keep others out of the area when cutting, grinding or chipping. [Control (procedures)]
- Keep an eye wash station or eye wash bottles on site. [Control (procedures)]
	Medium (8)
	

	3
	Mix and apply mortar
	Wet concrete and cement burns
Repetitive work and awkward postures
	Workers
	Medium (9)
	- Use long-handled tools and pumps to cut down contact. [Control (engineering)]
- Wash concrete off skin straight away with clean water. [Control (procedures)]
- Have clean water and eye wash where concrete or mortar is mixed and used. [Control (procedures)]
- Do a COSHH assessment for cement, lime and mortar, and check hands regularly for early signs of dermatitis. [Control (procedures)]
- Wear waterproof gloves, long sleeves and waterproof boots with trousers worn over the top. [PPE]
- Wear safety glasses or goggles to stop splashes. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Reduce / substitute]
- Set work up at waist height on benches or trestles where you can. [Control (engineering)]
- Use light tools with good grips, and keep blades and bits sharp. [Control (engineering)]
- Rotate tasks and take short breaks every hour on repetitive work. [Control (procedures)]
- Warm up before heavy physical work and report aches and pains early. [Control (procedures)]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium (6)
	

	4
	Clean down and vacuum dust
	Silica dust from concrete, brick, stone and tiles
Poor housekeeping and waste
	Workers, People nearby, Visitors
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Medium (5)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Set up access and barricade below
2. Rake out joints with a grinder on extraction, wearing a respirator
3. Mix and apply mortar
4. Clean down and vacuum dust
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety glasses
Half-mask respirator (P3 filters)
Ear defenders
Rigger gloves
Safety boots
Hi-vis vest
Face shield
Cut-resistant gloves
Safety goggles
Chemical-resistant gloves
Knee pads
	Angle grinder (disc cutter)
Mobile access tower (PASMA certificate)
H-class dust extractor
Hand tools
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/uk/rams/bricklaying/repointing/
