RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Stair installation · Carpentry · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Guard the stair void before and during installation
	Falling through a floor opening or void
Falling from height
	Workers, Visitors, People below
	Very high (20)
	- Cover every hole and penetration with a fixed, secured cover marked "HOLE" or "DANGER". [Isolate]
- Put guardrails with toe boards around stairwells, lift shafts, voids and open edges. [Isolate]
- Install stairs early and fit temporary handrails as soon as they go in. [Control (engineering)]
- Never remove a cover or guardrail without approval. Put it back straight away. [Control (procedures)]
- Inspect covers and barriers daily and after other trades have been through. [Control (procedures)]
- Keep lighting good enough to see openings, especially on lower floors and in the evening. [Control (procedures)]
- Use a harness clipped to a rated anchor when working right next to an open void. [PPE]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile tower or MEWP instead of working off a ladder. [Control (engineering)]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Control (engineering)]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Control (procedures)]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
	Medium (5)
	

	2
	Move stair parts in with enough people
	Lifting and carrying heavy loads
	Workers
	High (12)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium (6)
	

	3
	Fit stringers and treads, working from a stable platform
	Falling from a ladder
Injury from power tools
	Workers, People nearby
	High (12)
	- Use a podium step, mobile tower or MEWP for longer jobs instead of a straight ladder. [Reduce / substitute]
- Use EN 131 professional ladders in good condition. Remove any damaged ladder from site. [Control (engineering)]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Control (engineering)]
- Use ladders only for short, light work (about 30 minutes in one spot). Do not carry heavy or awkward loads up a ladder. [Control (procedures)]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Control (procedures)]
- Do not work off the top three rungs of a leaning ladder. On a stepladder, do not stand on the top two steps (top three on swing-back or double-sided steps) unless there is a suitable handhold. [Control (procedures)]
- Check the ladder before each use: feet, rungs, stiles and locks. [Control (procedures)]
- Wear non-slip safety boots with clean soles. [PPE]
- Keep all guards fitted and working. Never tie back or remove a guard. [Control (engineering)]
- Clamp or secure the work piece. Do not hold it by hand. [Control (engineering)]
- Only trained, competent people use power tools, following the maker's instructions. [Control (procedures)]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Control (procedures)]
- No loose clothing, jewellery or long hair near spinning parts. [Control (procedures)]
- Wear safety glasses and hearing protection. Do not wear loose gloves on drills or other rotating tools. [PPE]
	Medium (8)
	

	4
	Install handrails and balustrade as soon as possible
	Falling from height
Nail gun injuries
	Workers, People below, People nearby
	Very high (20)
	- Falling from height: see step 1 for the full controls [Control (procedures)]
- Use a nail gun with a sequential (single shot) trigger, not a contact or bump trigger. [Reduce / substitute]
- Disconnect the air or battery before clearing jams, adjusting or moving between work areas. [Control (engineering)]
- Keep your free hand at least 30 cm from the nailing point. [Control (procedures)]
- Never point the gun at anyone or carry it with your finger on the trigger. [Control (procedures)]
- Train new users before they use a nail gun, and check for pipes, cables and metal behind the surface. [Control (procedures)]
- Wear safety glasses and hearing protection. [PPE]
	Medium (8)
	

	5
	Remove the void guard only once the balustrade is fixed, then clean up
	Poor housekeeping and waste
	Workers, Visitors
	Medium (8)
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Guard the stair void before and during installation
2. Move stair parts in with enough people
3. Fit stringers and treads, working from a stable platform
4. Install handrails and balustrade as soon as possible
5. Remove the void guard only once the balustrade is fixed, then clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety glasses
Ear defenders
Rigger gloves
Safety helmet
	Circular saw
Power drill
Nail gun
Hand tools
Podium step
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/carpentry/stair-installation/
