RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Concrete cutting and core drilling · Concreting · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Get the engineer's approval for every cut, then scan the slab and mark cables, conduits, reo and post-tension tendons. Never cut or core through a tendon
	Electric shock from live wiring
Stored energy
Hitting underground services
	Workers, Occupants, Public
	Very high (15)
	- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- Release or block all stored energy before work: release the pressure in pipes, tanks and hoses, bleed hydraulics, release springs, lower loads. [Eliminate]
- Lock out and tag all energy sources with personal locks. [Isolate]
- Put mechanical blocks or props under raised parts like buckets, tipper bodies and doors. [Control (engineering)]
- Test that the system is dead and nothing can move before you start. [Control (procedures)]
- Follow the maker's procedure, for example for garage door and roller door springs. [Control (procedures)]
- Keep machine buckets well clear of marked services and use a spotter. [Isolate]
- Do a CAT and Genny scan before digging and mark services on the ground. [Control (engineering)]
- Hand dig trial holes to find services before machine digging (safe digging practice). [Control (engineering)]
- Get utility plans before digging and check them against what you see on site. [Control (procedures)]
- Keep plans or locate tickets on site and check them again if the work area grows. [Control (procedures)]
	Medium (5)
	

	2
	Set an exclusion zone, including the floor below for coring, and keep occupants out
	Falling tools and materials
Public entering the work area
Working in an occupied home or building
	Workers, Public, People below, Children, Residents, Staff
	High (12)
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Control (engineering)]
- Use catch fans, debris netting or covered walkways where people pass below. [Control (engineering)]
- Tether hand tools when working at height. [Control (engineering)]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Control (procedures)]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Control (engineering)]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Control (procedures)]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Control (procedures)]
- Plan noisy, dusty or risky work for when the building is empty. [Eliminate]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Isolate]
- Keep fire exits and paths clear at all times. [Control (procedures)]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Control (procedures)]
- Lock away tools, chemicals and materials each day, out of reach of children. [Control (procedures)]
	Medium (8)
	

	3
	Plan where the water and slurry will go and keep leads off wet ground, using RCD protection
	Electric shock from leads and power tools
Slips and trips
	Workers, Visitors, Public
	High (12)
	- Use battery-powered tools where you can. [Reduce / substitute]
- Use 110V tools through a centre-tapped transformer, or battery tools. Use an RCD on any 230V supply. [Control (engineering)]
- Keep leads off the ground and out of water, using lead stands or hooks. [Control (engineering)]
- Check leads, plugs and tools before every use. Tag out and remove anything damaged. [Control (procedures)]
- Keep tools and leads inspected and PAT tested on a regular schedule. [Control (procedures)]
- Do not use tools in rain or wet areas unless they are rated for it. [Control (procedures)]
- Wear safety boots and dry gloves. [PPE]
- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Control (engineering)]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Control (engineering)]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Control (procedures)]
- Keep work areas, stairs and access paths well lit. [Control (procedures)]
- Wear safety boots with good grip, laced up. [PPE]
	Low (4)
	

	4
	Check the blade or bit, guard and water feed before starting
	Saw cuts and kickback
Injury from power tools
	Workers, People nearby
	High (12)
	- Keep blade guards fitted and working, and use the riving knife on table saws. [Control (engineering)]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Control (engineering)]
- Use a sharp, undamaged blade made for the material. [Control (procedures)]
- Stand to one side of the blade line, out of the kickback path. [Control (procedures)]
- Let the blade stop fully before reaching in or putting the saw down. [Control (procedures)]
- Wear safety glasses, hearing protection and close-fitting clothes. [PPE]
- Keep all guards fitted and working. Never tie back or remove a guard. [Control (engineering)]
- Clamp or secure the work piece. Do not hold it by hand. [Control (engineering)]
- Only trained, competent people use power tools, following the maker's instructions. [Control (procedures)]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Control (procedures)]
- No loose clothing, jewellery or long hair near spinning parts. [Control (procedures)]
- Wear safety glasses and hearing protection. Do not wear loose gloves on drills or other rotating tools. [PPE]
	Medium (8)
	

	5
	Fix the core drill rig with an anchor or vacuum base so it cannot spin
	Injury from power tools
Lifting and carrying heavy loads
	Workers, People nearby
	High (12)
	- Injury from power tools: see step 4 for the full controls [Control (procedures)]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium (6)
	

	6
	Cut with water suppression or extraction, never dry cut. Indoors, use electric or hydraulic saws; never run petrol saws or generators inside (carbon monoxide)
	Silica dust from concrete, brick, stone and tiles
Saw cuts and kickback
Loud noise
Hand-arm and whole-body vibration
	Workers, People nearby
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Saw cuts and kickback: see step 4 for the full controls [Control (procedures)]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Reduce / substitute]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Control (engineering)]
- Limit trigger time using the HSE vibration calculator to stay below the exposure action value, and rotate workers. [Control (procedures)]
- Keep hands warm and dry, and take regular breaks. [Control (procedures)]
	Medium (8)
	

	7
	Support cut pieces and cores so they do not drop or pinch the blade
	Lifting and carrying heavy loads
Falling tools and materials
Structural collapse during alterations
	Workers, Public, People below, Occupants
	High (12)
	- Lifting and carrying heavy loads: see step 5 for the full controls [Control (procedures)]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Control (procedures)]
- Wear a hard hat anywhere objects could fall. [PPE]
- Falling tools and materials: see step 2 for the full controls [Control (procedures)]
- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Eliminate]
- Keep everyone clear of the area under and next to the work. [Isolate]
- Install temporary props, needles or shoring as designed before removing any support. [Control (engineering)]
- Follow the engineer's sequence. Do not change it without approval. [Control (procedures)]
- Check props daily. Do not remove them until the permanent support is in and approved. [Control (procedures)]
	Medium (8)
	

	8
	Cover or guard new holes, vacuum slurry and clean up
	Falling through a floor opening or void
Poor housekeeping and waste
Slips and trips
	Workers, Visitors, Public
	Very high (15)
	- Cover every hole and penetration with a fixed, secured cover marked "HOLE" or "DANGER". [Isolate]
- Put guardrails with toe boards around stairwells, lift shafts, voids and open edges. [Isolate]
- Install stairs early and fit temporary handrails as soon as they go in. [Control (engineering)]
- Never remove a cover or guardrail without approval. Put it back straight away. [Control (procedures)]
- Inspect covers and barriers daily and after other trades have been through. [Control (procedures)]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Slips and trips: see step 3 for the full controls [Control (procedures)]
	Medium (5)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Get the engineer's approval for every cut, then scan the slab and mark cables, conduits, reo and post-tension tendons. Never cut or core through a tendon
2. Set an exclusion zone, including the floor below for coring, and keep occupants out
3. Plan where the water and slurry will go and keep leads off wet ground, using RCD protection
4. Check the blade or bit, guard and water feed before starting
5. Fix the core drill rig with an anchor or vacuum base so it cannot spin
6. Cut with water suppression or extraction, never dry cut. Indoors, use electric or hydraulic saws; never run petrol saws or generators inside (carbon monoxide)
7. Support cut pieces and cores so they do not drop or pinch the blade
8. Cover or guard new holes, vacuum slurry and clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety glasses
Ear defenders
FFP3 dust mask
Rigger gloves
Safety helmet
Hi-vis vest
Half-mask respirator (P3 filters)
	Cut-off saw (Stihl saw)
Diamond core drill
Generator (110V site transformer)
H-class dust extractor
	Permit to work (electrical isolation)


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/concreting/concrete-cutting-coring/
