RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Concrete breaking and removal · Demolition · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Locate services under the slab before breaking
	Hitting underground services
Electric shock from live wiring
	Workers, Public, Occupants
	Very high (15)
	- Keep machine buckets well clear of marked services and use a spotter. [Isolate]
- Do a CAT and Genny scan before digging and mark services on the ground. [Control (engineering)]
- Hand dig trial holes to find services before machine digging (safe digging practice). [Control (engineering)]
- Get utility plans before digging and check them against what you see on site. [Control (procedures)]
- Keep plans or locate tickets on site and check them again if the work area grows. [Control (procedures)]
- If you hit a service, stop, get everyone clear, and call the owner and emergency services. [Control (procedures)]
- Wear safety boots, gloves and hi-vis when digging. [PPE]
- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Control (procedures)]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium (5)
	

	2
	Saw cut edges with water suppression
	Silica dust from concrete, brick, stone and tiles
Saw cuts and kickback
Loud noise
	Workers, People nearby
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Control (engineering)]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Control (engineering)]
- Use a sharp, undamaged blade made for the material. [Control (procedures)]
- Stand to one side of the blade line, out of the kickback path. [Control (procedures)]
- Let the blade stop fully before reaching in or putting the saw down. [Control (procedures)]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Loud noise: see step 3 for the full controls [Control (procedures)]
	Medium (8)
	

	3
	Break with a jackhammer or excavator breaker, rotating jackhammer work
	Hand-arm and whole-body vibration
Loud noise
Being hit by mobile plant
	Workers, People nearby, Visitors, Public
	Very high (15)
	- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Reduce / substitute]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Control (engineering)]
- Limit trigger time using the HSE vibration calculator to stay below the exposure action value, and rotate workers. [Control (procedures)]
- Keep hands warm and dry, and take regular breaks. [Control (procedures)]
- Report tingling, numbness or white fingers early. [Control (procedures)]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- If you have to shout to be heard by someone 2 metres away, the noise is probably 85 dB(A) or more: wear hearing protection. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
- Separate people and plant with barriers, exclusion zones and marked walkways. [Isolate]
- Use plant with working reversing alarms, cameras and lights. [Control (engineering)]
- Have a traffic management plan showing plant routes, loading areas and pedestrian paths. [Control (procedures)]
- Use a spotter when reversing or working near people. [Control (procedures)]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Control (procedures)]
	Medium (6)
	

	4
	Watch for flying chips and keep others back
	Eye injuries
Demolition and falling debris
	Workers, People nearby, Public, Neighbours
	Very high (15)
	- Use tool guards and screens to stop flying particles. [Control (engineering)]
- Use dust extraction and water to keep dust out of the air. [Control (engineering)]
- Keep others out of the area when cutting, grinding or chipping. [Control (procedures)]
- Keep an eye wash station or eye wash bottles on site. [Control (procedures)]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
- Check for asbestos, lead, live services and structural risks before demolition starts. [Eliminate]
- Disconnect and cap power, gas and water before demolition. [Isolate]
- Set an exclusion zone bigger than the distance the structure could fall. [Isolate]
- Use a machine with a guarded cab instead of hand demolition where practical. [Control (engineering)]
- Use chutes or bins to get debris down. Never drop it from height. [Control (engineering)]
- Follow a written demolition plan, working from the top down. Do not remove supports out of sequence. [Control (procedures)]
- Record the demolition, dismantling or strip-out arrangements in writing before work starts (CDM 2015 reg 20(2)). [Control (procedures)]
- Wear a hard hat, safety glasses, dust mask, gloves and safety boots. [PPE]
	Medium (5)
	

	5
	Load rubble by machine where possible, then clean up
	Lifting and carrying heavy loads
Poor housekeeping and waste
	Workers, Visitors
	High (12)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Medium (6)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Locate services under the slab before breaking
2. Saw cut edges with water suppression
3. Break with a jackhammer or excavator breaker, rotating jackhammer work
4. Watch for flying chips and keep others back
5. Load rubble by machine where possible, then clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Ear defenders
Safety glasses
FFP3 dust mask
Rigger gloves
Hi-vis vest
Half-mask respirator (P3 filters)
Safety helmet
Safety goggles
Face shield
	Breaker
Excavator (360) (CPCS or NPORS excavator card)
Skid steer loader (CPCS or NPORS skid steer card)
Cut-off saw (Stihl saw)
Air compressor
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/demolition/concrete-breaking-removal/
