RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Internal strip-out · Demolition · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check the refurbishment and demolition asbestos survey and have any asbestos removed first, by an HSE licensed asbestos contractor where the work is licensable
	Disturbing asbestos
	Workers, Occupants, Public
	Very high (15)
	- Before work on any building built before 2000, check the refurbishment and demolition asbestos survey for the work area (HSE HSG264). If there is none, presume asbestos is present or have it sampled before you start. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Control (engineering)]
- Most asbestos insulation, coatings and insulating board need a licensed contractor. Notifiable non-licensed work is notified to HSE before it starts. Other work needs trained workers and controls. [Control (procedures)]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Control (procedures)]
- Wear a fit-tested FFP3 mask (or better) and disposable type 5 coveralls. [PPE]
	Medium (5)
	

	2
	Check for lead paint and other hazardous materials before work starts
	Lead paint dust and fumes
Hazardous chemicals
	Workers, Residents, Children, Occupants
	High (12)
	- Test old paint for lead before you sand, scrape, cut or heat it. [Eliminate]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Reduce / substitute]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Isolate]
- Clean up with an H-class vacuum and wet wipes. Never dry sweep. [Control (engineering)]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Control (procedures)]
- Wear an FFP3 mask, disposable coveralls and gloves. [PPE]
- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Reduce / substitute]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Control (engineering)]
- Do a COSHH assessment and read the Safety Data Sheet (SDS) before use. [Control (procedures)]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Control (procedures)]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Control (procedures)]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Control (procedures)]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
	Medium (6)
	

	3
	Isolate and cap power, gas and water to the area, and confirm they are dead
	Electric shock from live wiring
Gas and fuel lines
	Workers, Occupants, Public
	Very high (15)
	- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Control (procedures)]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
- Isolate and purge the line before work, with the owner's approval. [Eliminate]
- Lock off and tag the isolation valve. [Isolate]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Control (engineering)]
- Only Gas Safe registered engineers work on gas fittings. [Control (procedures)]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Control (procedures)]
- Know where the shut-off valve is and what to do if a leak happens. [Control (procedures)]
- Wear safety glasses and gloves, and keep a fire extinguisher close by. [PPE]
	Medium (5)
	

	4
	Seal the area from occupants, set up dust control and keep exits clear
	Working in an occupied home or building
General dust
Fire and emergencies
	Residents, Children, Staff, Workers, Occupants, Visitors
	High (10)
	- Plan noisy, dusty or risky work for when the building is empty. [Eliminate]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Isolate]
- Keep fire exits and paths clear at all times. [Control (procedures)]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Control (procedures)]
- Lock away tools, chemicals and materials each day, out of reach of children. [Control (procedures)]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
- Provide fire extinguishers suited to the site, checked and easy to reach. [Control (engineering)]
- Keep exits and escape routes clear and signed. [Control (engineering)]
- Have a site emergency plan: alarm, exits, assembly point and emergency contacts. [Control (procedures)]
- Keep a stocked first aid kit and at least one trained first aider on site. [Control (procedures)]
- Know the site address and how emergency services get in. Call 999. [Control (procedures)]
	Medium (5)
	

	5
	Confirm which walls are load bearing and leave them alone without an engineer design
	Structural collapse during alterations
	Workers, Occupants
	High (10)
	- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Eliminate]
- Keep everyone clear of the area under and next to the work. [Isolate]
- Install temporary props, needles or shoring as designed before removing any support. [Control (engineering)]
- Follow the engineer's sequence. Do not change it without approval. [Control (procedures)]
- Check props daily. Do not remove them until the permanent support is in and approved. [Control (procedures)]
- Wear a hard hat and safety boots. [PPE]
	Medium (5)
	

	6
	Strip fittings and linings from the top down, using a platform ladder or mobile scaffold for ceilings
	Falling tools and materials
Cuts from sharp edges
Falling from a ladder
	Workers, Public, People below
	High (12)
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Control (engineering)]
- Use catch fans, debris netting or covered walkways where people pass below. [Control (engineering)]
- Tether hand tools when working at height. [Control (engineering)]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Control (procedures)]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Control (engineering)]
- Use knives with retractable or self-retracting blades. [Control (engineering)]
- Cut away from your body and keep your other hand clear. [Control (procedures)]
- Put used blades in a blade bin or sharps container. [Control (procedures)]
- Use two people to handle large sheets of metal or glass. [Control (procedures)]
- Use a podium step, mobile tower or MEWP for longer jobs instead of a straight ladder. [Reduce / substitute]
- Use EN 131 professional ladders in good condition. Remove any damaged ladder from site. [Control (engineering)]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Control (engineering)]
- Use ladders only for short, light work (about 30 minutes in one spot). Do not carry heavy or awkward loads up a ladder. [Control (procedures)]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Control (procedures)]
	Medium (8)
	

	7
	Cut or break materials with dust extraction
	Angle grinder injuries
Loud noise
Hand-arm and whole-body vibration
Silica dust from concrete, brick, stone and tiles
	Workers, People nearby
	Very high (20)
	- Use a guarded saw or a different tool where you can. [Reduce / substitute]
- Keep the guard on and use the side handle. Never remove the guard. [Control (engineering)]
- Use the right disc for the job, rated for the grinder's speed. Check it for cracks first. [Control (procedures)]
- Only trained people change discs, with the grinder unplugged or the battery out. [Control (procedures)]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Reduce / substitute]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Control (engineering)]
- Limit trigger time using the HSE vibration calculator to stay below the exposure action value, and rotate workers. [Control (procedures)]
- Keep hands warm and dry, and take regular breaks. [Control (procedures)]
- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
	Medium (8)
	

	8
	Watch for needles, droppings and mould in wall and ceiling cavities
	Needles and sharps
Mould and droppings
	Workers, Occupants
	Medium (9)
	- Use tongs or a pick-up tool. Never pick up needles by hand. [Control (engineering)]
- Put needles in a hard sharps container with a lid. [Control (engineering)]
- Look before you reach. Use a torch to check ceilings, cavities and rubbish. [Control (procedures)]
- If you are stuck, wash the area with soap and water and see a doctor straight away. [Control (procedures)]
- Wear puncture-resistant gloves and safety boots. [PPE]
- Fix the water leak and dry the area before removing mould. [Eliminate]
- Seal off the area with plastic sheeting and keep occupants out. [Isolate]
- Clean up with an H-class vacuum and wet wipes. Never dry sweep. [Control (engineering)]
- Bag mouldy material on site and remove it promptly. [Control (procedures)]
- Wash hands and face before eating and at the end of each shift. [Control (procedures)]
- Wear an FFP3 mask, gloves, goggles and disposable coveralls. [PPE]
	Low (4)
	

	9
	Load waste into the skip by hand or chute, keeping walkways clear
	Lifting and carrying heavy loads
Poor housekeeping and waste
	Workers, Visitors
	High (12)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Medium (6)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Check the refurbishment and demolition asbestos survey and have any asbestos removed first, by an HSE licensed asbestos contractor where the work is licensable
2. Check for lead paint and other hazardous materials before work starts
3. Isolate and cap power, gas and water to the area, and confirm they are dead
4. Seal the area from occupants, set up dust control and keep exits clear
5. Confirm which walls are load bearing and leave them alone without an engineer design
6. Strip fittings and linings from the top down, using a platform ladder or mobile scaffold for ceilings
7. Cut or break materials with dust extraction
8. Watch for needles, droppings and mould in wall and ceiling cavities
9. Load waste into the skip by hand or chute, keeping walkways clear
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety helmet
Safety glasses
FFP3 dust mask
Cut-resistant gloves
Ear defenders
Half-mask respirator (P3 filters)
Coveralls
Rigger gloves
Chemical-resistant gloves
Safety goggles
Face shield
	Hand tools
Angle grinder (disc cutter)
Breaker
H-class dust extractor
Trailer
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/uk/rams/demolition/internal-strip-out/
