RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Install sockets · Electrical · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Locate the circuit at the consumer unit, isolate it, lock off and label and test to prove dead
	Electric shock from live wiring
	Workers, Occupants
	Very high (15)
	- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Control (procedures)]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium (5)
	

	2
	Scan the wall for pipes and cables before cutting the hole
	Electric shock from live wiring
Gas and fuel lines
	Workers, Occupants, Public
	Very high (15)
	- Electric shock from live wiring: see step 1 for the full controls [Control (procedures)]
- Isolate and purge the line before work, with the owner's approval. [Eliminate]
- Lock off and tag the isolation valve. [Isolate]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Control (engineering)]
- Only Gas Safe registered engineers work on gas fittings. [Control (procedures)]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Control (procedures)]
- Know where the shut-off valve is and what to do if a leak happens. [Control (procedures)]
- Wear safety glasses and gloves, and keep a fire extinguisher close by. [PPE]
	Medium (5)
	

	3
	Cut in the box and run the cable, keeping dust down
	General dust
Injury from power tools
Falling from a ladder
	Workers, Occupants, People nearby
	High (12)
	- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
- Keep all guards fitted and working. Never tie back or remove a guard. [Control (engineering)]
- Clamp or secure the work piece. Do not hold it by hand. [Control (engineering)]
- Only trained, competent people use power tools, following the maker's instructions. [Control (procedures)]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Control (procedures)]
- No loose clothing, jewellery or long hair near spinning parts. [Control (procedures)]
- Use a podium step, mobile tower or MEWP for longer jobs instead of a straight ladder. [Reduce / substitute]
- Use EN 131 professional ladders in good condition. Remove any damaged ladder from site. [Control (engineering)]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Control (engineering)]
- Use ladders only for short, light work (about 30 minutes in one spot). Do not carry heavy or awkward loads up a ladder. [Control (procedures)]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Control (procedures)]
	Medium (8)
	

	4
	Terminate the socket and check connections are tight
	Electric shock from leads and power tools
Repetitive work and awkward postures
	Workers
	High (12)
	- Use battery-powered tools where you can. [Reduce / substitute]
- Use 110V tools through a centre-tapped transformer, or battery tools. Use an RCD on any 230V supply. [Control (engineering)]
- Keep leads off the ground and out of water, using lead stands or hooks. [Control (engineering)]
- Check leads, plugs and tools before every use. Tag out and remove anything damaged. [Control (procedures)]
- Keep tools and leads inspected and PAT tested on a regular schedule. [Control (procedures)]
- Do not use tools in rain or wet areas unless they are rated for it. [Control (procedures)]
- Wear safety boots and dry gloves. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Reduce / substitute]
- Set work up at waist height on benches or trestles where you can. [Control (engineering)]
- Use light tools with good grips, and keep blades and bits sharp. [Control (engineering)]
- Rotate tasks and take short breaks every hour on repetitive work. [Control (procedures)]
- Warm up before heavy physical work and report aches and pains early. [Control (procedures)]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium (6)
	

	5
	Test polarity, earth and RCD protection, then restore power and clean up
	Electric shock from live wiring
Poor housekeeping and waste
	Workers, Occupants, Visitors
	Very high (15)
	- Electric shock from live wiring: see step 1 for the full controls [Control (procedures)]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Medium (5)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Locate the circuit at the consumer unit, isolate it, lock off and label and test to prove dead
2. Scan the wall for pipes and cables before cutting the hole
3. Cut in the box and run the cable, keeping dust down
4. Terminate the socket and check connections are tight
5. Test polarity, earth and RCD protection, then restore power and clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety glasses
Rigger gloves
Insulated electrical gloves
Arc-rated clothing and face shield
FFP3 dust mask
Ear defenders
Safety helmet
Knee pads
	Electrical test equipment (multifunction tester)
Power drill
Hand tools
	Permit to work (electrical isolation)


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/uk/rams/electrical/power-point-installation/
