RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Install smoke alarms · Electrical · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Plan alarm locations and let the occupants know
	Working in an occupied home or building
	Residents, Children, Staff, Workers
	Medium (9)
	- Plan noisy, dusty or risky work for when the building is empty. [Eliminate]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Isolate]
- Keep fire exits and paths clear at all times. [Control (procedures)]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Control (procedures)]
- Lock away tools, chemicals and materials each day, out of reach of children. [Control (procedures)]
- Clean up dust and debris at the end of each day. [Control (procedures)]
	Low (3)
	

	2
	Isolate the circuit for hard wired alarms, lock off and label and prove dead
	Electric shock from live wiring
	Workers, Occupants
	Very high (15)
	- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Control (procedures)]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium (5)
	

	3
	Set up a platform ladder and cut ceiling holes, wearing glasses and a dust mask
	Falling from a ladder
General dust
Eye injuries
	Workers, Occupants, People nearby
	High (12)
	- Use a podium step, mobile tower or MEWP for longer jobs instead of a straight ladder. [Reduce / substitute]
- Use EN 131 professional ladders in good condition. Remove any damaged ladder from site. [Control (engineering)]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Control (engineering)]
- Use ladders only for short, light work (about 30 minutes in one spot). Do not carry heavy or awkward loads up a ladder. [Control (procedures)]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Control (procedures)]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
- Use tool guards and screens to stop flying particles. [Control (engineering)]
- Use dust extraction and water to keep dust out of the air. [Control (engineering)]
- Keep others out of the area when cutting, grinding or chipping. [Control (procedures)]
- Keep an eye wash station or eye wash bottles on site. [Control (procedures)]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
	Medium (8)
	

	4
	Run cable in the ceiling space, staying on joists
	Falling through a floor opening or void
Heat stress
	Workers, Visitors
	Very high (15)
	- Cover every hole and penetration with a fixed, secured cover marked "HOLE" or "DANGER". [Isolate]
- Put guardrails with toe boards around stairwells, lift shafts, voids and open edges. [Isolate]
- Install stairs early and fit temporary handrails as soon as they go in. [Control (engineering)]
- Never remove a cover or guardrail without approval. Put it back straight away. [Control (procedures)]
- Inspect covers and barriers daily and after other trades have been through. [Control (procedures)]
- Keep lighting good enough to see openings, especially on lower floors and in the evening. [Control (procedures)]
- Use a harness clipped to a rated anchor when working right next to an open void. [PPE]
- Schedule heavy work for the cooler part of the day. [Eliminate]
- Provide shade over work and rest areas, and fans or cooling in roof spaces. [Control (engineering)]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Control (procedures)]
- Take regular rest breaks in the shade, more often as it gets hotter. [Control (procedures)]
- Let new and returning workers build up to full work in the heat over about a week. [Control (procedures)]
- Watch each other for dizziness, headache, confusion or stopping sweating. Stop work, cool down and get help. [Control (procedures)]
- Have a hot weather plan, including when work stops. [Control (procedures)]
- Wear light, loose, long-sleeved clothing, a hat or brim, and sunscreen. [PPE]
	Medium (8)
	

	5
	Connect and test every alarm, then clean up
	Electric shock from live wiring
Poor housekeeping and waste
	Workers, Occupants, Visitors
	Very high (15)
	- Electric shock from live wiring: see step 2 for the full controls [Control (procedures)]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Medium (5)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Plan alarm locations and let the occupants know
2. Isolate the circuit for hard wired alarms, lock off and label and prove dead
3. Set up a platform ladder and cut ceiling holes, wearing glasses and a dust mask
4. Run cable in the ceiling space, staying on joists
5. Connect and test every alarm, then clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety glasses
FFP3 dust mask
Insulated electrical gloves
Arc-rated clothing and face shield
Safety helmet
Safety goggles
Face shield
Sun protection (sunscreen and neck cover)
Rigger gloves
	Podium step
Power drill
Electrical test equipment (multifunction tester)
Hand tools
	Permit to work (electrical isolation)


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/electrical/smoke-alarm-installation/
