RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
New home construction · General building · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up the site: fencing, signs, toilets, power and induction
	Public entering the work area
Electric shock from leads and power tools
	Public, Children, Workers
	High (12)
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Control (engineering)]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Control (procedures)]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Control (procedures)]
- Use a spotter when moving plant or materials across public paths. [Control (procedures)]
- Use battery-powered tools where you can. [Reduce / substitute]
- Use 110V tools through a centre-tapped transformer, or battery tools. Use an RCD on any 230V supply. [Control (engineering)]
- Keep leads off the ground and out of water, using lead stands or hooks. [Control (engineering)]
- Check leads, plugs and tools before every use. Tag out and remove anything damaged. [Control (procedures)]
- Keep tools and leads inspected and PAT tested on a regular schedule. [Control (procedures)]
- Do not use tools in rain or wet areas unless they are rated for it. [Control (procedures)]
- Wear safety boots and dry gloves. [PPE]
	Low (4)
	

	2
	Site cut, footings and slab
	Being hit by mobile plant
Hitting underground services
Trench or excavation collapse
Wet concrete and cement burns
	Workers, Visitors, Public
	Very high (15)
	- Separate people and plant with barriers, exclusion zones and marked walkways. [Isolate]
- Use plant with working reversing alarms, cameras and lights. [Control (engineering)]
- Have a traffic management plan showing plant routes, loading areas and pedestrian paths. [Control (procedures)]
- Use a spotter when reversing or working near people. [Control (procedures)]
- Keep machine buckets well clear of marked services and use a spotter. [Isolate]
- Do a CAT and Genny scan before digging and mark services on the ground. [Control (engineering)]
- Hand dig trial holes to find services before machine digging (safe digging practice). [Control (engineering)]
- Get utility plans before digging and check them against what you see on site. [Control (procedures)]
- Use methods that keep people out of the trench, such as directional boring or working from the surface. [Eliminate]
- Barricade or cover the excavation so people and plant cannot fall in. [Isolate]
- Support or batter back the sides of any excavation where collapse could happen. Use trench boxes or sheet piling for deeper trenches. [Control (engineering)]
- Keep spoil, materials and plant at least 1 metre back from the edge. [Control (engineering)]
- Inspect the excavation at the start of each shift and after rain or anything that could weaken it. Record it. [Control (procedures)]
- Use long-handled tools and pumps to cut down contact. [Control (engineering)]
- Wash concrete off skin straight away with clean water. [Control (procedures)]
- Have clean water and eye wash where concrete or mortar is mixed and used. [Control (procedures)]
- Do a COSHH assessment for cement, lime and mortar, and check hands regularly for early signs of dermatitis. [Control (procedures)]
- Wear waterproof gloves, long sleeves and waterproof boots with trousers worn over the top. [PPE]
	Medium (5)
	

	3
	Frame and roof with scaffold and edge protection
	Falling from height
Falling from a roof edge
Crane and lifting failure
	Workers, People below, Public
	Very high (20)
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile tower or MEWP instead of working off a ladder. [Control (engineering)]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Control (engineering)]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Control (procedures)]
- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Eliminate]
- Install edge protection or guardrails on all open roof edges before work starts. [Isolate]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Control (engineering)]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Control (engineering)]
- Use one safe, controlled access point and keep others off the roof. [Control (procedures)]
- Barricade the lift zone and keep everyone out from under the load. [Isolate]
- Use a crane rated for the load at the radius, set up on firm ground with outrigger pads. [Control (engineering)]
- Check slings, chains, shackles and hooks before use. Remove anything damaged or not tagged. [Control (engineering)]
- Have a lift plan made by an appointed person, following LOLER. [Control (procedures)]
- Use CPCS or NPORS carded crane operators, slingers and signallers. [Control (procedures)]
	Medium (5)
	

	4
	Lock up: brick, windows and roof covering
	Lifting and carrying heavy loads
Silica dust from concrete, brick, stone and tiles
Glass handling and breakage
	Workers, People nearby, Occupants
	Very high (20)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Use suction lifters, glass trolleys or a glazing robot for large panes. [Control (engineering)]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Control (engineering)]
- Use two or more people for large panes, and clear the carry route first. [Control (procedures)]
- Mark new glass with tape or stickers so nobody walks into it. [Control (procedures)]
- Clean up broken glass straight away into a marked container. [Control (procedures)]
	Medium (8)
	

	5
	Fit out with all trades, managing who works where
	Slips and trips
Electric shock from live wiring
General dust
	Workers, Visitors, Public, Occupants
	Very high (15)
	- Plan walkways and keep them clear of materials, hoses and leads. [Eliminate]
- Run leads and hoses overhead on hooks or stands, or along walls, not across walkways. [Control (engineering)]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Control (engineering)]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Control (procedures)]
- Keep work areas, stairs and access paths well lit. [Control (procedures)]
- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
	Medium (5)
	

	6
	Final clean, remove the site fence and hand over
	Poor housekeeping and waste
	Workers, Visitors
	Medium (8)
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Set up the site: fencing, signs, toilets, power and induction
2. Site cut, footings and slab
3. Frame and roof with scaffold and edge protection
4. Lock up: brick, windows and roof covering
5. Fit out with all trades, managing who works where
6. Final clean, remove the site fence and hand over
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Hi-vis vest
Safety helmet
Safety glasses
Ear defenders
Rigger gloves
Full body harness and lanyard
Sun protection (sunscreen and neck cover)
Chemical-resistant gloves
Safety goggles
Knee pads
Half-mask respirator (P3 filters)
Cut-resistant gloves
FFP3 dust mask
	Excavator (360) (CPCS or NPORS excavator card)
Concrete pump
Mobile crane (CPCS or NPORS crane operator card, plus slinger signaller card; lift plan by an Appointed Person)
Tube and fitting or system scaffold (CISRS scaffolder card to erect, alter or dismantle)
Nail gun
Circular saw
Telehandler (CPCS or NPORS telehandler card)
	Roof access permit
Work at height permit
Lift plan (LOLER reg 8)


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/general-building/new-home-construction/
