RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Glass balustrade installation · Glazing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Install temporary edge protection until the balustrade is complete
	Falling from height
Falling through a floor opening or void
	Workers, People below, Visitors
	Very high (20)
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile tower or MEWP instead of working off a ladder. [Control (engineering)]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Control (engineering)]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Control (procedures)]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
- Cover every hole and penetration with a fixed, secured cover marked "HOLE" or "DANGER". [Isolate]
- Put guardrails with toe boards around stairwells, lift shafts, voids and open edges. [Isolate]
- Install stairs early and fit temporary handrails as soon as they go in. [Control (engineering)]
- Never remove a cover or guardrail without approval. Put it back straight away. [Control (procedures)]
- Inspect covers and barriers daily and after other trades have been through. [Control (procedures)]
- Keep lighting good enough to see openings, especially on lower floors and in the evening. [Control (procedures)]
- Use a harness clipped to a rated anchor when working right next to an open void. [PPE]
	Medium (5)
	

	2
	Drill fixings with dust extraction
	Silica dust from concrete, brick, stone and tiles
Loud noise
Hand-arm and whole-body vibration
	Workers, People nearby
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- If you have to shout to be heard by someone 2 metres away, the noise is probably 85 dB(A) or more: wear hearing protection. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Reduce / substitute]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Control (engineering)]
- Limit trigger time using the HSE vibration calculator to stay below the exposure action value, and rotate workers. [Control (procedures)]
- Keep hands warm and dry, and take regular breaks. [Control (procedures)]
- Report tingling, numbness or white fingers early. [Control (procedures)]
	Medium (6)
	

	3
	Lift panels with suction lifters and enough people
	Lifting and carrying heavy loads
Glass handling and breakage
	Workers, Occupants
	High (12)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Use suction lifters, glass trolleys or a glazing robot for large panes. [Control (engineering)]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Control (engineering)]
- Use two or more people for large panes, and clear the carry route first. [Control (procedures)]
- Mark new glass with tape or stickers so nobody walks into it. [Control (procedures)]
- Clean up broken glass straight away into a marked container. [Control (procedures)]
- Wear cut-resistant gloves, arm guards, safety glasses and safety boots. [PPE]
	Medium (8)
	

	4
	Fix and check each panel before removing temporary protection
	Falling from height
Structural collapse during alterations
	Workers, People below, Occupants
	Very high (20)
	- Falling from height: see step 1 for the full controls [Control (procedures)]
- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Eliminate]
- Keep everyone clear of the area under and next to the work. [Isolate]
- Install temporary props, needles or shoring as designed before removing any support. [Control (engineering)]
- Follow the engineer's sequence. Do not change it without approval. [Control (procedures)]
- Check props daily. Do not remove them until the permanent support is in and approved. [Control (procedures)]
- Wear a hard hat and safety boots. [PPE]
	Medium (5)
	

	5
	Clean up
	Poor housekeeping and waste
	Workers, Visitors
	Medium (8)
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Install temporary edge protection until the balustrade is complete
2. Drill fixings with dust extraction
3. Lift panels with suction lifters and enough people
4. Fix and check each panel before removing temporary protection
5. Clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Cut-resistant gloves
Safety glasses
Full body harness and lanyard
Ear defenders
Half-mask respirator (P3 filters)
Rigger gloves
	Power drill
SDS drill
Hand tools
Scissor lift (MEWP) (IPAF PAL card (3a))
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/glazing/glass-balustrade/
