RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Paving installation · Landscaping · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Get utility plans and excavate the base
	Hitting underground services
Being hit by mobile plant
	Workers, Public, Visitors
	Very high (15)
	- Keep machine buckets well clear of marked services and use a spotter. [Isolate]
- Do a CAT and Genny scan before digging and mark services on the ground. [Control (engineering)]
- Hand dig trial holes to find services before machine digging (safe digging practice). [Control (engineering)]
- Get utility plans before digging and check them against what you see on site. [Control (procedures)]
- Keep plans or locate tickets on site and check them again if the work area grows. [Control (procedures)]
- If you hit a service, stop, get everyone clear, and call the owner and emergency services. [Control (procedures)]
- Wear safety boots, gloves and hi-vis when digging. [PPE]
- Separate people and plant with barriers, exclusion zones and marked walkways. [Isolate]
- Use plant with working reversing alarms, cameras and lights. [Control (engineering)]
- Have a traffic management plan showing plant routes, loading areas and pedestrian paths. [Control (procedures)]
- Use a spotter when reversing or working near people. [Control (procedures)]
- Make eye contact with the operator before going near. Stay out of the swing radius. [Control (procedures)]
- Operators hold a CPCS, NPORS or equal card for the plant they use. [Control (procedures)]
- Do a pre-start check on each machine every day and record it. [Control (procedures)]
- Wear hi-vis clothing and a hard hat. [PPE]
	Medium (5)
	

	2
	Compact road base, rotating operators
	Hand-arm and whole-body vibration
Loud noise
	Workers, People nearby
	High (12)
	- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Reduce / substitute]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Control (engineering)]
- Limit trigger time using the HSE vibration calculator to stay below the exposure action value, and rotate workers. [Control (procedures)]
- Keep hands warm and dry, and take regular breaks. [Control (procedures)]
- Report tingling, numbness or white fingers early. [Control (procedures)]
- Wear gloves to keep hands warm and dry. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- If you have to shout to be heard by someone 2 metres away, the noise is probably 85 dB(A) or more: wear hearing protection. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
- Wear earplugs or earmuffs rated for the noise. [PPE]
	Medium (6)
	

	3
	Lay paving slabs, using a lifter or two people for big ones
	Lifting and carrying heavy loads
Repetitive work and awkward postures
	Workers
	High (12)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Reduce / substitute]
- Set work up at waist height on benches or trestles where you can. [Control (engineering)]
- Use light tools with good grips, and keep blades and bits sharp. [Control (engineering)]
- Rotate tasks and take short breaks every hour on repetitive work. [Control (procedures)]
- Warm up before heavy physical work and report aches and pains early. [Control (procedures)]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium (6)
	

	4
	Cut paving slabs wet, never dry
	Silica dust from concrete, brick, stone and tiles
Saw cuts and kickback
Loud noise
	Workers, People nearby
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Control (engineering)]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Control (engineering)]
- Use a sharp, undamaged blade made for the material. [Control (procedures)]
- Stand to one side of the blade line, out of the kickback path. [Control (procedures)]
- Let the blade stop fully before reaching in or putting the saw down. [Control (procedures)]
- Loud noise: see step 2 for the full controls [Control (procedures)]
	Medium (8)
	

	5
	Sand, compact and clean up
	Sun exposure (UV)
Heat stress
Poor housekeeping and waste
	Workers, Visitors
	High (12)
	- Plan outdoor work for early morning or late afternoon when UV is lower. [Eliminate]
- Put shade covers over fixed work areas. [Control (engineering)]
- Check the UV index each day. Use sun protection when it is 3 or higher. [Control (procedures)]
- Check your skin regularly and see a doctor about any new or changing spots. [Control (procedures)]
- Wear a broad-brim hat or hard hat brim, long sleeves, sunglasses and SPF 30 or higher sunscreen, reapplied every 2 hours. [PPE]
- Schedule heavy work for the cooler part of the day. [Eliminate]
- Provide shade over work and rest areas, and fans or cooling in roof spaces. [Control (engineering)]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Control (procedures)]
- Take regular rest breaks in the shade, more often as it gets hotter. [Control (procedures)]
- Let new and returning workers build up to full work in the heat over about a week. [Control (procedures)]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
	Medium (8)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Get utility plans and excavate the base
2. Compact road base, rotating operators
3. Lay paving slabs, using a lifter or two people for big ones
4. Cut paving slabs wet, never dry
5. Sand, compact and clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Knee pads
Safety glasses
FFP3 dust mask
Ear defenders
Sun protection (sunscreen and neck cover)
Hi-vis vest
Safety helmet
Rigger gloves
Half-mask respirator (P3 filters)
	Skid steer loader (CPCS or NPORS skid steer card)
Wacker plate
Cut-off saw (Stihl saw)
Wet tile cutter
Hand tools
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/landscaping/paving-installation/
