RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
External rendering · Plastering and dry lining · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Use scaffold with guardrails, not ladders
	Falling from height
Scaffold collapse or fall from scaffold
	Workers, People below, Public
	Very high (20)
	- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile tower or MEWP instead of working off a ladder. [Control (engineering)]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Control (engineering)]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Control (procedures)]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
- Scaffold is built, altered and taken down only by CISRS-carded scaffolders, to TG20 or a specific design. [Control (engineering)]
- Fit guardrails, mid rails and toe boards on every working platform. [Control (engineering)]
- Use mobile scaffolds only on firm, level ground with castors locked and outriggers fitted. Never move one with anyone on it. [Control (engineering)]
- Mobile towers are built by PASMA-trained workers. [Control (procedures)]
- Inspect the scaffold before first use, after any change or bad weather, and at least every 7 days. Record it on the tag and register. [Control (procedures)]
- Do not overload platforms. Know the duty rating and keep material stacks over the standards. [Control (procedures)]
- Never remove ties, braces, guardrails or boards. Only the scaffolder alters the scaffold. [Control (procedures)]
- Wear a hard hat and safety boots on and around the scaffold. [PPE]
	Medium (5)
	

	2
	Mix render with gloves and goggles
	Wet concrete and cement burns
General dust
Eye injuries
	Workers, Occupants, People nearby
	Medium (9)
	- Use long-handled tools and pumps to cut down contact. [Control (engineering)]
- Wash concrete off skin straight away with clean water. [Control (procedures)]
- Have clean water and eye wash where concrete or mortar is mixed and used. [Control (procedures)]
- Do a COSHH assessment for cement, lime and mortar, and check hands regularly for early signs of dermatitis. [Control (procedures)]
- Wear waterproof gloves, long sleeves and waterproof boots with trousers worn over the top. [PPE]
- Wear safety glasses or goggles to stop splashes. [PPE]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
- Use tool guards and screens to stop flying particles. [Control (engineering)]
- Use dust extraction and water to keep dust out of the air. [Control (engineering)]
- Keep others out of the area when cutting, grinding or chipping. [Control (procedures)]
- Keep an eye wash station or eye wash bottles on site. [Control (procedures)]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
	Low (4)
	

	3
	Apply render, avoiding skin contact
	Wet concrete and cement burns
Repetitive work and awkward postures
	Workers
	Medium (9)
	- Wet concrete and cement burns: see step 2 for the full controls [Control (procedures)]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Reduce / substitute]
- Set work up at waist height on benches or trestles where you can. [Control (engineering)]
- Use light tools with good grips, and keep blades and bits sharp. [Control (engineering)]
- Rotate tasks and take short breaks every hour on repetitive work. [Control (procedures)]
- Warm up before heavy physical work and report aches and pains early. [Control (procedures)]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium (6)
	

	4
	Watch for heat and sun
	Heat stress
Sun exposure (UV)
	Workers
	High (12)
	- Schedule heavy work for the cooler part of the day. [Eliminate]
- Provide shade over work and rest areas, and fans or cooling in roof spaces. [Control (engineering)]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Control (procedures)]
- Take regular rest breaks in the shade, more often as it gets hotter. [Control (procedures)]
- Let new and returning workers build up to full work in the heat over about a week. [Control (procedures)]
- Watch each other for dizziness, headache, confusion or stopping sweating. Stop work, cool down and get help. [Control (procedures)]
- Have a hot weather plan, including when work stops. [Control (procedures)]
- Wear light, loose, long-sleeved clothing, a hat or brim, and sunscreen. [PPE]
- Plan outdoor work for early morning or late afternoon when UV is lower. [Eliminate]
- Put shade covers over fixed work areas. [Control (engineering)]
- Check the UV index each day. Use sun protection when it is 3 or higher. [Control (procedures)]
- Check your skin regularly and see a doctor about any new or changing spots. [Control (procedures)]
- Wear a broad-brim hat or hard hat brim, long sleeves, sunglasses and SPF 30 or higher sunscreen, reapplied every 2 hours. [PPE]
	Medium (8)
	

	5
	Clean the scaffold and area
	Poor housekeeping and waste
Falling tools and materials
	Workers, Visitors, Public, People below
	High (12)
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Control (engineering)]
- Use catch fans, debris netting or covered walkways where people pass below. [Control (engineering)]
- Tether hand tools when working at height. [Control (engineering)]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Control (procedures)]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Control (procedures)]
- Wear a hard hat anywhere objects could fall. [PPE]
	Medium (8)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Use scaffold with guardrails, not ladders
2. Mix render with gloves and goggles
3. Apply render, avoiding skin contact
4. Watch for heat and sun
5. Clean the scaffold and area
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Chemical-resistant gloves
Safety goggles
FFP3 dust mask
Sun protection (sunscreen and neck cover)
Safety helmet
Hi-vis vest
Knee pads
Safety glasses
Face shield
Rigger gloves
	Tube and fitting or system scaffold (CISRS scaffolder card to erect, alter or dismantle)
Cement mixer
Airless paint sprayer
Hand tools
	Work at height permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/uk/rams/plastering/external-rendering/
