RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Suspended ceiling installation · Plastering and dry lining · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Plan MEWP use and close the area below
	MEWP tip-over or crush
Falling tools and materials
	Workers, People nearby, Public, People below
	Very high (15)
	- Check the ground before setting up. Use outriggers and spreader pads, and keep clear of trenches, pits and slopes. [Control (engineering)]
- Use a platform with tilt alarm and secondary guarding (anti-entrapment) where there is an overhead crush risk. [Control (engineering)]
- Use IPAF-trained operators for MEWPs, carrying their PAL card. [Control (procedures)]
- Do a pre-start check each day. Keep a trained person on the ground who can lower the platform in an emergency. [Control (procedures)]
- Never exceed the safe working load, climb on the rails or use a ladder in the basket. [Control (procedures)]
- In boom-type platforms, wear a harness clipped to the basket anchor point. [PPE]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Control (engineering)]
- Use catch fans, debris netting or covered walkways where people pass below. [Control (engineering)]
- Tether hand tools when working at height. [Control (engineering)]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Control (procedures)]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Control (procedures)]
- Wear a hard hat anywhere objects could fall. [PPE]
	Medium (8)
	

	2
	Drill fixings into the slab with dust extraction
	Silica dust from concrete, brick, stone and tiles
Loud noise
Injury from power tools
	Workers, People nearby
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- If you have to shout to be heard by someone 2 metres away, the noise is probably 85 dB(A) or more: wear hearing protection. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
- Keep all guards fitted and working. Never tie back or remove a guard. [Control (engineering)]
- Clamp or secure the work piece. Do not hold it by hand. [Control (engineering)]
- Only trained, competent people use power tools, following the maker's instructions. [Control (procedures)]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Control (procedures)]
- No loose clothing, jewellery or long hair near spinning parts. [Control (procedures)]
	Medium (6)
	

	3
	Hang grid and wires, watching sharp grid ends
	Cuts from sharp edges
Repetitive work and awkward postures
	Workers
	Medium (9)
	- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Control (engineering)]
- Use knives with retractable or self-retracting blades. [Control (engineering)]
- Cut away from your body and keep your other hand clear. [Control (procedures)]
- Put used blades in a blade bin or sharps container. [Control (procedures)]
- Use two people to handle large sheets of metal or glass. [Control (procedures)]
- Wear cut-resistant gloves and long sleeves. [PPE]
- Use tools that cut the effort: powered screwdrivers, long-handled tools and extension poles for overhead work. [Reduce / substitute]
- Set work up at waist height on benches or trestles where you can. [Control (engineering)]
- Use light tools with good grips, and keep blades and bits sharp. [Control (engineering)]
- Rotate tasks and take short breaks every hour on repetitive work. [Control (procedures)]
- Warm up before heavy physical work and report aches and pains early. [Control (procedures)]
- Wear knee pads for kneeling work and gloves for grip. [PPE]
	Medium (6)
	

	4
	Drop in tiles and clean up
	General dust
Poor housekeeping and waste
	Workers, Occupants, Visitors
	Medium (8)
	- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Reduce / substitute]
- Seal off the work area with plastic sheeting in occupied buildings. [Isolate]
- Use tools with dust extraction and a vacuum for clean up. [Control (engineering)]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Control (engineering)]
- Never dry sweep or blow dust off with compressed air. [Control (procedures)]
- Wear a dust mask and safety glasses. [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Plan MEWP use and close the area below
2. Drill fixings into the slab with dust extraction
3. Hang grid and wires, watching sharp grid ends
4. Drop in tiles and clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety glasses
Safety helmet
FFP3 dust mask
Cut-resistant gloves
Full body harness and lanyard
Hi-vis vest
Half-mask respirator (P3 filters)
Ear defenders
Rigger gloves
Knee pads
	Scissor lift (MEWP) (IPAF PAL card (3a))
Podium step
Power drill
SDS drill
Hand tools
	Work at height permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/uk/rams/plastering/suspended-ceiling-installation/
