RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Gas fitting and appliance connection · Plumbing · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Only a Gas Safe registered engineer does this work. Tell occupants and remove ignition sources
	Gas and fuel lines
Working in an occupied home or building
	Workers, Occupants, Public, Residents, Children, Staff
	High (10)
	- Isolate and purge the line before work, with the owner's approval. [Eliminate]
- Lock off and tag the isolation valve. [Isolate]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Control (engineering)]
- Only Gas Safe registered engineers work on gas fittings. [Control (procedures)]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Control (procedures)]
- Know where the shut-off valve is and what to do if a leak happens. [Control (procedures)]
- Wear safety glasses and gloves, and keep a fire extinguisher close by. [PPE]
- Plan noisy, dusty or risky work for when the building is empty. [Eliminate]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Isolate]
- Keep fire exits and paths clear at all times. [Control (procedures)]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Control (procedures)]
- Lock away tools, chemicals and materials each day, out of reach of children. [Control (procedures)]
- Clean up dust and debris at the end of each day. [Control (procedures)]
	Medium (5)
	

	2
	Isolate gas at the meter, lock off and label, and purge the line
	Gas and fuel lines
Stored energy
Fire and emergencies
	Workers, Occupants, Public, Visitors
	High (10)
	- Gas and fuel lines: see step 1 for the full controls [Control (procedures)]
- Release or block all stored energy before work: release the pressure in pipes, tanks and hoses, bleed hydraulics, release springs, lower loads. [Eliminate]
- Lock out and tag all energy sources with personal locks. [Isolate]
- Put mechanical blocks or props under raised parts like buckets, tipper bodies and doors. [Control (engineering)]
- Test that the system is dead and nothing can move before you start. [Control (procedures)]
- Follow the maker's procedure, for example for garage door and roller door springs. [Control (procedures)]
- Provide fire extinguishers suited to the site, checked and easy to reach. [Control (engineering)]
- Keep exits and escape routes clear and signed. [Control (engineering)]
- Have a site emergency plan: alarm, exits, assembly point and emergency contacts. [Control (procedures)]
- Keep a stocked first aid kit and at least one trained first aider on site. [Control (procedures)]
- Know the site address and how emergency services get in. Call 999. [Control (procedures)]
	Medium (5)
	

	3
	Run and join new pipe, checking there are no electrical cables in the way
	Electric shock from live wiring
Injury from power tools
Tight spaces: roof spaces and under floors
	Workers, Occupants, People nearby
	Very high (15)
	- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- Keep all guards fitted and working. Never tie back or remove a guard. [Control (engineering)]
- Clamp or secure the work piece. Do not hold it by hand. [Control (engineering)]
- Only trained, competent people use power tools, following the maker's instructions. [Control (procedures)]
- Check tools before use. Unplug or remove the battery before changing blades or bits. [Control (procedures)]
- No loose clothing, jewellery or long hair near spinning parts. [Control (procedures)]
- Do as much of the work as you can from outside the tight space. [Eliminate]
- Turn the power off at the consumer unit or distribution board before entering where you can, as damaged cables may be live. [Isolate]
- Lay crawl boards across the joists so you cannot step through the ceiling. [Control (engineering)]
- Set up ventilation and lighting in the space. [Control (engineering)]
- Limit time in hot roof spaces and take breaks somewhere cool. [Control (procedures)]
	Medium (6)
	

	4
	Connect the appliance and seal all joints
	Gas and fuel lines
Lifting and carrying heavy loads
	Workers, Occupants, Public
	High (12)
	- Gas and fuel lines: see step 1 for the full controls [Control (procedures)]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium (6)
	

	5
	Pressure and leak test, then light and commission the appliance
	Pressure testing
Gas and fuel lines
Fire from hot works
	Workers, Occupants, Public
	Very high (15)
	- Test with water instead of air or gas where the system allows it. Never put water in refrigerant pipework, which is tested with dry nitrogen. [Reduce / substitute]
- Keep people out of the test area with signs and barriers. [Isolate]
- Use a calibrated gauge and a relief valve set to protect the system. [Control (engineering)]
- Test to the pressure the system calls for and hold it for the set time. Never go over. [Control (procedures)]
- Release the pressure fully before tightening anything or fixing leaks. [Control (procedures)]
- Gas and fuel lines: see step 1 for the full controls [Control (procedures)]
- Use cold work methods where you can, such as bolting, press fittings or cutting with a saw instead of a torch. [Eliminate]
- Move anything that can burn at least 10 metres away, or cover it with fire blankets. [Isolate]
- Use fire-resistant screens to stop sparks reaching people or gaps in walls and floors. [Control (engineering)]
- Get a hot work permit before starting. [Control (procedures)]
- Keep a charged fire extinguisher and fire blanket at the work spot. [Control (procedures)]
	Medium (5)
	

	6
	Issue the compliance certificate and clean up
	Poor housekeeping and waste
	Workers, Visitors
	Medium (8)
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Only a Gas Safe registered engineer does this work. Tell occupants and remove ignition sources
2. Isolate gas at the meter, lock off and label, and purge the line
3. Run and join new pipe, checking there are no electrical cables in the way
4. Connect the appliance and seal all joints
5. Pressure and leak test, then light and commission the appliance
6. Issue the compliance certificate and clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety glasses
Rigger gloves
FFP3 dust mask
Ear defenders
Knee pads
Safety helmet
Face shield
Welding gauntlets
Coveralls
	Hand tools
Press fitting tool
Electrical test equipment (multifunction tester)
Power drill
	Permit to work (electrical isolation)
Hot works permit (fire watch at least 60 minutes after)


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/uk/rams/plumbing/gas-fitting/
