RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Replace fascia and soffits · Roofing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Barricade below and set up a mobile scaffold or secured ladder
	Public entering the work area
Falling from a ladder
Falling from height
	Public, Children, Workers, People below
	Very high (20)
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Control (engineering)]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Control (procedures)]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Control (procedures)]
- Use a podium step, mobile tower or MEWP for longer jobs instead of a straight ladder. [Reduce / substitute]
- Use EN 131 professional ladders in good condition. Remove any damaged ladder from site. [Control (engineering)]
- Set extension ladders at a 4 to 1 angle on firm, level ground, tied or footed, and reaching 1 metre above the landing. [Control (engineering)]
- Use ladders only for short, light work (about 30 minutes in one spot). Do not carry heavy or awkward loads up a ladder. [Control (procedures)]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Control (procedures)]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile tower or MEWP instead of working off a ladder. [Control (engineering)]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Control (engineering)]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Control (procedures)]
	Medium (8)
	

	2
	Check soffit sheets for asbestos and old paint for lead before removing
	Disturbing asbestos
Lead paint dust and fumes
	Workers, Occupants, Public, Residents, Children
	Very high (15)
	- Before work on any building built before 2000, check the refurbishment and demolition asbestos survey for the work area (HSE HSG264). If there is none, presume asbestos is present or have it sampled before you start. [Eliminate]
- Seal off the work area and keep everyone else out. [Isolate]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with an H-class vacuum. [Control (engineering)]
- Most asbestos insulation, coatings and insulating board need a licensed contractor. Notifiable non-licensed work is notified to HSE before it starts. Other work needs trained workers and controls. [Control (procedures)]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Control (procedures)]
- Wear a fit-tested FFP3 mask (or better) and disposable type 5 coveralls. [PPE]
- Test old paint for lead before you sand, scrape, cut or heat it. [Eliminate]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Reduce / substitute]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Isolate]
- Clean up with an H-class vacuum and wet wipes. Never dry sweep. [Control (engineering)]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Control (procedures)]
- Wear an FFP3 mask, disposable coveralls and gloves. [PPE]
	Medium (5)
	

	3
	Remove gutters and old fascia boards, lowering them by hand
	Lifting and carrying heavy loads
Falling tools and materials
Cuts from sharp edges
	Workers, Public, People below
	High (12)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Control (engineering)]
- Use catch fans, debris netting or covered walkways where people pass below. [Control (engineering)]
- Tether hand tools when working at height. [Control (engineering)]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Control (procedures)]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Control (engineering)]
- Use knives with retractable or self-retracting blades. [Control (engineering)]
- Cut away from your body and keep your other hand clear. [Control (procedures)]
- Put used blades in a blade bin or sharps container. [Control (procedures)]
- Use two people to handle large sheets of metal or glass. [Control (procedures)]
	Medium (8)
	

	4
	Cut and fix new boards and soffit lining
	Saw cuts and kickback
Nail gun injuries
Wood and MDF dust
Loud noise
	Workers, People nearby
	High (12)
	- Keep blade guards fitted and working, and use the riving knife on table saws. [Control (engineering)]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Control (engineering)]
- Use a sharp, undamaged blade made for the material. [Control (procedures)]
- Stand to one side of the blade line, out of the kickback path. [Control (procedures)]
- Use a nail gun with a sequential (single shot) trigger, not a contact or bump trigger. [Reduce / substitute]
- Disconnect the air or battery before clearing jams, adjusting or moving between work areas. [Control (engineering)]
- Keep your free hand at least 30 cm from the nailing point. [Control (procedures)]
- Never point the gun at anyone or carry it with your finger on the trigger. [Control (procedures)]
- Buy pre-cut or pre-finished timber where you can. [Reduce / substitute]
- Cut outdoors or in a well-ventilated area away from others. [Isolate]
- Use saws and sanders with dust extraction connected to an M-class (or better) vacuum. [Control (engineering)]
- Clean up with a vacuum, not a broom or compressed air. [Control (procedures)]
- Do a COSHH assessment for hardwood and MDF dust. [Control (procedures)]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Reduce / substitute]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Isolate]
- Keep tools maintained and use mufflers on compressors and generators. [Control (engineering)]
- Limit time on noisy tools and rotate workers. [Control (procedures)]
- Assess noise. At 85 dB(A) or more, hearing protection is required and the zone must be marked. [Control (procedures)]
	Medium (8)
	

	5
	Refit gutters, clean up and remove access
	Poor housekeeping and waste
Falling from a ladder
	Workers, Visitors
	High (12)
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
- Do not work off the top three rungs of a leaning ladder. On a stepladder, do not stand on the top two steps (top three on swing-back or double-sided steps) unless there is a suitable handhold. [Control (procedures)]
- Check the ladder before each use: feet, rungs, stiles and locks. [Control (procedures)]
- Wear non-slip safety boots with clean soles. [PPE]
- Falling from a ladder: see step 1 for the full controls [Control (procedures)]
	Medium (8)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Barricade below and set up a mobile scaffold or secured ladder
2. Check soffit sheets for asbestos and old paint for lead before removing
3. Remove gutters and old fascia boards, lowering them by hand
4. Cut and fix new boards and soffit lining
5. Refit gutters, clean up and remove access
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety glasses
Rigger gloves
FFP3 dust mask
Ear defenders
Hi-vis vest
Safety helmet
Half-mask respirator (P3 filters)
Coveralls
Cut-resistant gloves
	Mobile access tower (PASMA certificate)
Extension ladder
Circular saw
Nail gun
Hand tools
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/roofing/fascia-soffit-replacement/
