RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Scaffold dismantling · Scaffolding · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check the scaffold is clear of other trades and materials
	Falling tools and materials
	Workers, Public, People below
	High (12)
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Control (engineering)]
- Falling tools and materials: see step 4 for the full controls [Control (procedures)]
	Medium (8)
	

	2
	Set an exclusion zone below
	Public entering the work area
Falling tools and materials
	Public, Children, Workers, People below
	High (12)
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Isolate]
- Give pedestrians a safe, marked path around the work, with ramps for prams and wheelchairs. [Isolate]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Control (engineering)]
- Put signs at each entry: site name, contact number and "No unauthorised entry". [Control (procedures)]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Control (procedures)]
- Use a spotter when moving plant or materials across public paths. [Control (procedures)]
- Use catch fans, debris netting or covered walkways where people pass below. [Control (engineering)]
- Tether hand tools when working at height. [Control (engineering)]
- Falling tools and materials: see step 4 for the full controls [Control (procedures)]
	Medium (8)
	

	3
	Dismantle top down, removing ties only as each lift comes down
	Scaffold collapse or fall from scaffold
Falling from height
	Workers, Public, People below
	Very high (20)
	- Scaffold is built, altered and taken down only by CISRS-carded scaffolders, to TG20 or a specific design. [Control (engineering)]
- Fit guardrails, mid rails and toe boards on every working platform. [Control (engineering)]
- Use mobile scaffolds only on firm, level ground with castors locked and outriggers fitted. Never move one with anyone on it. [Control (engineering)]
- Mobile towers are built by PASMA-trained workers. [Control (procedures)]
- Inspect the scaffold before first use, after any change or bad weather, and at least every 7 days. Record it on the tag and register. [Control (procedures)]
- Do not overload platforms. Know the duty rating and keep material stacks over the standards. [Control (procedures)]
- Never remove ties, braces, guardrails or boards. Only the scaffolder alters the scaffold. [Control (procedures)]
- Wear a hard hat and safety boots on and around the scaffold. [PPE]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Eliminate]
- Install guardrails or edge protection on all open edges before work starts. [Isolate]
- Use a scaffold, mobile tower or MEWP instead of working off a ladder. [Control (engineering)]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Control (engineering)]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Control (procedures)]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
	Medium (5)
	

	4
	Lower components, never drop them
	Falling tools and materials
Lifting and carrying heavy loads
	Workers, Public, People below
	High (12)
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Isolate]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Control (engineering)]
- Use catch fans, debris netting or covered walkways where people pass below. [Control (engineering)]
- Tether hand tools when working at height. [Control (engineering)]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Control (procedures)]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Control (procedures)]
- Wear a hard hat anywhere objects could fall. [PPE]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium (8)
	

	5
	Load the truck safely and clean the area
	Road traffic
Poor housekeeping and waste
	Workers, Road users, Public, Visitors
	Very high (15)
	- Do the work at low-traffic times, or close the road or lane with approval. [Eliminate]
- Put solid barriers between the work and traffic where speeds are high, not just cones. [Isolate]
- Use a truck-mounted attenuator or buffer vehicle on high speed roads. [Control (engineering)]
- Set up signs and cones to Chapter 8 (Traffic Signs Manual) by trained operatives. [Control (procedures)]
- Get a street works permit or licence from the highway authority before you start. [Control (procedures)]
- Park work vehicles to shield the work zone, with beacons on. [Control (procedures)]
- Wear Class 2 or 3 hi-vis clothing (EN ISO 20471). [PPE]
- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Medium (5)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Check the scaffold is clear of other trades and materials
2. Set an exclusion zone below
3. Dismantle top down, removing ties only as each lift comes down
4. Lower components, never drop them
5. Load the truck safely and clean the area
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Safety helmet
Full body harness and lanyard
Rigger gloves
Hi-vis vest
Safety glasses
	Tube and fitting or system scaffold (CISRS scaffolder card to erect, alter or dismantle)
Trailer
Hand tools
	Work at height permit


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/scaffolding/scaffold-dismantling/
