RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Home battery installation · Solar · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check the location meets clearance and fire rules
	Fire and emergencies
	Workers, Occupants, Visitors
	High (10)
	- Provide fire extinguishers suited to the site, checked and easy to reach. [Control (engineering)]
- Keep exits and escape routes clear and signed. [Control (engineering)]
- Have a site emergency plan: alarm, exits, assembly point and emergency contacts. [Control (procedures)]
- Keep a stocked first aid kit and at least one trained first aider on site. [Control (procedures)]
- Know the site address and how emergency services get in. Call 999. [Control (procedures)]
- Go through the emergency plan with every worker and visitor at induction. [Control (procedures)]
- Keep flammable materials and rubbish away from exits and escape routes. [Control (procedures)]
	Medium (5)
	

	2
	Move and mount the battery with lifting aids, it is very heavy
	Lifting and carrying heavy loads
	Workers
	High (12)
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Eliminate]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Reduce / substitute]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Control (engineering)]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Control (procedures)]
- Keep the load close, back straight and no twisting. Turn with your feet. [Control (procedures)]
- Rotate tasks and take breaks on long lifting jobs. [Control (procedures)]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium (6)
	

	3
	Isolate all sources, lock off and label and prove dead
	Electric shock from live wiring
Stored energy
	Workers, Occupants
	Very high (15)
	- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Control (procedures)]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
- Release or block all stored energy before work: release the pressure in pipes, tanks and hoses, bleed hydraulics, release springs, lower loads. [Eliminate]
- Lock out and tag all energy sources with personal locks. [Isolate]
- Put mechanical blocks or props under raised parts like buckets, tipper bodies and doors. [Control (engineering)]
- Test that the system is dead and nothing can move before you start. [Control (procedures)]
- Follow the maker's procedure, for example for garage door and roller door springs. [Control (procedures)]
- Wear safety glasses and gloves. [PPE]
	Medium (5)
	

	4
	Connect battery and inverter, treating battery terminals as always live
	Electric shock from live wiring
Stored energy
	Workers, Occupants
	Very high (15)
	- Electric shock from live wiring: see step 3 for the full controls [Control (procedures)]
- Stored energy: see step 3 for the full controls [Control (procedures)]
	Medium (5)
	

	5
	Commission, label and clean up
	Poor housekeeping and waste
	Workers, Visitors
	Medium (8)
	- Order materials to size and send packaging back where you can. [Eliminate]
- Put skips and waste chutes close to the work. [Control (engineering)]
- Clean as you go, and do a full clean up at the end of each day. [Control (procedures)]
- Keep exits, stairs and walkways clear at all times. [Control (procedures)]
- Stack materials neatly on level ground, away from edges. [Control (procedures)]
- Use a registered waste carrier and keep waste transfer notes for at least 2 years. Keep hazardous waste such as asbestos separate, with consignment notes (special waste in Scotland). [Control (procedures)]
- Wear gloves when handling waste. [PPE]
	Low (4)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Check the location meets clearance and fire rules
2. Move and mount the battery with lifting aids, it is very heavy
3. Isolate all sources, lock off and label and prove dead
4. Connect battery and inverter, treating battery terminals as always live
5. Commission, label and clean up
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety boots
Insulated electrical gloves
Safety glasses
Arc-rated clothing and face shield
Rigger gloves
	Power drill
Electrical test equipment (multifunction tester)
Hand tools
	Permit to work (electrical isolation)


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/uk/rams/solar/home-battery-installation/
