RISK ASSESSMENT AND METHOD STATEMENT (RAMS)
Kitchen splashback tiling · Tiling · Template from SiteSorted
1. BUSINESS AND JOB DETAILS
	Company name and number
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client and principal contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by / approved by
	

	Document reference and revision
	

	Review date
	


2. RISK ASSESSMENT
	#
	Activity
	Hazards
	Who might be harmed
	Risk before
	Controls
	Risk after
	Responsible

	1
	Isolate power to sockets in the splashback
	Electric shock from live wiring
	Workers, Occupants
	Very high (15)
	- Isolate the power before any work. Do not work live. [Eliminate]
- Lock out and tag the isolation point with your own personal lock and danger tag. [Isolate]
- Prove dead at the point of work with an approved voltage indicator (GS38), and prove the tester before and after. [Control (engineering)]
- Only competent, qualified electricians do electrical work, following a safe isolation procedure. [Control (procedures)]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Control (procedures)]
- If live work cannot be avoided, use a permit, a safety observer and insulated tools. [Control (procedures)]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
	Medium (5)
	

	2
	Protect benches and appliances
	Working in an occupied home or building
	Residents, Children, Staff, Workers
	Medium (9)
	- Plan noisy, dusty or risky work for when the building is empty. [Eliminate]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Isolate]
- Keep fire exits and paths clear at all times. [Control (procedures)]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Control (procedures)]
- Lock away tools, chemicals and materials each day, out of reach of children. [Control (procedures)]
- Clean up dust and debris at the end of each day. [Control (procedures)]
	Low (3)
	

	3
	Cut tiles wet and drill holes with water
	Silica dust from concrete, brick, stone and tiles
Saw cuts and kickback
Eye injuries
	Workers, People nearby
	Very high (20)
	- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Reduce / substitute]
- Cut outdoors or in a separate area, with other people well away and upwind. [Isolate]
- Use water on the blade or on-tool dust extraction connected to an H-class vacuum. [Control (engineering)]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Control (procedures)]
- Do a COSHH assessment and keep exposure below the workplace exposure limit (0.1 mg/m3 respirable crystalline silica, 8 hours). [Control (procedures)]
- Workers regularly exposed to silica dust get health surveillance (COSHH reg 11, HSE G404). [Control (procedures)]
- Wear a fit-tested FFP3 mask. [PPE]
- Keep blade guards fitted and working, and use the riving knife on table saws. [Control (engineering)]
- Use push sticks and clamps, and support long pieces so they do not pinch the blade. [Control (engineering)]
- Use a sharp, undamaged blade made for the material. [Control (procedures)]
- Stand to one side of the blade line, out of the kickback path. [Control (procedures)]
- Let the blade stop fully before reaching in or putting the saw down. [Control (procedures)]
- Use tool guards and screens to stop flying particles. [Control (engineering)]
- Use dust extraction and water to keep dust out of the air. [Control (engineering)]
- Keep others out of the area when cutting, grinding or chipping. [Control (procedures)]
- Keep an eye wash station or eye wash bottles on site. [Control (procedures)]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
	Medium (8)
	

	4
	Set, grout and clean
	Hazardous chemicals
Cuts from sharp edges
	Workers, Occupants
	Medium (9)
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Reduce / substitute]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Control (engineering)]
- Do a COSHH assessment and read the Safety Data Sheet (SDS) before use. [Control (procedures)]
- Keep chemicals in labelled containers. Never decant into drink bottles. [Control (procedures)]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Control (procedures)]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Control (procedures)]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Control (engineering)]
- Use knives with retractable or self-retracting blades. [Control (engineering)]
- Cut away from your body and keep your other hand clear. [Control (procedures)]
- Put used blades in a blade bin or sharps container. [Control (procedures)]
- Use two people to handle large sheets of metal or glass. [Control (procedures)]
- Wear cut-resistant gloves and long sleeves. [PPE]
	Medium (6)
	


3. METHOD STATEMENT: SEQUENCE OF WORK
1. Isolate power to sockets in the splashback
2. Protect benches and appliances
3. Cut tiles wet and drill holes with water
4. Set, grout and clean
4. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety glasses
FFP3 dust mask
Chemical-resistant gloves
Half-mask respirator (P3 filters)
Ear defenders
Safety goggles
Face shield
Coveralls
Cut-resistant gloves
	Wet tile cutter
Hand tools
Power drill
	None required


5. EMERGENCY ARRANGEMENTS
	Emergency number: 999
	

	Nearest A&E
	

	Assembly point
	

	First aider
	

	First aid kit location
	

	Fire extinguisher location
	


6. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: Management of Health and Safety at Work Regulations 1999 and the Construction (Design and Management) Regulations 2015.
Keep this RAMS, every revision and the signed briefing register with the site file for the length of the job, and keep a copy in your records afterwards.
7. BRIEFING REGISTER
By signing below, each person confirms they have read and understood this RAMS and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from SiteSorted. Make it in 2 minutes and get it signed on your phone: https://sitesorted.pages.dev/uk/rams/tiling/splashback-tiling/
