JOB HAZARD ANALYSIS (JHA)
Brick cleaning and acid washing · Bricklaying · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Read the safety data sheet and set up an eyewash
	Hazardous chemicals
	Medium
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and labels before use, following OSHA Hazard Communication. [Administrative]
- Keep chemicals in labeled containers. Never pour them into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
	Medium
	

	2
	Protect windows, plants and drains
	Hazardous chemicals
Public entering the work area
	High
	- Hazardous chemicals: see step 1 for the full controls [Administrative]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorized entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving plant or materials across public paths. [Administrative]
	Medium
	

	3
	Always add acid to water, never water to acid
	Hazardous chemicals
Eye injuries
	Medium
	- Hazardous chemicals: see step 1 for the full controls [Administrative]
- Use tool guards and screens to stop flying particles. [Engineering]
- Use dust extraction and water to keep dust out of the air. [Engineering]
- Keep others out of the area when cutting, grinding or chipping. [Administrative]
- Keep an eye wash station or eye wash bottles on site. [Administrative]
- Wear safety glasses at all times, goggles for dust and chemicals, and a face shield for grinding. [PPE]
	Medium
	

	4
	Apply and wash off from the bottom up
	High pressure water jetting
Slips and trips
	Medium
	- Set an exclusion zone around the jetting area. [Engineering (guarding)]
- Use a dead man's trigger that stops the jet when released, and check hoses and fittings before use. [Engineering]
- Only trained operators use high pressure jetting gear. [Administrative]
- Never point the lance at anyone or put a hand in front of it. [Administrative]
- Treat any jetting injury as serious and go to hospital, even if it looks small. [Administrative]
- Wear a face shield, waterproof clothing, gloves, hearing protection and safety boots. [PPE]
- Plan walkways and keep them clear of materials, hoses and leads. [Elimination]
- Run cords and hoses overhead on hooks or stands, or along walls, not across walkways. [Engineering]
- Fill or cover holes, and lay boards or mats on muddy access paths. [Engineering]
- Clean up offcuts, packaging and spills as you go, not at the end of the day. [Administrative]
- Keep work areas, stairs and access paths well lit. [Administrative]
- Wear safety boots with good grip, laced up. [PPE]
	Low
	

	5
	Neutralise and dispose of runoff, then clean up
	Poor housekeeping and waste
	Medium
	- Order materials to size and send packaging back where you can. [Elimination]
- Put dumpsters and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Low
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety goggles (ANSI Z87.1)
Face shield (ANSI Z87.1)
Chemical-resistant gloves
Coveralls
Safety-toe boots (ASTM F2413)
Half-face respirator (P100 cartridges)
High-visibility safety apparel, ANSI/ISEA 107 Class 2 or 3 (Type R near roadways)
Safety glasses (ANSI Z87.1)
Work gloves
Hearing protection (earmuffs or plugs)
	Pressure washer
Backpack sprayer (State pesticide applicator license for commercial herbicide work)
Mobile (rolling) scaffold (Erected under a competent person (29 CFR 1926.451))
	None required


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/bricklaying/brick-cleaning/
