JOB HAZARD ANALYSIS (JHA)
Internal strip-out · Demolition · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Check the asbestos survey and remove any asbestos first
	Disturbing asbestos
	Critical
	- Treat insulation, surfacing and resilient flooring in buildings built before 1981 as asbestos unless testing shows otherwise, and get the owner's asbestos survey before you start. [Elimination]
- Seal off the work area and keep everyone else out. [Engineering (guarding)]
- If asbestos must be disturbed, keep it wet, use hand tools not power tools, and clean up with a HEPA vacuum. [Engineering]
- Follow 29 CFR 1926.1101: competent person, work class, regulated area and exposure monitoring. [Administrative]
- Commercial renovation and any demolition need a NESHAP asbestos inspection first, and demolition needs written notice to the state or EPA 10 working days before work starts (40 CFR 61 Subpart M). [Administrative]
- Roofing felts, cement shingles and siding, roof coatings and old panel backboards can also contain asbestos. Test them or treat them as asbestos; asbestos roofing is removed intact with hand tools by trained workers (29 CFR 1926.1101(g)(8)). [Administrative]
- Stop work straight away if you find suspect asbestos. Do not touch it and tell your supervisor. [Administrative]
- Wear a fit-tested NIOSH-approved respirator suited to the work class, and disposable coveralls. [PPE]
	Medium
	

	2
	Check for lead paint and other hazardous materials before work starts
	Lead paint dust and fumes
Hazardous chemicals
	High
	- Test old paint for lead before you sand, scrape, cut or heat it. [Elimination]
- Use wet scraping, chemical strippers or shrouded tools with extraction instead of dry sanding. Never burn off lead paint with an open flame. [Substitution]
- Seal off the work area with plastic sheeting and keep residents, children and pets out. [Engineering (guarding)]
- Clean up with a HEPA vacuum and wet wipes. Never dry sweep. [Engineering]
- In homes and child-occupied facilities built before 1978 (such as child care centers, preschools and kindergarten classrooms), work that disturbs more than 6 sq ft inside or 20 sq ft outside is done by an EPA Lead-Safe Certified firm with a certified renovator (RRP rule). [Administrative]
- Do an initial lead exposure assessment and protect workers as if over the limit until results are in. Over 50 micrograms per cubic meter, follow a written lead compliance program (29 CFR 1926.62(d), (e)). [Administrative]
- Never torch painted surfaces, keep heat guns below 1,100 degrees F, and use sanders, grinders or planers only with a shroud and HEPA vacuum attachment (40 CFR 745.85(a)(3)). [Administrative]
- Provide a clean change area and handwashing, and keep food, drink and tobacco out of the work area (29 CFR 1926.62(i)). [Administrative]
- Wash hands and face before eating, drinking or smoking. Change out of dusty clothes before going home. [Administrative]
- Wear a NIOSH-approved respirator with N100 or P100 filters, disposable coveralls and gloves. [PPE]
- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and labels before use, following OSHA Hazard Communication. [Administrative]
- Keep chemicals in labeled containers. Never pour them into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
	Medium
	

	3
	Isolate and cap power, gas and water to the area, and confirm they are dead
	Electric shock from live wiring
Gas and fuel lines
	Critical
	- Isolate the power before any work. Do not work live. [Elimination]
- Lock out and tag the disconnecting means with your own personal lock and tag so the circuit cannot be energized (29 CFR 1926.417). [Engineering (guarding)]
- Test before you touch: prove dead at the point of work with a tested voltage tester. [Engineering]
- Only qualified persons work on or near exposed energized parts. [Administrative]
- Check for back feeds from solar, batteries and generators that can keep a circuit live after the main switch is off. [Administrative]
- If energized work cannot be avoided, use an energized work permit, a safety observer and insulated tools, following NFPA 70E. [Administrative]
- Wear insulated gloves, arc-rated clothing and a face shield when testing or working near live parts. [PPE]
- Isolate and purge the line before work, with the owner's approval. [Elimination]
- Lock off and tag the isolation valve. [Engineering (guarding)]
- Check for leaks with a gas detector before and during work, and ventilate the area. [Engineering]
- Only licensed gas fitters work on gas lines. [Administrative]
- Remove ignition sources: no smoking, no hot work and no sparking tools near the line. [Administrative]
- Know where the shut-off valve is and what to do if a leak happens. [Administrative]
- Wear safety glasses and gloves, and keep a fire extinguisher close by. [PPE]
	Medium
	

	4
	Seal the area from occupants, set up dust control and keep exits clear
	Working in an occupied home or building
General dust
Fire and emergencies
	High
	- Plan noisy, dusty or risky work for when the building is empty. [Elimination]
- Close off the work area with barriers, plastic sheeting or locked doors, and put up signs. [Engineering (guarding)]
- Keep fire exits and paths clear at all times. [Administrative]
- Tell occupants before you turn off power, water or gas, and before noisy or dusty work. [Administrative]
- Lock away tools, chemicals and materials each day, out of reach of children. [Administrative]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitution]
- Seal off the work area with plastic sheeting in occupied buildings. [Engineering (guarding)]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
- Provide fire extinguishers suited to the site, checked and easy to reach. [Engineering]
- Keep exits and escape routes clear and signed. [Engineering]
- Have a site emergency plan: alarm, exits, assembly point and emergency contacts. [Administrative]
- Keep a stocked first aid kit and at least one trained first aider on site. [Administrative]
- Know the site address and how emergency services get in. Call 911. [Administrative]
	Medium
	

	5
	Confirm which walls are load bearing and leave them alone without an engineer design
	Structural collapse during alterations
	High
	- Get an engineer to check before removing any wall, beam, post or bracing that may be load-bearing. [Elimination]
- Keep everyone clear of the area under and next to the work. [Engineering (guarding)]
- Install temporary props, needles or shoring as designed before removing any support. [Engineering]
- Follow the engineer's sequence. Do not change it without approval. [Administrative]
- Check props daily. Do not remove them until the permanent support is in and approved. [Administrative]
- Wear a hard hat and safety boots. [PPE]
	Medium
	

	6
	Strip fittings and linings from the top down, using a platform ladder or mobile scaffold for ceilings
	Falling tools and materials
Cuts from sharp edges
Falling from a ladder
	High
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Use a platform ladder, mobile scaffold or aerial lift for longer jobs instead of a straight ladder. [Substitution]
- Use Type I, IA or IAA ladders in good condition. Tag and remove any damaged ladder. [Engineering]
- Set extension ladders at a 4 to 1 angle on firm, level ground, secured, and reaching 3 feet above the landing. [Engineering]
- Use ladders only for short, light work. Do not carry heavy or awkward loads up a ladder. [Administrative]
- Keep three points of contact and your belt buckle between the stiles. Do not overreach. [Administrative]
	Medium
	

	7
	Cut or break materials with dust extraction
	Angle grinder injuries
Loud noise
Hand-arm and whole-body vibration
Silica dust from concrete, brick, stone and tiles
	Critical
	- Use a guarded saw or a different tool where you can. [Substitution]
- Keep the guard on and use the side handle. Never remove the guard. [Engineering]
- Use the right disc for the job, rated for the grinder's speed. Check it for cracks first. [Administrative]
- Only trained people change discs, with the grinder unplugged or the battery out. [Administrative]
- Use quieter tools and methods, such as cut-to-size materials, low-noise machines and battery tools. [Substitution]
- Keep noisy plant away from work areas, and use screens or distance between the noise and people. [Engineering (guarding)]
- Keep tools maintained and use mufflers on compressors and generators. [Engineering]
- Limit time on noisy tools and rotate workers. [Administrative]
- Use low-vibration tools and methods, such as a breaker on an excavator instead of a hand jackhammer. [Substitution]
- Keep tools sharp and well maintained, and use anti-vibration handles and seats. [Engineering]
- Limit trigger time on high-vibration tools and rotate workers. [Administrative]
- Keep hands warm and dry, and take regular breaks. [Administrative]
- Order materials cut to size, or use low-dust methods such as score and snap or a block splitter. [Substitution]
- Cut outdoors or in a separate area, with other people well away and upwind. [Engineering (guarding)]
- Use wet cutting or on-tool dust collection with a HEPA vacuum, as set out in Table 1 of 29 CFR 1926.1153. [Engineering]
- Clean up with a vacuum or wet methods. Never dry sweep or use compressed air. [Administrative]
- Have a written exposure control plan and a competent person for silica (29 CFR 1926.1153). [Administrative]
- Workers who must wear a respirator 30 or more days a year get a free medical exam every 3 years (29 CFR 1926.1153(h)). [Administrative]
	Medium
	

	8
	Watch for needles, droppings and mould in wall and ceiling cavities
	Needles and sharps
Mold and droppings
	Medium
	- Use tongs or a pick-up tool. Never pick up needles by hand. [Engineering]
- Put needles in a hard sharps container with a lid. [Engineering]
- Look before you reach. Use a flashlight to check ceilings, cavities and trash. [Administrative]
- If you are stuck, wash the area with soap and water and see a doctor straight away. [Administrative]
- Wear puncture-resistant gloves and safety boots. [PPE]
- Fix the water leak and dry the area before removing mold. [Elimination]
- Seal off the area with plastic sheeting and keep occupants out. [Engineering (guarding)]
- Clean up with a HEPA vacuum and wet wipes. Never dry sweep. [Engineering]
- Bag moldy material on site and remove it promptly. [Administrative]
- Wash hands and face before eating and at the end of each shift. [Administrative]
- Wear an N95 (or better) respirator, gloves, goggles and disposable coveralls. [PPE]
	Low
	

	9
	Load waste into the dumpster by hand or chute, keeping walkways clear
	Lifting and carrying heavy loads
Poor housekeeping and waste
	High
	- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Order materials to size and send packaging back where you can. [Elimination]
- Put dumpsters and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety-toe boots (ASTM F2413)
Hard hat (ANSI Z89.1)
Safety glasses (ANSI Z87.1)
N95 respirator
Cut-resistant gloves
Hearing protection (earmuffs or plugs)
Half-face respirator (P100 cartridges)
Coveralls
Work gloves
Chemical-resistant gloves
Safety goggles (ANSI Z87.1)
Face shield (ANSI Z87.1)
	Hand tools
Angle grinder
Jackhammer
HEPA vacuum
Trailer
	None required


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/demolition/internal-strip-out/
