JOB HAZARD ANALYSIS (JHA)
Shopfront and commercial glazing · Glazing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up pedestrian control on the sidewalk
	Public entering the work area
Road traffic
	Critical
	- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorized entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Administrative]
- Use a spotter when moving plant or materials across public paths. [Administrative]
- Do the work at low-traffic times, or close the road or lane with approval. [Elimination]
- Put solid barriers between the work and traffic where speeds are high, not just cones. [Engineering (guarding)]
- Use a truck-mounted attenuator or buffer vehicle on high speed roads. [Engineering]
- Set up work zone signs and cones to MUTCD Part 6, with trained flaggers. [Administrative]
- Get any permit needed from the city, county or state DOT before you start. [Administrative]
- Park work vehicles to shield the work zone, with beacons on. [Administrative]
- Wear ANSI/ISEA 107 Class 2 or 3 high-visibility clothing. [PPE]
	Medium
	

	2
	Plan large lifts with vacuum lifters or crane
	Crane and lifting failure
Glass handling and breakage
	High
	- Barricade the lift zone and keep everyone out from under the load. [Engineering (guarding)]
- Use a crane rated for the load at the radius, set up on firm ground with outrigger pads. [Engineering]
- Check slings, chains, shackles and hooks before use. Remove anything damaged or not tagged. [Engineering]
- Plan the lift: weight, radius, ground, path and landing area. Use a written lift plan for complex lifts. [Administrative]
- Use a certified crane operator who has also been evaluated by the employer, with the evaluation documented on site (29 CFR 1926.1427), plus a qualified rigger (1926.1425) and a qualified signal person (1926.1428). [Administrative]
- Use tag lines to control loads and agree on clear radio or hand signals. [Administrative]
- Stop lifting in high wind or when the operator cannot see the signal person. [Administrative]
- Never ride on a load or hook. [Administrative]
- Wear a hard hat, hi-vis, gloves and safety boots. [PPE]
- Use suction lifters, glass trolleys or a glazing robot for large panes. [Engineering]
- Store glass upright on racks and secure it. Never lay it flat or lean it loosely. [Engineering]
- Use two or more people for large panes, and clear the carry route first. [Administrative]
- Mark new glass with tape or stickers so nobody walks into it. [Administrative]
- Clean up broken glass straight away into a marked container. [Administrative]
- Wear cut-resistant gloves, arm guards, safety glasses and safety boots. [PPE]
	Medium
	

	3
	Work from a aerial lift for high panes
	Aerial lift tip-over or crush
Falling from height
	Critical
	- Check the ground before setting up. Use outriggers and spreader pads, and keep clear of trenches, pits and slopes. [Engineering]
- Use a platform with tilt alarm and secondary guarding (anti-entrapment) where there is an overhead crush risk. [Engineering]
- Only trained and authorized operators use aerial lifts and scissor lifts (29 CFR 1926.453 for boom lifts, 1926.452(w) and 1926.454 for scissor lifts). [Administrative]
- Do a pre-start check each day. Keep a trained person on the ground who can lower the platform in an emergency. [Administrative]
- Never exceed the safe working load, climb on the rails or use a ladder in the basket. [Administrative]
- In boom-type platforms, wear a harness clipped to the basket anchor point. [PPE]
- Do the work from the ground where you can, for example pre-assemble on the ground or use extension poles. [Elimination]
- Install guardrails or edge protection on all open edges before work starts. [Engineering (guarding)]
- Use a scaffold, mobile work platform or aerial lift instead of working off a ladder. [Engineering]
- Where edge protection is not practical, use a fall restraint or fall arrest system on a rated anchor point. [Engineering]
- Provide fall protection at 6 feet or more and train workers to recognize fall hazards (29 CFR 1926.503). [Administrative]
- Have a rescue plan so a worker hanging in a harness can be brought down within minutes. [Administrative]
- Wear a full body harness with a shock-absorbing lanyard, clipped on at all times when using fall arrest. [PPE]
	Medium
	

	4
	Install frames and glass, keeping everyone out from under the load
	Falling tools and materials
Lifting and carrying heavy loads
	High
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Lower materials with a hoist, chute or rope. Never throw or drop anything down. [Administrative]
- Wear a hard hat anywhere objects could fall. [PPE]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
	Medium
	

	5
	Seal, clean up and reopen the sidewalk
	Hazardous chemicals
Poor housekeeping and waste
	Medium
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and labels before use, following OSHA Hazard Communication. [Administrative]
- Keep chemicals in labeled containers. Never pour them into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Order materials to size and send packaging back where you can. [Elimination]
- Put dumpsters and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Wear gloves when handling waste. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety-toe boots (ASTM F2413)
Hard hat (ANSI Z89.1)
High-visibility safety apparel, ANSI/ISEA 107 Class 2 or 3 (Type R near roadways)
Cut-resistant gloves
Safety glasses (ANSI Z87.1)
Personal fall arrest system (harness)
Work gloves
Chemical-resistant gloves
Safety goggles (ANSI Z87.1)
Half-face respirator (P100 cartridges)
Coveralls
	Mobile crane (Operator certified by an accredited body or audited employer program (29 CFR 1926.1427) and evaluated by the employer, with a signed evaluation on site (1926.1427(f)); qualified rigger (1926.1425) and qualified signal person (1926.1428))
Boom lift (aerial lift) (Trained and authorized operator (29 CFR 1926.453, ANSI A92.24 training and familiarization))
Telehandler (Trained and evaluated operator, certified by the employer with name, training date, evaluation date and evaluator; re-evaluated every 3 years (29 CFR 1910.178(l), via 1926.602(d)). If used to hoist a suspended load with a winch or jib, crane rules apply (29 CFR 1926 Subpart CC))
Power drill
Hand tools
	Critical lift plan
Written fall protection plan (only where guardrails, nets or personal fall arrest are not feasible, 1926.502(k))


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/glazing/shopfront-glazing/
