JOB HAZARD ANALYSIS (JHA)
Flat roof and membrane roofing · Roofing · Template from Safety Paperwork
1. BUSINESS AND JOB DETAILS
	Company
	

	Business address and phone
	

	Job / scope of work
	

	Site address
	

	Client / general contractor
	

	Start date and duration
	

	Working hours
	

	Supervisor
	

	Prepared by
	

	Document number and revision
	

	Competent person
	

	Review date
	


2. JOB STEPS, HAZARDS AND CONTROLS
	#
	Job step
	Hazards
	Risk before
	Controls
	Risk after
	Responsible

	1
	Set up edge protection around the flat roof and guard any roof openings or skylights
	Falling from a roof edge
Falling through a floor opening or void
Falling through a fragile roof or skylight
	Critical
	- Do what you can from the ground or from a scaffold at the gutter line, for example pre-assemble parts on the ground. [Elimination]
- Install edge protection or guardrails on all open roof edges before work starts. [Engineering (guarding)]
- Use a perimeter scaffold with handrails and toe boards along the eaves where practical. [Engineering]
- Where guardrails cannot be fitted, use fall restraint on certified roof anchors so workers cannot reach the edge. [Engineering]
- Low-slope roofs: guardrails, safety nets, personal fall arrest, or a warning line combined with one of these or with a safety monitor (a safety monitor alone only on roofs 50 feet wide or less). Steep roofs: guardrails with toe boards, safety nets or personal fall arrest (29 CFR 1926.501(b)(10), (11)). [Administrative]
- Use one safe, controlled access point and keep others off the roof. [Administrative]
- Cover every hole with a secured cover marked "HOLE" or "COVER" that can hold twice the weight it may carry. [Engineering (guarding)]
- Put guardrails with toe boards around stairwells, elevator shafts, floor holes and open edges. [Engineering (guarding)]
- Install stairs early and fit temporary handrails as soon as they go in. [Engineering]
- Never remove a cover or guardrail without approval. Put it back straight away. [Administrative]
- Inspect covers and barriers daily and after other trades have been through. [Administrative]
- Work from underneath or from an aerial lift so nobody stands on the fragile roof. [Elimination]
- Cover every skylight with a fixed, marked cover that can hold at least twice the weight it may carry, or guard it with a guardrail. [Engineering (guarding)]
- Use crawl boards or staging to spread the load on fragile or rotten decking, and cover or guard any hole left where decking is removed (29 CFR 1926.501(b)(4)). [Engineering]
- Use fall arrest on rated anchors when working near fragile areas. [Engineering]
- Treat all roof sheets as fragile until a competent person confirms they are not. Old fiber cement and plastic sheets are fragile. [Administrative]
	Medium
	

	2
	Lift materials up with a hoist, keeping the area below closed off
	Falling tools and materials
Lifting and carrying heavy loads
Public entering the work area
	High
	- Barricade and sign the drop zone under overhead work so nobody walks beneath. [Engineering (guarding)]
- Fit toe boards, kick plates and mesh screens on scaffolds and edges. [Engineering]
- Use catch fans, debris netting or covered walkways where people pass below. [Engineering]
- Tether hand tools when working at height. [Engineering]
- Keep platforms tidy. Do not stack materials near edges or above toe board height. [Administrative]
- Plan to avoid carrying: have materials delivered, and old items picked up, as close as possible to where they are used. [Elimination]
- Use lighter or smaller loads: order smaller bags and shorter lengths, and drain or break down old items before moving them. [Substitution]
- Use trolleys, pallet jacks, hoists, vacuum lifters or plant instead of carrying by hand. [Engineering]
- Use a two-person lift for anything heavy, long or awkward. Plan the route first and clear it. [Administrative]
- Keep the load close, back straight and no twisting. Turn with your feet. [Administrative]
- Fence off the site with secure temporary fencing and lock the gates when you leave. [Engineering (guarding)]
- Give pedestrians a safe, marked path around the work, with ramps for strollers and wheelchairs. [Engineering (guarding)]
- Use hoarding, covered walkways or catch fans where work is above public areas. [Engineering]
- Put signs at each entry: site name, contact number and "No unauthorized entry". [Administrative]
- Make the site safe at the end of each day: cover holes, lower plant, remove ladders and lock tools away. [Administrative]
	Medium
	

	3
	Strip the old covering and check the deck for rot
	Lifting and carrying heavy loads
Cuts from sharp edges
General dust
	High
	- Rotate tasks and take breaks on long lifting jobs. [Administrative]
- Wear gloves for grip and safety boots to protect your feet. [PPE]
- Lifting and carrying heavy loads: see step 2 for the full controls [Administrative]
- Deburr or cover sharp edges, and fit edge protectors on exposed sheet metal. [Engineering]
- Use knives with retractable or self-retracting blades. [Engineering]
- Cut away from your body and keep your other hand clear. [Administrative]
- Put used blades in a blade bin or sharps container. [Administrative]
- Use two people to handle large sheets of metal or glass. [Administrative]
- Use low-dust products, such as dust-reduced or pre-mixed compounds. [Substitution]
- Seal off the work area with plastic sheeting in occupied buildings. [Engineering (guarding)]
- Use tools with dust extraction and a vacuum for clean up. [Engineering]
- Lightly mist the area with water to keep dust down, away from anything electrical. [Engineering]
- Never dry sweep or blow dust off with compressed air. [Administrative]
	Medium
	

	4
	Apply primers and adhesives with good airflow and away from flames
	Hazardous chemicals
Flammable liquids and gases
	High
	- Choose the least harmful product that does the job, for example water-based instead of solvent-based. [Substitution]
- Use chemicals in well-ventilated areas, or use fans and extraction in closed rooms. [Engineering]
- Read the Safety Data Sheet (SDS) and labels before use, following OSHA Hazard Communication. [Administrative]
- Keep chemicals in labeled containers. Never pour them into drink bottles. [Administrative]
- Store chemicals away from heat, food and drink, and keep products that react with each other apart. [Administrative]
- Have eye wash and a spill kit nearby, and wash hands before eating. [Administrative]
- Wear chemical-resistant gloves and safety glasses or goggles as listed on the SDS. [PPE]
- Use a respirator with the right cartridge if the SDS calls for one. [PPE]
- Use non-flammable or water-based products where you can. [Substitution]
- Keep ignition sources away: no smoking, no hot work and no running engines near flammables. [Engineering (guarding)]
- Store fuels and solvents in approved, closed containers in a ventilated area away from the work. [Engineering]
- Refuel equipment outdoors with the engine off and cool. [Administrative]
- Keep only what you need for the day on site. [Administrative]
- Store gas cylinders upright, secured and outdoors. [Administrative]
- Keep a suitable fire extinguisher where flammables are used or stored. [Administrative]
- Wear chemical gloves and safety glasses when pouring or mixing. [PPE]
	Medium
	

	5
	Torch on membrane under a hot work permit, with an extinguisher and a fire watch after
	Fire from hot works
Burns from hot surfaces
Fire and emergencies
	Critical
	- Use cold work methods where you can, such as bolting, press fittings or cutting with a saw instead of a torch. [Elimination]
- Move anything that can burn at least 35 feet away, or cover it with fire blankets. [Engineering (guarding)]
- Use fire-resistant screens to stop sparks reaching people or gaps in walls and floors. [Engineering]
- Get a hot work permit before starting. [Administrative]
- Keep a charged fire extinguisher and fire blanket at the work spot. [Administrative]
- Isolate heating systems and let parts cool before you touch them. [Elimination]
- Fit guards or insulation on hot pipes and equipment. [Engineering]
- Mark hot items with chalk or a "HOT" sign so others know. [Administrative]
- Keep a first aid kit and cool running water nearby for burns. [Administrative]
- Wear heat-resistant gloves and long sleeves. [PPE]
- Provide fire extinguishers suited to the site, checked and easy to reach. [Engineering]
- Keep exits and escape routes clear and signed. [Engineering]
- Have a site emergency plan: alarm, exits, assembly point and emergency contacts. [Administrative]
- Keep a stocked first aid kit and at least one trained first aider on site. [Administrative]
- Know the site address and how emergency services get in. Call 911. [Administrative]
	Medium
	

	6
	Seal outlets and edges, clear the roof and remove access
	Poor housekeeping and waste
Heat stress
Sun exposure (UV)
	High
	- Order materials to size and send packaging back where you can. [Elimination]
- Put dumpsters and waste chutes close to the work. [Engineering]
- Clean as you go, and do a full clean up at the end of each day. [Administrative]
- Keep exits, stairs and walkways clear at all times. [Administrative]
- Stack materials neatly on level ground, away from edges. [Administrative]
- Schedule heavy work for the cooler part of the day. [Elimination]
- Provide shade over work and rest areas, and fans or cooling in attics. [Engineering]
- Supply cool drinking water close by and drink a cup every 15 to 20 minutes. [Administrative]
- Take regular rest breaks in the shade, more often as it gets hotter. [Administrative]
- Let new and returning workers build up to full work in the heat over about a week. [Administrative]
- In California, Washington, Oregon and Maryland, follow the state heat illness rule: written plan, shade, water, rest and high-heat procedures. [Administrative]
- Plan outdoor work for early morning or late afternoon when UV is lower. [Elimination]
- Put shade covers over fixed work areas. [Engineering]
- Check the UV index each day. Use sun protection when it is 3 or higher. [Administrative]
- Check your skin regularly and see a doctor about any new or changing spots. [Administrative]
- Wear a broad-brim hat or hard hat brim, long sleeves, sunglasses and SPF 30 or higher sunscreen, reapplied every 2 hours. [PPE]
	Medium
	


3. PPE, PLANT AND PERMITS
	Required PPE
	Plant and equipment (licence or training)
	Permits and plans

	Safety-toe boots (ASTM F2413)
Personal fall arrest system (harness)
Work gloves
Safety glasses (ANSI Z87.1)
Half-face respirator (P100 cartridges)
Sun protection (sunscreen, hat, long sleeves)
Hard hat (ANSI Z89.1)
High-visibility safety apparel, ANSI/ISEA 107 Class 2 or 3 (Type R near roadways)
Cut-resistant gloves
N95 respirator
Chemical-resistant gloves
Safety goggles (ANSI Z87.1)
Coveralls
Welding gloves
Face shield (ANSI Z87.1)
	Propane torch
Hand tools
Extension ladder
Material hoist
	Written fall protection plan (only where guardrails, nets or personal fall arrest are not feasible, 1926.502(k))
Hot work permit (fire watch at least 60 minutes after, NFPA 51B)


4. EMERGENCY ARRANGEMENTS
	Emergency number: 911
	

	Nearest hospital
	

	Assembly point
	

	First aid / CPR person
	

	First aid kit location
	

	Fire extinguisher location
	


5. MONITORING, REVIEW AND LEGAL BASIS
The supervisor checks the controls at the start of each day and during the work. Stop work and review this document if the job, the crew or the site conditions change, or after any incident or near miss.
Legal basis: OSH Act Section 5(a)(1) and 29 CFR 1926, Safety and Health Regulations for Construction (incl. 1926.20 and 1926.21).
Keep this JHA on site during the job, and keep it with the training and inspection records for at least 1 year after the job (longer if your state plan or general contractor requires it). OSHA does not set a retention period for JHAs themselves.
6. SIGN-OFF
By signing below, each person confirms they have read and understood this JHA and will follow it.
	Name
	Role
	Tickets / licences
	Signature
	Date

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Free template from Safety Paperwork. Make it in 2 minutes and get it signed on your phone: https://safetypaperwork.com/us/jha/roofing/flat-roof-membrane/
